<?xml version="1.0" encoding="utf-8"?>
<EduNetworkBuilder>
  <!--This is a network file for EduNetworkBuilder.-->
  <Network>
    <en_message>There is no switch.  Add one and link the devices to it.  Click on the switch and add it to the network (make sure you add a switch and not a hub).  Then, drag links from the switch to the computers, choosing the ports to connect.</en_message>
    <en_title>No Switch</en_title>
    <height>1024</height>
    <width>1024</width>
    <itemsize>100</itemsize>
    <showlabels>False</showlabels>
    <level>0</level>
    <sortorder>2</sortorder>
    <uniqueidentifier>119</uniqueidentifier>
    <startinghelplevel>full</startinghelplevel>
    <device>
      <hostname>pc0</hostname>
      <size>100</size>
      <uniqueidentifier>100</uniqueidentifier>
      <location>187,465</location>
      <mytype>pc</mytype>
      <isdns>False</isdns>
      <isdhcp>False</isdhcp>
      <gateway>
        <ip>0.0.0.0</ip>
        <mask>0.0.0.0</mask>
        <gateway>0.0.0.0</gateway>
        <type>gw</type>
      </gateway>
      <nic>
        <nictype>lo</nictype>
        <nicname>lo0</nicname>
        <myid>
          <hostid>100</hostid>
          <nicid>101</nicid>
          <hostname>pc0</hostname>
          <nicname>lo0</nicname>
        </myid>
        <nictype>lo</nictype>
        <uniqueidentifier>101</uniqueidentifier>
        <usesdhcp>False</usesdhcp>
        <encryptionkey />
        <interface>
          <nicname>lo0</nicname>
          <myip>
            <ip>127.0.0.1</ip>
            <mask>255.0.0.0</mask>
            <gateway>0.0.0.0</gateway>
            <type>ip</type>
          </myip>
        </interface>
      </nic>
      <nic>
        <nictype>eth</nictype>
        <nicname>eth0</nicname>
        <myid>
          <hostid>100</hostid>
          <nicid>102</nicid>
          <hostname>pc0</hostname>
          <nicname>eth0</nicname>
        </myid>
        <nictype>eth</nictype>
        <uniqueidentifier>102</uniqueidentifier>
        <usesdhcp>False</usesdhcp>
        <encryptionkey />
        <interface>
          <nicname>eth0</nicname>
          <myip>
            <ip>192.168.1.2</ip>
            <mask>255.255.255.0</mask>
            <gateway>0.0.0.0</gateway>
            <type>ip</type>
          </myip>
        </interface>
      </nic>
    </device>
    <device>
      <hostname>pc1</hostname>
      <size>100</size>
      <uniqueidentifier>103</uniqueidentifier>
      <location>562,472</location>
      <mytype>pc</mytype>
      <isdns>False</isdns>
      <isdhcp>False</isdhcp>
      <gateway>
        <ip>0.0.0.0</ip>
        <mask>0.0.0.0</mask>
        <gateway>0.0.0.0</gateway>
        <type>gw</type>
      </gateway>
      <nic>
        <nictype>lo</nictype>
        <nicname>lo0</nicname>
        <myid>
          <hostid>103</hostid>
          <nicid>104</nicid>
          <hostname>pc1</hostname>
          <nicname>lo0</nicname>
        </myid>
        <nictype>lo</nictype>
        <uniqueidentifier>104</uniqueidentifier>
        <usesdhcp>False</usesdhcp>
        <encryptionkey />
        <interface>
          <nicname>lo0</nicname>
          <myip>
            <ip>127.0.0.1</ip>
            <mask>255.0.0.0</mask>
            <gateway>0.0.0.0</gateway>
            <type>ip</type>
          </myip>
        </interface>
      </nic>
      <nic>
        <nictype>eth</nictype>
        <nicname>eth0</nicname>
        <myid>
          <hostid>103</hostid>
          <nicid>105</nicid>
          <hostname>pc1</hostname>
          <nicname>eth0</nicname>
        </myid>
        <nictype>eth</nictype>
        <uniqueidentifier>105</uniqueidentifier>
        <usesdhcp>False</usesdhcp>
        <encryptionkey />
        <interface>
          <nicname>eth0</nicname>
          <myip>
            <ip>192.168.1.4</ip>
            <mask>255.255.255.0</mask>
            <gateway>0.0.0.0</gateway>
            <type>ip</type>
          </myip>
        </interface>
      </nic>
    </device>
    <device>
      <hostname>pc2</hostname>
      <size>100</size>
      <uniqueidentifier>116</uniqueidentifier>
      <location>378,455</location>
      <mytype>pc</mytype>
      <isdns>False</isdns>
      <isdhcp>False</isdhcp>
      <gateway>
        <ip>0.0.0.0</ip>
        <mask>0.0.0.0</mask>
        <gateway>0.0.0.0</gateway>
        <type>gw</type>
      </gateway>
      <nic>
        <nictype>lo</nictype>
        <nicname>lo0</nicname>
        <myid>
          <hostid>116</hostid>
          <nicid>117</nicid>
          <hostname>pc2</hostname>
          <nicname>lo0</nicname>
        </myid>
        <nictype>lo</nictype>
        <uniqueidentifier>117</uniqueidentifier>
        <usesdhcp>False</usesdhcp>
        <encryptionkey />
        <interface>
          <nicname>lo0</nicname>
          <myip>
            <ip>127.0.0.1</ip>
            <mask>255.0.0.0</mask>
            <gateway>0.0.0.0</gateway>
            <type>ip</type>
          </myip>
        </interface>
      </nic>
      <nic>
        <nictype>eth</nictype>
        <nicname>eth0</nicname>
        <myid>
          <hostid>116</hostid>
          <nicid>118</nicid>
          <hostname>pc2</hostname>
          <nicname>eth0</nicname>
        </myid>
        <nictype>eth</nictype>
        <uniqueidentifier>118</uniqueidentifier>
        <usesdhcp>False</usesdhcp>
        <encryptionkey />
        <interface>
          <nicname>eth0</nicname>
          <myip>
            <ip>192.168.1.3</ip>
            <mask>255.255.255.0</mask>
            <gateway>0.0.0.0</gateway>
            <type>ip</type>
          </myip>
        </interface>
      </nic>
    </device>
    <nettest>
      <shost>pc0</shost>
      <dhost>net_switch0</dhost>
      <thetest>NeedsLinkToDevice</thetest>
    </nettest>
    <nettest>
      <shost>pc1</shost>
      <dhost>net_switch0</dhost>
      <thetest>NeedsLinkToDevice</thetest>
    </nettest>
    <nettest>
      <shost>pc2</shost>
      <dhost>net_switch0</dhost>
      <thetest>NeedsLinkToDevice</thetest>
    </nettest>
    <tag>Link</tag>
    <tag>Switch</tag>
  </Network>
</EduNetworkBuilder>