<?xml version="1.0" encoding="utf-8"?>
<EduNetworkBuilder>
  <!--This is a network file for EduNetworkBuilder.-->
  <Network>
    <en_message>A staff memner brought in a laptop and they have problems.  As always, they want you to fix it.
Some vlan issues are a lot simpler than they originally look.</en_message>
    <en_title>A Tale of Two Access Points</en_title>
    <height>1024</height>
    <width>1024</width>
    <itemsize>100</itemsize>
    <showlabels>True</showlabels>
    <level>6</level>
    <sortorder>9</sortorder>
    <uniqueidentifier>202</uniqueidentifier>
    <startinghelplevel>full</startinghelplevel>
    <vlansenabled>True</vlansenabled>
    <VLANPacketColors>True</VLANPacketColors>
    <device>
      <hostname>firewall0</hostname>
      <size>100</size>
      <uniqueidentifier>148</uniqueidentifier>
      <location>450,170</location>
      <mytype>firewall</mytype>
      <isdns>False</isdns>
      <isdhcp>True</isdhcp>
      <gateway>
        <ip>10.0.0.1</ip>
        <mask>0.0.0.0</mask>
        <gateway>0.0.0.0</gateway>
        <type>gw</type>
      </gateway>
      <nic>
        <nictype>lo</nictype>
        <nicname>lo0</nicname>
        <myid>
          <hostid>148</hostid>
          <nicid>149</nicid>
          <hostname>firewall0</hostname>
          <nicname>lo0</nicname>
        </myid>
        <nictype>lo</nictype>
        <uniqueidentifier>149</uniqueidentifier>
        <usesdhcp>False</usesdhcp>
        <interface>
          <nicname>lo0</nicname>
          <myip>
            <ip>127.0.0.1</ip>
            <mask>255.0.0.0</mask>
            <gateway>0.0.0.0</gateway>
            <type>ip</type>
          </myip>
          <VLAN
            ID="1">Untagged</VLAN>
        </interface>
      </nic>
      <nic>
        <nictype>wan</nictype>
        <nicname>wan0</nicname>
        <myid>
          <hostid>148</hostid>
          <nicid>152</nicid>
          <hostname>firewall0</hostname>
          <nicname>wan0</nicname>
        </myid>
        <nictype>wan</nictype>
        <uniqueidentifier>152</uniqueidentifier>
        <usesdhcp>False</usesdhcp>
        <interface>
          <nicname>wan0</nicname>
          <myip>
            <ip>10.0.0.2</ip>
            <mask>255.255.255.0</mask>
            <gateway>0.0.0.0</gateway>
            <type>ip</type>
          </myip>
          <VLAN
            ID="1">Untagged</VLAN>
        </interface>
      </nic>
      <nic>
        <nictype>eth</nictype>
        <nicname>eth0</nicname>
        <myid>
          <hostid>148</hostid>
          <nicid>150</nicid>
          <hostname>firewall0</hostname>
          <nicname>eth0</nicname>
        </myid>
        <nictype>eth</nictype>
        <uniqueidentifier>150</uniqueidentifier>
        <usesdhcp>False</usesdhcp>
        <interface>
          <nicname>eth0</nicname>
          <myip>
            <ip>192.168.1.1</ip>
            <mask>255.255.255.0</mask>
            <gateway>0.0.0.0</gateway>
            <type>ip</type>
          </myip>
          <VLAN
            ID="1">Tagged</VLAN>
        </interface>
        <interface>
          <nicname>eth0:1</nicname>
          <myip>
            <ip>192.168.2.1</ip>
            <mask>255.255.255.0</mask>
            <gateway>0.0.0.0</gateway>
            <type>ip</type>
          </myip>
          <VLAN
            ID="1">Forbidden</VLAN>
          <VLAN
            ID="2">Tagged</VLAN>
        </interface>
        <interface>
          <nicname>eth0:2</nicname>
          <myip>
            <ip>192.168.3.1</ip>
            <mask>255.255.255.0</mask>
            <gateway>0.0.0.0</gateway>
            <type>ip</type>
          </myip>
          <VLAN
            ID="1">Forbidden</VLAN>
          <VLAN
            ID="3">Tagged</VLAN>
        </interface>
      </nic>
      <nic>
        <nictype>eth</nictype>
        <nicname>eth1</nicname>
        <myid>
          <hostid>148</hostid>
          <nicid>151</nicid>
          <hostname>firewall0</hostname>
          <nicname>eth1</nicname>
        </myid>
        <nictype>eth</nictype>
        <uniqueidentifier>151</uniqueidentifier>
        <usesdhcp>False</usesdhcp>
        <interface>
          <nicname>eth1</nicname>
          <myip>
            <ip>0.0.0.0</ip>
            <mask>0.0.0.0</mask>
            <gateway>0.0.0.0</gateway>
            <type>ip</type>
          </myip>
          <VLAN
            ID="1">Untagged</VLAN>
        </interface>
      </nic>
      <dhcprange>
        <ip>127.0.0.1</ip>
        <mask>0.0.0.0</mask>
        <gateway>0.0.0.0</gateway>
        <type>route</type>
      </dhcprange>
      <dhcprange>
        <ip>0.0.0.0</ip>
        <mask>0.0.0.0</mask>
        <gateway>0.0.0.0</gateway>
        <type>route</type>
      </dhcprange>
      <dhcprange>
        <ip>192.168.1.1</ip>
        <mask>192.168.1.5</mask>
        <gateway>192.168.1.10</gateway>
        <type>route</type>
      </dhcprange>
      <dhcprange>
        <ip>192.168.2.1</ip>
        <mask>192.168.2.5</mask>
        <gateway>192.168.2.10</gateway>
        <type>route</type>
      </dhcprange>
      <dhcprange>
        <ip>192.168.3.1</ip>
        <mask>192.168.3.5</mask>
        <gateway>192.168.3.10</gateway>
        <type>route</type>
      </dhcprange>
      <dhcprange>
        <ip>10.0.0.2</ip>
        <mask>0.0.0.0</mask>
        <gateway>0.0.0.0</gateway>
        <type>route</type>
      </dhcprange>
    </device>
    <device>
      <hostname>laptop0</hostname>
      <size>100</size>
      <uniqueidentifier>195</uniqueidentifier>
      <location>20,460</location>
      <mytype>laptop</mytype>
      <isdns>False</isdns>
      <isdhcp>False</isdhcp>
      <gateway>
        <ip>0.0.0.0</ip>
        <mask>0.0.0.0</mask>
        <gateway>0.0.0.0</gateway>
        <type>gw</type>
      </gateway>
      <nic>
        <nictype>lo</nictype>
        <nicname>lo0</nicname>
        <myid>
          <hostid>195</hostid>
          <nicid>196</nicid>
          <hostname>laptop0</hostname>
          <nicname>lo0</nicname>
        </myid>
        <nictype>lo</nictype>
        <uniqueidentifier>196</uniqueidentifier>
        <usesdhcp>False</usesdhcp>
        <encryptionkey />
        <ssid />
        <interface>
          <nicname>lo0</nicname>
          <myip>
            <ip>127.0.0.1</ip>
            <mask>255.0.0.0</mask>
            <gateway>0.0.0.0</gateway>
            <type>ip</type>
          </myip>
          <VLAN
            ID="1">Untagged</VLAN>
        </interface>
      </nic>
      <nic>
        <nictype>wlan</nictype>
        <nicname>wlan2</nicname>
        <myid>
          <hostid>195</hostid>
          <nicid>198</nicid>
          <hostname>laptop0</hostname>
          <nicname>wlan2</nicname>
        </myid>
        <nictype>wlan</nictype>
        <uniqueidentifier>198</uniqueidentifier>
        <usesdhcp>True</usesdhcp>
        <encryptionkey>TheKey</encryptionkey>
        <ssid>Students</ssid>
        <interface>
          <nicname>wlan2</nicname>
          <myip>
            <ip>192.168.2.5</ip>
            <mask>255.255.255.0</mask>
            <gateway>192.168.2.1</gateway>
            <type>route</type>
          </myip>
          <VLAN
            ID="1">Untagged</VLAN>
        </interface>
      </nic>
    </device>
    <device>
      <hostname>net_switch0</hostname>
      <size>100</size>
      <uniqueidentifier>100</uniqueidentifier>
      <location>250,450</location>
      <mytype>net_switch</mytype>
      <isdns>False</isdns>
      <isdhcp>False</isdhcp>
      <gateway>
        <ip>192.168.1.1</ip>
        <mask>0.0.0.0</mask>
        <gateway>0.0.0.0</gateway>
        <type>gw</type>
      </gateway>
      <nic>
        <nictype>lo</nictype>
        <nicname>lo0</nicname>
        <myid>
          <hostid>100</hostid>
          <nicid>101</nicid>
          <hostname>net_switch0</hostname>
          <nicname>lo0</nicname>
        </myid>
        <nictype>lo</nictype>
        <uniqueidentifier>101</uniqueidentifier>
        <usesdhcp>False</usesdhcp>
        <interface>
          <nicname>lo0</nicname>
          <myip>
            <ip>127.0.0.1</ip>
            <mask>255.0.0.0</mask>
            <gateway>0.0.0.0</gateway>
            <type>ip</type>
          </myip>
          <VLAN
            ID="1">Untagged</VLAN>
        </interface>
      </nic>
      <nic>
        <nictype>management_interface</nictype>
        <nicname>management_interface0</nicname>
        <myid>
          <hostid>100</hostid>
          <nicid>102</nicid>
          <hostname>net_switch0</hostname>
          <nicname>management_interface0</nicname>
        </myid>
        <nictype>management_interface</nictype>
        <uniqueidentifier>102</uniqueidentifier>
        <usesdhcp>False</usesdhcp>
        <interface>
          <nicname>management_interface0</nicname>
          <myip>
            <ip>192.168.1.252</ip>
            <mask>255.255.255.0</mask>
            <gateway>0.0.0.0</gateway>
            <type>ip</type>
          </myip>
          <VLAN
            ID="1">Untagged</VLAN>
        </interface>
      </nic>
      <nic>
        <nictype>port</nictype>
        <nicname>port1</nicname>
        <myid>
          <hostid>100</hostid>
          <nicid>103</nicid>
          <hostname>net_switch0</hostname>
          <nicname>port1</nicname>
        </myid>
        <nictype>port</nictype>
        <uniqueidentifier>103</uniqueidentifier>
        <usesdhcp>False</usesdhcp>
        <interface>
          <nicname>port1</nicname>
          <myip>
            <ip>0.0.0.0</ip>
            <mask>0.0.0.0</mask>
            <gateway>0.0.0.0</gateway>
            <type>ip</type>
          </myip>
          <VLAN
            ID="1">Untagged</VLAN>
          <VLAN
            ID="3">Forbidden</VLAN>
          <VLAN
            ID="2">Forbidden</VLAN>
        </interface>
      </nic>
      <nic>
        <nictype>port</nictype>
        <nicname>port2</nicname>
        <myid>
          <hostid>100</hostid>
          <nicid>104</nicid>
          <hostname>net_switch0</hostname>
          <nicname>port2</nicname>
        </myid>
        <nictype>port</nictype>
        <uniqueidentifier>104</uniqueidentifier>
        <usesdhcp>False</usesdhcp>
        <interface>
          <nicname>port2</nicname>
          <myip>
            <ip>0.0.0.0</ip>
            <mask>0.0.0.0</mask>
            <gateway>0.0.0.0</gateway>
            <type>ip</type>
          </myip>
          <VLAN
            ID="1">Untagged</VLAN>
          <VLAN
            ID="3">Forbidden</VLAN>
          <VLAN
            ID="2">Forbidden</VLAN>
        </interface>
      </nic>
      <nic>
        <nictype>port</nictype>
        <nicname>port3</nicname>
        <myid>
          <hostid>100</hostid>
          <nicid>105</nicid>
          <hostname>net_switch0</hostname>
          <nicname>port3</nicname>
        </myid>
        <nictype>port</nictype>
        <uniqueidentifier>105</uniqueidentifier>
        <usesdhcp>False</usesdhcp>
        <interface>
          <nicname>port3</nicname>
          <myip>
            <ip>0.0.0.0</ip>
            <mask>0.0.0.0</mask>
            <gateway>0.0.0.0</gateway>
            <type>ip</type>
          </myip>
          <VLAN
            ID="1">Forbidden</VLAN>
          <VLAN
            ID="3">Untagged</VLAN>
          <VLAN
            ID="2">Forbidden</VLAN>
        </interface>
      </nic>
      <nic>
        <nictype>port</nictype>
        <nicname>port4</nicname>
        <myid>
          <hostid>100</hostid>
          <nicid>106</nicid>
          <hostname>net_switch0</hostname>
          <nicname>port4</nicname>
        </myid>
        <nictype>port</nictype>
        <uniqueidentifier>106</uniqueidentifier>
        <usesdhcp>False</usesdhcp>
        <interface>
          <nicname>port4</nicname>
          <myip>
            <ip>0.0.0.0</ip>
            <mask>0.0.0.0</mask>
            <gateway>0.0.0.0</gateway>
            <type>ip</type>
          </myip>
          <VLAN
            ID="1">Untagged</VLAN>
          <VLAN
            ID="3">Forbidden</VLAN>
          <VLAN
            ID="2">Forbidden</VLAN>
        </interface>
      </nic>
      <nic>
        <nictype>port</nictype>
        <nicname>port5</nicname>
        <myid>
          <hostid>100</hostid>
          <nicid>107</nicid>
          <hostname>net_switch0</hostname>
          <nicname>port5</nicname>
        </myid>
        <nictype>port</nictype>
        <uniqueidentifier>107</uniqueidentifier>
        <usesdhcp>False</usesdhcp>
        <interface>
          <nicname>port5</nicname>
          <myip>
            <ip>0.0.0.0</ip>
            <mask>0.0.0.0</mask>
            <gateway>0.0.0.0</gateway>
            <type>ip</type>
          </myip>
          <VLAN
            ID="1">Forbidden</VLAN>
          <VLAN
            ID="2">Forbidden</VLAN>
          <VLAN
            ID="3">Untagged</VLAN>
        </interface>
      </nic>
      <nic>
        <nictype>port</nictype>
        <nicname>port6</nicname>
        <myid>
          <hostid>100</hostid>
          <nicid>108</nicid>
          <hostname>net_switch0</hostname>
          <nicname>port6</nicname>
        </myid>
        <nictype>port</nictype>
        <uniqueidentifier>108</uniqueidentifier>
        <usesdhcp>False</usesdhcp>
        <interface>
          <nicname>port6</nicname>
          <myip>
            <ip>0.0.0.0</ip>
            <mask>0.0.0.0</mask>
            <gateway>0.0.0.0</gateway>
            <type>ip</type>
          </myip>
          <VLAN
            ID="1">Forbidden</VLAN>
          <VLAN
            ID="3">Forbidden</VLAN>
          <VLAN
            ID="2">Untagged</VLAN>
        </interface>
      </nic>
      <nic>
        <nictype>port</nictype>
        <nicname>port7</nicname>
        <myid>
          <hostid>100</hostid>
          <nicid>109</nicid>
          <hostname>net_switch0</hostname>
          <nicname>port7</nicname>
        </myid>
        <nictype>port</nictype>
        <uniqueidentifier>109</uniqueidentifier>
        <usesdhcp>False</usesdhcp>
        <interface>
          <nicname>port7</nicname>
          <myip>
            <ip>0.0.0.0</ip>
            <mask>0.0.0.0</mask>
            <gateway>0.0.0.0</gateway>
            <type>ip</type>
          </myip>
          <VLAN
            ID="1">Tagged</VLAN>
          <VLAN
            ID="2">Tagged</VLAN>
          <VLAN
            ID="3">Tagged</VLAN>
        </interface>
      </nic>
    </device>
    <device>
      <hostname>net_switch1</hostname>
      <size>100</size>
      <uniqueidentifier>110</uniqueidentifier>
      <location>450,400</location>
      <mytype>net_switch</mytype>
      <isdns>False</isdns>
      <isdhcp>False</isdhcp>
      <gateway>
        <ip>192.168.1.1</ip>
        <mask>0.0.0.0</mask>
        <gateway>0.0.0.0</gateway>
        <type>gw</type>
      </gateway>
      <nic>
        <nictype>lo</nictype>
        <nicname>lo0</nicname>
        <myid>
          <hostid>110</hostid>
          <nicid>111</nicid>
          <hostname>net_switch1</hostname>
          <nicname>lo0</nicname>
        </myid>
        <nictype>lo</nictype>
        <uniqueidentifier>111</uniqueidentifier>
        <usesdhcp>False</usesdhcp>
        <interface>
          <nicname>lo0</nicname>
          <myip>
            <ip>127.0.0.1</ip>
            <mask>255.0.0.0</mask>
            <gateway>0.0.0.0</gateway>
            <type>ip</type>
          </myip>
          <VLAN
            ID="1">Untagged</VLAN>
        </interface>
      </nic>
      <nic>
        <nictype>management_interface</nictype>
        <nicname>management_interface0</nicname>
        <myid>
          <hostid>110</hostid>
          <nicid>112</nicid>
          <hostname>net_switch1</hostname>
          <nicname>management_interface0</nicname>
        </myid>
        <nictype>management_interface</nictype>
        <uniqueidentifier>112</uniqueidentifier>
        <usesdhcp>False</usesdhcp>
        <interface>
          <nicname>management_interface0</nicname>
          <myip>
            <ip>192.168.1.251</ip>
            <mask>255.255.255.0</mask>
            <gateway>0.0.0.0</gateway>
            <type>ip</type>
          </myip>
          <VLAN
            ID="1">Untagged</VLAN>
        </interface>
      </nic>
      <nic>
        <nictype>port</nictype>
        <nicname>port1</nicname>
        <myid>
          <hostid>110</hostid>
          <nicid>113</nicid>
          <hostname>net_switch1</hostname>
          <nicname>port1</nicname>
        </myid>
        <nictype>port</nictype>
        <uniqueidentifier>113</uniqueidentifier>
        <usesdhcp>False</usesdhcp>
        <interface>
          <nicname>port1</nicname>
          <myip>
            <ip>0.0.0.0</ip>
            <mask>0.0.0.0</mask>
            <gateway>0.0.0.0</gateway>
            <type>ip</type>
          </myip>
          <VLAN
            ID="1">Forbidden</VLAN>
          <VLAN
            ID="2">Untagged</VLAN>
          <VLAN
            ID="3">Forbidden</VLAN>
        </interface>
      </nic>
      <nic>
        <nictype>port</nictype>
        <nicname>port2</nicname>
        <myid>
          <hostid>110</hostid>
          <nicid>114</nicid>
          <hostname>net_switch1</hostname>
          <nicname>port2</nicname>
        </myid>
        <nictype>port</nictype>
        <uniqueidentifier>114</uniqueidentifier>
        <usesdhcp>False</usesdhcp>
        <interface>
          <nicname>port2</nicname>
          <myip>
            <ip>0.0.0.0</ip>
            <mask>0.0.0.0</mask>
            <gateway>0.0.0.0</gateway>
            <type>ip</type>
          </myip>
          <VLAN
            ID="1">Forbidden</VLAN>
          <VLAN
            ID="2">Untagged</VLAN>
          <VLAN
            ID="3">Forbidden</VLAN>
        </interface>
      </nic>
      <nic>
        <nictype>port</nictype>
        <nicname>port3</nicname>
        <myid>
          <hostid>110</hostid>
          <nicid>115</nicid>
          <hostname>net_switch1</hostname>
          <nicname>port3</nicname>
        </myid>
        <nictype>port</nictype>
        <uniqueidentifier>115</uniqueidentifier>
        <usesdhcp>False</usesdhcp>
        <interface>
          <nicname>port3</nicname>
          <myip>
            <ip>0.0.0.0</ip>
            <mask>0.0.0.0</mask>
            <gateway>0.0.0.0</gateway>
            <type>ip</type>
          </myip>
          <VLAN
            ID="1">Forbidden</VLAN>
          <VLAN
            ID="2">Untagged</VLAN>
          <VLAN
            ID="3">Forbidden</VLAN>
        </interface>
      </nic>
      <nic>
        <nictype>port</nictype>
        <nicname>port4</nicname>
        <myid>
          <hostid>110</hostid>
          <nicid>116</nicid>
          <hostname>net_switch1</hostname>
          <nicname>port4</nicname>
        </myid>
        <nictype>port</nictype>
        <uniqueidentifier>116</uniqueidentifier>
        <usesdhcp>False</usesdhcp>
        <interface>
          <nicname>port4</nicname>
          <myip>
            <ip>0.0.0.0</ip>
            <mask>0.0.0.0</mask>
            <gateway>0.0.0.0</gateway>
            <type>ip</type>
          </myip>
          <VLAN
            ID="1">Forbidden</VLAN>
          <VLAN
            ID="2">Untagged</VLAN>
          <VLAN
            ID="3">Forbidden</VLAN>
        </interface>
      </nic>
      <nic>
        <nictype>port</nictype>
        <nicname>port5</nicname>
        <myid>
          <hostid>110</hostid>
          <nicid>117</nicid>
          <hostname>net_switch1</hostname>
          <nicname>port5</nicname>
        </myid>
        <nictype>port</nictype>
        <uniqueidentifier>117</uniqueidentifier>
        <usesdhcp>False</usesdhcp>
        <interface>
          <nicname>port5</nicname>
          <myip>
            <ip>0.0.0.0</ip>
            <mask>0.0.0.0</mask>
            <gateway>0.0.0.0</gateway>
            <type>ip</type>
          </myip>
          <VLAN
            ID="1">Tagged</VLAN>
          <VLAN
            ID="2">Tagged</VLAN>
          <VLAN
            ID="3">Tagged</VLAN>
        </interface>
      </nic>
      <nic>
        <nictype>port</nictype>
        <nicname>port6</nicname>
        <myid>
          <hostid>110</hostid>
          <nicid>118</nicid>
          <hostname>net_switch1</hostname>
          <nicname>port6</nicname>
        </myid>
        <nictype>port</nictype>
        <uniqueidentifier>118</uniqueidentifier>
        <usesdhcp>False</usesdhcp>
        <interface>
          <nicname>port6</nicname>
          <myip>
            <ip>0.0.0.0</ip>
            <mask>0.0.0.0</mask>
            <gateway>0.0.0.0</gateway>
            <type>ip</type>
          </myip>
          <VLAN
            ID="1">Tagged</VLAN>
          <VLAN
            ID="2">Tagged</VLAN>
          <VLAN
            ID="3">Tagged</VLAN>
        </interface>
      </nic>
      <nic>
        <nictype>port</nictype>
        <nicname>port7</nicname>
        <myid>
          <hostid>110</hostid>
          <nicid>119</nicid>
          <hostname>net_switch1</hostname>
          <nicname>port7</nicname>
        </myid>
        <nictype>port</nictype>
        <uniqueidentifier>119</uniqueidentifier>
        <usesdhcp>False</usesdhcp>
        <interface>
          <nicname>port7</nicname>
          <myip>
            <ip>0.0.0.0</ip>
            <mask>0.0.0.0</mask>
            <gateway>0.0.0.0</gateway>
            <type>ip</type>
          </myip>
          <VLAN
            ID="1">Tagged</VLAN>
          <VLAN
            ID="2">Tagged</VLAN>
          <VLAN
            ID="3">Tagged</VLAN>
        </interface>
      </nic>
    </device>
    <device>
      <hostname>net_switch2</hostname>
      <size>100</size>
      <uniqueidentifier>120</uniqueidentifier>
      <location>690,430</location>
      <mytype>net_switch</mytype>
      <isdns>False</isdns>
      <isdhcp>False</isdhcp>
      <gateway>
        <ip>192.168.1.1</ip>
        <mask>0.0.0.0</mask>
        <gateway>0.0.0.0</gateway>
        <type>gw</type>
      </gateway>
      <nic>
        <nictype>lo</nictype>
        <nicname>lo0</nicname>
        <myid>
          <hostid>120</hostid>
          <nicid>121</nicid>
          <hostname>net_switch2</hostname>
          <nicname>lo0</nicname>
        </myid>
        <nictype>lo</nictype>
        <uniqueidentifier>121</uniqueidentifier>
        <usesdhcp>False</usesdhcp>
        <interface>
          <nicname>lo0</nicname>
          <myip>
            <ip>127.0.0.1</ip>
            <mask>255.0.0.0</mask>
            <gateway>0.0.0.0</gateway>
            <type>ip</type>
          </myip>
          <VLAN
            ID="1">Untagged</VLAN>
        </interface>
      </nic>
      <nic>
        <nictype>management_interface</nictype>
        <nicname>management_interface0</nicname>
        <myid>
          <hostid>120</hostid>
          <nicid>122</nicid>
          <hostname>net_switch2</hostname>
          <nicname>management_interface0</nicname>
        </myid>
        <nictype>management_interface</nictype>
        <uniqueidentifier>122</uniqueidentifier>
        <usesdhcp>False</usesdhcp>
        <interface>
          <nicname>management_interface0</nicname>
          <myip>
            <ip>192.168.1.250</ip>
            <mask>255.255.255.0</mask>
            <gateway>0.0.0.0</gateway>
            <type>ip</type>
          </myip>
          <VLAN
            ID="1">Untagged</VLAN>
        </interface>
      </nic>
      <nic>
        <nictype>port</nictype>
        <nicname>port1</nicname>
        <myid>
          <hostid>120</hostid>
          <nicid>123</nicid>
          <hostname>net_switch2</hostname>
          <nicname>port1</nicname>
        </myid>
        <nictype>port</nictype>
        <uniqueidentifier>123</uniqueidentifier>
        <usesdhcp>False</usesdhcp>
        <interface>
          <nicname>port1</nicname>
          <myip>
            <ip>0.0.0.0</ip>
            <mask>0.0.0.0</mask>
            <gateway>0.0.0.0</gateway>
            <type>ip</type>
          </myip>
          <VLAN
            ID="1">Forbidden</VLAN>
          <VLAN
            ID="3">Untagged</VLAN>
          <VLAN
            ID="2">Forbidden</VLAN>
        </interface>
      </nic>
      <nic>
        <nictype>port</nictype>
        <nicname>port2</nicname>
        <myid>
          <hostid>120</hostid>
          <nicid>124</nicid>
          <hostname>net_switch2</hostname>
          <nicname>port2</nicname>
        </myid>
        <nictype>port</nictype>
        <uniqueidentifier>124</uniqueidentifier>
        <usesdhcp>False</usesdhcp>
        <interface>
          <nicname>port2</nicname>
          <myip>
            <ip>0.0.0.0</ip>
            <mask>0.0.0.0</mask>
            <gateway>0.0.0.0</gateway>
            <type>ip</type>
          </myip>
          <VLAN
            ID="1">Forbidden</VLAN>
          <VLAN
            ID="3">Untagged</VLAN>
          <VLAN
            ID="2">Forbidden</VLAN>
        </interface>
      </nic>
      <nic>
        <nictype>port</nictype>
        <nicname>port3</nicname>
        <myid>
          <hostid>120</hostid>
          <nicid>125</nicid>
          <hostname>net_switch2</hostname>
          <nicname>port3</nicname>
        </myid>
        <nictype>port</nictype>
        <uniqueidentifier>125</uniqueidentifier>
        <usesdhcp>False</usesdhcp>
        <interface>
          <nicname>port3</nicname>
          <myip>
            <ip>0.0.0.0</ip>
            <mask>0.0.0.0</mask>
            <gateway>0.0.0.0</gateway>
            <type>ip</type>
          </myip>
          <VLAN
            ID="1">Forbidden</VLAN>
          <VLAN
            ID="3">Untagged</VLAN>
          <VLAN
            ID="2">Forbidden</VLAN>
        </interface>
      </nic>
      <nic>
        <nictype>port</nictype>
        <nicname>port4</nicname>
        <myid>
          <hostid>120</hostid>
          <nicid>126</nicid>
          <hostname>net_switch2</hostname>
          <nicname>port4</nicname>
        </myid>
        <nictype>port</nictype>
        <uniqueidentifier>126</uniqueidentifier>
        <usesdhcp>False</usesdhcp>
        <interface>
          <nicname>port4</nicname>
          <myip>
            <ip>0.0.0.0</ip>
            <mask>0.0.0.0</mask>
            <gateway>0.0.0.0</gateway>
            <type>ip</type>
          </myip>
          <VLAN
            ID="1">Forbidden</VLAN>
          <VLAN
            ID="3">Untagged</VLAN>
          <VLAN
            ID="2">Forbidden</VLAN>
        </interface>
      </nic>
      <nic>
        <nictype>port</nictype>
        <nicname>port5</nicname>
        <myid>
          <hostid>120</hostid>
          <nicid>127</nicid>
          <hostname>net_switch2</hostname>
          <nicname>port5</nicname>
        </myid>
        <nictype>port</nictype>
        <uniqueidentifier>127</uniqueidentifier>
        <usesdhcp>False</usesdhcp>
        <interface>
          <nicname>port5</nicname>
          <myip>
            <ip>0.0.0.0</ip>
            <mask>0.0.0.0</mask>
            <gateway>0.0.0.0</gateway>
            <type>ip</type>
          </myip>
          <VLAN
            ID="1">Tagged</VLAN>
          <VLAN
            ID="3">Tagged</VLAN>
          <VLAN
            ID="2">Tagged</VLAN>
        </interface>
      </nic>
      <nic>
        <nictype>port</nictype>
        <nicname>port6</nicname>
        <myid>
          <hostid>120</hostid>
          <nicid>128</nicid>
          <hostname>net_switch2</hostname>
          <nicname>port6</nicname>
        </myid>
        <nictype>port</nictype>
        <uniqueidentifier>128</uniqueidentifier>
        <usesdhcp>False</usesdhcp>
        <interface>
          <nicname>port6</nicname>
          <myip>
            <ip>0.0.0.0</ip>
            <mask>0.0.0.0</mask>
            <gateway>0.0.0.0</gateway>
            <type>ip</type>
          </myip>
          <VLAN
            ID="1">Tagged</VLAN>
          <VLAN
            ID="3">Tagged</VLAN>
          <VLAN
            ID="2">Tagged</VLAN>
        </interface>
      </nic>
      <nic>
        <nictype>port</nictype>
        <nicname>port7</nicname>
        <myid>
          <hostid>120</hostid>
          <nicid>129</nicid>
          <hostname>net_switch2</hostname>
          <nicname>port7</nicname>
        </myid>
        <nictype>port</nictype>
        <uniqueidentifier>129</uniqueidentifier>
        <usesdhcp>False</usesdhcp>
        <interface>
          <nicname>port7</nicname>
          <myip>
            <ip>0.0.0.0</ip>
            <mask>0.0.0.0</mask>
            <gateway>0.0.0.0</gateway>
            <type>ip</type>
          </myip>
          <VLAN
            ID="1">Tagged</VLAN>
          <VLAN
            ID="3">Tagged</VLAN>
          <VLAN
            ID="2">Tagged</VLAN>
        </interface>
      </nic>
    </device>
    <device>
      <hostname>pc2</hostname>
      <size>100</size>
      <uniqueidentifier>136</uniqueidentifier>
      <location>370,690</location>
      <mytype>pc</mytype>
      <isdns>False</isdns>
      <isdhcp>False</isdhcp>
      <morphcolor>Green</morphcolor>
      <gateway>
        <ip>192.168.2.1</ip>
        <mask>0.0.0.0</mask>
        <gateway>0.0.0.0</gateway>
        <type>gw</type>
      </gateway>
      <nic>
        <nictype>lo</nictype>
        <nicname>lo0</nicname>
        <myid>
          <hostid>136</hostid>
          <nicid>137</nicid>
          <hostname>pc2</hostname>
          <nicname>lo0</nicname>
        </myid>
        <nictype>lo</nictype>
        <uniqueidentifier>137</uniqueidentifier>
        <usesdhcp>False</usesdhcp>
        <interface>
          <nicname>lo0</nicname>
          <myip>
            <ip>127.0.0.1</ip>
            <mask>255.0.0.0</mask>
            <gateway>0.0.0.0</gateway>
            <type>ip</type>
          </myip>
          <VLAN
            ID="1">Untagged</VLAN>
        </interface>
      </nic>
      <nic>
        <nictype>eth</nictype>
        <nicname>eth0</nicname>
        <myid>
          <hostid>136</hostid>
          <nicid>138</nicid>
          <hostname>pc2</hostname>
          <nicname>eth0</nicname>
        </myid>
        <nictype>eth</nictype>
        <uniqueidentifier>138</uniqueidentifier>
        <usesdhcp>False</usesdhcp>
        <interface>
          <nicname>eth0</nicname>
          <myip>
            <ip>192.168.2.3</ip>
            <mask>255.255.255.0</mask>
            <gateway>0.0.0.0</gateway>
            <type>ip</type>
          </myip>
          <VLAN
            ID="1">Untagged</VLAN>
        </interface>
      </nic>
    </device>
    <device>
      <hostname>pc3</hostname>
      <size>100</size>
      <uniqueidentifier>139</uniqueidentifier>
      <location>510,820</location>
      <mytype>pc</mytype>
      <isdns>False</isdns>
      <isdhcp>False</isdhcp>
      <morphcolor>Green</morphcolor>
      <gateway>
        <ip>192.168.2.1</ip>
        <mask>0.0.0.0</mask>
        <gateway>0.0.0.0</gateway>
        <type>gw</type>
      </gateway>
      <nic>
        <nictype>lo</nictype>
        <nicname>lo0</nicname>
        <myid>
          <hostid>139</hostid>
          <nicid>140</nicid>
          <hostname>pc3</hostname>
          <nicname>lo0</nicname>
        </myid>
        <nictype>lo</nictype>
        <uniqueidentifier>140</uniqueidentifier>
        <usesdhcp>False</usesdhcp>
        <interface>
          <nicname>lo0</nicname>
          <myip>
            <ip>127.0.0.1</ip>
            <mask>255.0.0.0</mask>
            <gateway>0.0.0.0</gateway>
            <type>ip</type>
          </myip>
          <VLAN
            ID="1">Untagged</VLAN>
        </interface>
      </nic>
      <nic>
        <nictype>eth</nictype>
        <nicname>eth0</nicname>
        <myid>
          <hostid>139</hostid>
          <nicid>141</nicid>
          <hostname>pc3</hostname>
          <nicname>eth0</nicname>
        </myid>
        <nictype>eth</nictype>
        <uniqueidentifier>141</uniqueidentifier>
        <usesdhcp>True</usesdhcp>
        <interface>
          <nicname>eth0</nicname>
          <myip>
            <ip>0.0.0.0</ip>
            <mask>0.0.0.0</mask>
            <gateway>0.0.0.0</gateway>
            <type>ip</type>
          </myip>
          <VLAN
            ID="1">Untagged</VLAN>
        </interface>
      </nic>
    </device>
    <device>
      <hostname>pc4</hostname>
      <size>100</size>
      <uniqueidentifier>142</uniqueidentifier>
      <location>830,600</location>
      <mytype>pc</mytype>
      <isdns>False</isdns>
      <isdhcp>False</isdhcp>
      <morphcolor>Yellow</morphcolor>
      <gateway>
        <ip>192.168.3.1</ip>
        <mask>0.0.0.0</mask>
        <gateway>0.0.0.0</gateway>
        <type>gw</type>
      </gateway>
      <nic>
        <nictype>lo</nictype>
        <nicname>lo0</nicname>
        <myid>
          <hostid>142</hostid>
          <nicid>143</nicid>
          <hostname>pc4</hostname>
          <nicname>lo0</nicname>
        </myid>
        <nictype>lo</nictype>
        <uniqueidentifier>143</uniqueidentifier>
        <usesdhcp>False</usesdhcp>
        <interface>
          <nicname>lo0</nicname>
          <myip>
            <ip>127.0.0.1</ip>
            <mask>255.0.0.0</mask>
            <gateway>0.0.0.0</gateway>
            <type>ip</type>
          </myip>
          <VLAN
            ID="1">Untagged</VLAN>
        </interface>
      </nic>
      <nic>
        <nictype>eth</nictype>
        <nicname>eth0</nicname>
        <myid>
          <hostid>142</hostid>
          <nicid>144</nicid>
          <hostname>pc4</hostname>
          <nicname>eth0</nicname>
        </myid>
        <nictype>eth</nictype>
        <uniqueidentifier>144</uniqueidentifier>
        <usesdhcp>False</usesdhcp>
        <interface>
          <nicname>eth0</nicname>
          <myip>
            <ip>192.168.3.3</ip>
            <mask>255.255.255.0</mask>
            <gateway>0.0.0.0</gateway>
            <type>ip</type>
          </myip>
          <VLAN
            ID="1">Untagged</VLAN>
        </interface>
      </nic>
    </device>
    <device>
      <hostname>pc5</hostname>
      <size>100</size>
      <uniqueidentifier>145</uniqueidentifier>
      <location>820,770</location>
      <mytype>pc</mytype>
      <isdns>False</isdns>
      <isdhcp>False</isdhcp>
      <morphcolor>Yellow</morphcolor>
      <gateway>
        <ip>192.168.3.1</ip>
        <mask>0.0.0.0</mask>
        <gateway>0.0.0.0</gateway>
        <type>gw</type>
      </gateway>
      <nic>
        <nictype>lo</nictype>
        <nicname>lo0</nicname>
        <myid>
          <hostid>145</hostid>
          <nicid>146</nicid>
          <hostname>pc5</hostname>
          <nicname>lo0</nicname>
        </myid>
        <nictype>lo</nictype>
        <uniqueidentifier>146</uniqueidentifier>
        <usesdhcp>False</usesdhcp>
        <interface>
          <nicname>lo0</nicname>
          <myip>
            <ip>127.0.0.1</ip>
            <mask>255.0.0.0</mask>
            <gateway>0.0.0.0</gateway>
            <type>ip</type>
          </myip>
          <VLAN
            ID="1">Untagged</VLAN>
        </interface>
      </nic>
      <nic>
        <nictype>eth</nictype>
        <nicname>eth0</nicname>
        <myid>
          <hostid>145</hostid>
          <nicid>147</nicid>
          <hostname>pc5</hostname>
          <nicname>eth0</nicname>
        </myid>
        <nictype>eth</nictype>
        <uniqueidentifier>147</uniqueidentifier>
        <usesdhcp>True</usesdhcp>
        <interface>
          <nicname>eth0</nicname>
          <myip>
            <ip>0.0.0.0</ip>
            <mask>0.0.0.0</mask>
            <gateway>0.0.0.0</gateway>
            <type>ip</type>
          </myip>
          <VLAN
            ID="1">Untagged</VLAN>
        </interface>
      </nic>
    </device>
    <device>
      <hostname>pc6</hostname>
      <size>100</size>
      <uniqueidentifier>166</uniqueidentifier>
      <location>820,40</location>
      <mytype>pc</mytype>
      <isdns>False</isdns>
      <isdhcp>False</isdhcp>
      <gateway>
        <ip>10.0.1.1</ip>
        <mask>0.0.0.0</mask>
        <gateway>0.0.0.0</gateway>
        <type>gw</type>
      </gateway>
      <nic>
        <nictype>lo</nictype>
        <nicname>lo0</nicname>
        <myid>
          <hostid>166</hostid>
          <nicid>167</nicid>
          <hostname>pc6</hostname>
          <nicname>lo0</nicname>
        </myid>
        <nictype>lo</nictype>
        <uniqueidentifier>167</uniqueidentifier>
        <usesdhcp>False</usesdhcp>
        <encryptionkey />
        <ssid />
        <interface>
          <nicname>lo0</nicname>
          <myip>
            <ip>127.0.0.1</ip>
            <mask>255.0.0.0</mask>
            <gateway>0.0.0.0</gateway>
            <type>ip</type>
          </myip>
          <VLAN
            ID="1">Untagged</VLAN>
        </interface>
      </nic>
      <nic>
        <nictype>eth</nictype>
        <nicname>eth0</nicname>
        <myid>
          <hostid>166</hostid>
          <nicid>168</nicid>
          <hostname>pc6</hostname>
          <nicname>eth0</nicname>
        </myid>
        <nictype>eth</nictype>
        <uniqueidentifier>168</uniqueidentifier>
        <usesdhcp>False</usesdhcp>
        <encryptionkey />
        <ssid />
        <interface>
          <nicname>eth0</nicname>
          <myip>
            <ip>10.0.1.2</ip>
            <mask>255.255.255.0</mask>
            <gateway>0.0.0.0</gateway>
            <type>ip</type>
          </myip>
          <VLAN
            ID="1">Untagged</VLAN>
        </interface>
      </nic>
    </device>
    <device>
      <hostname>router0</hostname>
      <size>100</size>
      <uniqueidentifier>162</uniqueidentifier>
      <location>570,40</location>
      <mytype>router</mytype>
      <isdns>False</isdns>
      <isdhcp>False</isdhcp>
      <gateway>
        <ip>0.0.0.0</ip>
        <mask>0.0.0.0</mask>
        <gateway>0.0.0.0</gateway>
        <type>gw</type>
      </gateway>
      <nic>
        <nictype>lo</nictype>
        <nicname>lo0</nicname>
        <myid>
          <hostid>162</hostid>
          <nicid>163</nicid>
          <hostname>router0</hostname>
          <nicname>lo0</nicname>
        </myid>
        <nictype>lo</nictype>
        <uniqueidentifier>163</uniqueidentifier>
        <usesdhcp>False</usesdhcp>
        <encryptionkey />
        <ssid />
        <interface>
          <nicname>lo0</nicname>
          <myip>
            <ip>127.0.0.1</ip>
            <mask>255.0.0.0</mask>
            <gateway>0.0.0.0</gateway>
            <type>ip</type>
          </myip>
          <VLAN
            ID="1">Untagged</VLAN>
        </interface>
      </nic>
      <nic>
        <nictype>eth</nictype>
        <nicname>eth0</nicname>
        <myid>
          <hostid>162</hostid>
          <nicid>164</nicid>
          <hostname>router0</hostname>
          <nicname>eth0</nicname>
        </myid>
        <nictype>eth</nictype>
        <uniqueidentifier>164</uniqueidentifier>
        <usesdhcp>False</usesdhcp>
        <encryptionkey />
        <ssid />
        <interface>
          <nicname>eth0</nicname>
          <myip>
            <ip>10.0.0.1</ip>
            <mask>255.255.255.0</mask>
            <gateway>0.0.0.0</gateway>
            <type>ip</type>
          </myip>
          <VLAN
            ID="1">Untagged</VLAN>
        </interface>
      </nic>
      <nic>
        <nictype>eth</nictype>
        <nicname>eth1</nicname>
        <myid>
          <hostid>162</hostid>
          <nicid>165</nicid>
          <hostname>router0</hostname>
          <nicname>eth1</nicname>
        </myid>
        <nictype>eth</nictype>
        <uniqueidentifier>165</uniqueidentifier>
        <usesdhcp>False</usesdhcp>
        <encryptionkey />
        <ssid />
        <interface>
          <nicname>eth1</nicname>
          <myip>
            <ip>10.0.1.1</ip>
            <mask>255.255.255.0</mask>
            <gateway>0.0.0.0</gateway>
            <type>ip</type>
          </myip>
          <VLAN
            ID="1">Untagged</VLAN>
        </interface>
      </nic>
      <route>
        <ip>192.168.3.0</ip>
        <mask>255.255.255.0</mask>
        <gateway>10.0.0.2</gateway>
        <type>route</type>
      </route>
      <route>
        <ip>192.168.2.0</ip>
        <mask>255.255.255.0</mask>
        <gateway>10.0.0.2</gateway>
        <type>route</type>
      </route>
      <route>
        <ip>192.168.1.0</ip>
        <mask>255.255.255.0</mask>
        <gateway>10.0.0.2</gateway>
        <type>route</type>
      </route>
    </device>
    <device>
      <hostname>wap0</hostname>
      <size>100</size>
      <uniqueidentifier>171</uniqueidentifier>
      <location>130,320</location>
      <mytype>wap</mytype>
      <isdns>False</isdns>
      <isdhcp>False</isdhcp>
      <morphcolor>Yellow</morphcolor>
      <gateway>
        <ip>192.168.3.1</ip>
        <mask>0.0.0.0</mask>
        <gateway>0.0.0.0</gateway>
        <type>gw</type>
      </gateway>
      <nic>
        <nictype>lo</nictype>
        <nicname>lo0</nicname>
        <myid>
          <hostid>171</hostid>
          <nicid>174</nicid>
          <hostname>wap0</hostname>
          <nicname>lo0</nicname>
        </myid>
        <nictype>lo</nictype>
        <uniqueidentifier>174</uniqueidentifier>
        <usesdhcp>False</usesdhcp>
        <encryptionkey />
        <ssid />
        <interface>
          <nicname>lo0</nicname>
          <myip>
            <ip>127.0.0.1</ip>
            <mask>255.0.0.0</mask>
            <gateway>0.0.0.0</gateway>
            <type>ip</type>
          </myip>
          <VLAN
            ID="1">Untagged</VLAN>
        </interface>
      </nic>
      <nic>
        <nictype>eth</nictype>
        <nicname>eth1</nicname>
        <myid>
          <hostid>171</hostid>
          <nicid>175</nicid>
          <hostname>wap0</hostname>
          <nicname>eth1</nicname>
        </myid>
        <nictype>eth</nictype>
        <uniqueidentifier>175</uniqueidentifier>
        <usesdhcp>False</usesdhcp>
        <encryptionkey />
        <ssid />
        <interface>
          <nicname>eth1</nicname>
          <myip>
            <ip>192.168.3.10</ip>
            <mask>255.255.255.0</mask>
            <gateway>0.0.0.0</gateway>
            <type>ip</type>
          </myip>
          <VLAN
            ID="1">Untagged</VLAN>
        </interface>
      </nic>
      <nic>
        <nictype>wport</nictype>
        <nicname>wport2</nicname>
        <myid>
          <hostid>171</hostid>
          <nicid>176</nicid>
          <hostname>wap0</hostname>
          <nicname>wport2</nicname>
        </myid>
        <nictype>wport</nictype>
        <uniqueidentifier>176</uniqueidentifier>
        <usesdhcp>False</usesdhcp>
        <encryptionkey>TheKey</encryptionkey>
        <ssid>Students</ssid>
        <interface>
          <nicname>wport2</nicname>
          <myip>
            <ip>0.0.0.0</ip>
            <mask>0.0.0.0</mask>
            <gateway>0.0.0.0</gateway>
            <type>ip</type>
          </myip>
          <VLAN
            ID="1">Untagged</VLAN>
        </interface>
      </nic>
      <nic>
        <nictype>wport</nictype>
        <nicname>wport3</nicname>
        <myid>
          <hostid>171</hostid>
          <nicid>177</nicid>
          <hostname>wap0</hostname>
          <nicname>wport3</nicname>
        </myid>
        <nictype>wport</nictype>
        <uniqueidentifier>177</uniqueidentifier>
        <usesdhcp>False</usesdhcp>
        <encryptionkey>TheKey</encryptionkey>
        <ssid>Students</ssid>
        <interface>
          <nicname>wport3</nicname>
          <myip>
            <ip>0.0.0.0</ip>
            <mask>0.0.0.0</mask>
            <gateway>0.0.0.0</gateway>
            <type>ip</type>
          </myip>
          <VLAN
            ID="1">Untagged</VLAN>
        </interface>
      </nic>
      <nic>
        <nictype>wport</nictype>
        <nicname>wport4</nicname>
        <myid>
          <hostid>171</hostid>
          <nicid>178</nicid>
          <hostname>wap0</hostname>
          <nicname>wport4</nicname>
        </myid>
        <nictype>wport</nictype>
        <uniqueidentifier>178</uniqueidentifier>
        <usesdhcp>False</usesdhcp>
        <encryptionkey>TheKey</encryptionkey>
        <ssid>Students</ssid>
        <interface>
          <nicname>wport4</nicname>
          <myip>
            <ip>0.0.0.0</ip>
            <mask>0.0.0.0</mask>
            <gateway>0.0.0.0</gateway>
            <type>ip</type>
          </myip>
          <VLAN
            ID="1">Untagged</VLAN>
        </interface>
      </nic>
      <nic>
        <nictype>wport</nictype>
        <nicname>wport5</nicname>
        <myid>
          <hostid>171</hostid>
          <nicid>179</nicid>
          <hostname>wap0</hostname>
          <nicname>wport5</nicname>
        </myid>
        <nictype>wport</nictype>
        <uniqueidentifier>179</uniqueidentifier>
        <usesdhcp>False</usesdhcp>
        <encryptionkey>TheKey</encryptionkey>
        <ssid>Students</ssid>
        <interface>
          <nicname>wport5</nicname>
          <myip>
            <ip>0.0.0.0</ip>
            <mask>0.0.0.0</mask>
            <gateway>0.0.0.0</gateway>
            <type>ip</type>
          </myip>
          <VLAN
            ID="1">Untagged</VLAN>
        </interface>
      </nic>
      <nic>
        <nictype>wport</nictype>
        <nicname>wport6</nicname>
        <myid>
          <hostid>171</hostid>
          <nicid>180</nicid>
          <hostname>wap0</hostname>
          <nicname>wport6</nicname>
        </myid>
        <nictype>wport</nictype>
        <uniqueidentifier>180</uniqueidentifier>
        <usesdhcp>False</usesdhcp>
        <encryptionkey>TheKey</encryptionkey>
        <ssid>Students</ssid>
        <interface>
          <nicname>wport6</nicname>
          <myip>
            <ip>0.0.0.0</ip>
            <mask>0.0.0.0</mask>
            <gateway>0.0.0.0</gateway>
            <type>ip</type>
          </myip>
          <VLAN
            ID="1">Untagged</VLAN>
        </interface>
      </nic>
      <nic>
        <nictype>wport</nictype>
        <nicname>wport7</nicname>
        <myid>
          <hostid>171</hostid>
          <nicid>181</nicid>
          <hostname>wap0</hostname>
          <nicname>wport7</nicname>
        </myid>
        <nictype>wport</nictype>
        <uniqueidentifier>181</uniqueidentifier>
        <usesdhcp>False</usesdhcp>
        <encryptionkey>TheKey</encryptionkey>
        <ssid>Students</ssid>
        <interface>
          <nicname>wport7</nicname>
          <myip>
            <ip>0.0.0.0</ip>
            <mask>0.0.0.0</mask>
            <gateway>0.0.0.0</gateway>
            <type>ip</type>
          </myip>
          <VLAN
            ID="1">Untagged</VLAN>
        </interface>
      </nic>
    </device>
    <device>
      <hostname>wap1</hostname>
      <size>100</size>
      <uniqueidentifier>182</uniqueidentifier>
      <location>140,600</location>
      <mytype>wap</mytype>
      <isdns>False</isdns>
      <isdhcp>False</isdhcp>
      <morphcolor>Green</morphcolor>
      <gateway>
        <ip>192.168.2.1</ip>
        <mask>0.0.0.0</mask>
        <gateway>0.0.0.0</gateway>
        <type>gw</type>
      </gateway>
      <nic>
        <nictype>lo</nictype>
        <nicname>lo0</nicname>
        <myid>
          <hostid>182</hostid>
          <nicid>185</nicid>
          <hostname>wap1</hostname>
          <nicname>lo0</nicname>
        </myid>
        <nictype>lo</nictype>
        <uniqueidentifier>185</uniqueidentifier>
        <usesdhcp>False</usesdhcp>
        <encryptionkey />
        <ssid />
        <interface>
          <nicname>lo0</nicname>
          <myip>
            <ip>127.0.0.1</ip>
            <mask>255.0.0.0</mask>
            <gateway>0.0.0.0</gateway>
            <type>ip</type>
          </myip>
          <VLAN
            ID="1">Untagged</VLAN>
        </interface>
      </nic>
      <nic>
        <nictype>eth</nictype>
        <nicname>eth1</nicname>
        <myid>
          <hostid>182</hostid>
          <nicid>186</nicid>
          <hostname>wap1</hostname>
          <nicname>eth1</nicname>
        </myid>
        <nictype>eth</nictype>
        <uniqueidentifier>186</uniqueidentifier>
        <usesdhcp>False</usesdhcp>
        <encryptionkey />
        <ssid />
        <interface>
          <nicname>eth1</nicname>
          <myip>
            <ip>192.168.2.10</ip>
            <mask>255.255.255.0</mask>
            <gateway>0.0.0.0</gateway>
            <type>ip</type>
          </myip>
          <VLAN
            ID="1">Untagged</VLAN>
        </interface>
      </nic>
      <nic>
        <nictype>wport</nictype>
        <nicname>wport2</nicname>
        <myid>
          <hostid>182</hostid>
          <nicid>187</nicid>
          <hostname>wap1</hostname>
          <nicname>wport2</nicname>
        </myid>
        <nictype>wport</nictype>
        <uniqueidentifier>187</uniqueidentifier>
        <usesdhcp>False</usesdhcp>
        <encryptionkey>OtherKey</encryptionkey>
        <ssid>Staff</ssid>
        <interface>
          <nicname>wport2</nicname>
          <myip>
            <ip>0.0.0.0</ip>
            <mask>0.0.0.0</mask>
            <gateway>0.0.0.0</gateway>
            <type>ip</type>
          </myip>
          <VLAN
            ID="1">Untagged</VLAN>
        </interface>
      </nic>
      <nic>
        <nictype>wport</nictype>
        <nicname>wport3</nicname>
        <myid>
          <hostid>182</hostid>
          <nicid>188</nicid>
          <hostname>wap1</hostname>
          <nicname>wport3</nicname>
        </myid>
        <nictype>wport</nictype>
        <uniqueidentifier>188</uniqueidentifier>
        <usesdhcp>False</usesdhcp>
        <encryptionkey>OtherKey</encryptionkey>
        <ssid>Staff</ssid>
        <interface>
          <nicname>wport3</nicname>
          <myip>
            <ip>0.0.0.0</ip>
            <mask>0.0.0.0</mask>
            <gateway>0.0.0.0</gateway>
            <type>ip</type>
          </myip>
          <VLAN
            ID="1">Untagged</VLAN>
        </interface>
      </nic>
      <nic>
        <nictype>wport</nictype>
        <nicname>wport4</nicname>
        <myid>
          <hostid>182</hostid>
          <nicid>189</nicid>
          <hostname>wap1</hostname>
          <nicname>wport4</nicname>
        </myid>
        <nictype>wport</nictype>
        <uniqueidentifier>189</uniqueidentifier>
        <usesdhcp>False</usesdhcp>
        <encryptionkey>OtherKey</encryptionkey>
        <ssid>Staff</ssid>
        <interface>
          <nicname>wport4</nicname>
          <myip>
            <ip>0.0.0.0</ip>
            <mask>0.0.0.0</mask>
            <gateway>0.0.0.0</gateway>
            <type>ip</type>
          </myip>
          <VLAN
            ID="1">Untagged</VLAN>
        </interface>
      </nic>
      <nic>
        <nictype>wport</nictype>
        <nicname>wport5</nicname>
        <myid>
          <hostid>182</hostid>
          <nicid>190</nicid>
          <hostname>wap1</hostname>
          <nicname>wport5</nicname>
        </myid>
        <nictype>wport</nictype>
        <uniqueidentifier>190</uniqueidentifier>
        <usesdhcp>False</usesdhcp>
        <encryptionkey>OtherKey</encryptionkey>
        <ssid>Staff</ssid>
        <interface>
          <nicname>wport5</nicname>
          <myip>
            <ip>0.0.0.0</ip>
            <mask>0.0.0.0</mask>
            <gateway>0.0.0.0</gateway>
            <type>ip</type>
          </myip>
          <VLAN
            ID="1">Untagged</VLAN>
        </interface>
      </nic>
      <nic>
        <nictype>wport</nictype>
        <nicname>wport6</nicname>
        <myid>
          <hostid>182</hostid>
          <nicid>191</nicid>
          <hostname>wap1</hostname>
          <nicname>wport6</nicname>
        </myid>
        <nictype>wport</nictype>
        <uniqueidentifier>191</uniqueidentifier>
        <usesdhcp>False</usesdhcp>
        <encryptionkey>OtherKey</encryptionkey>
        <ssid>Staff</ssid>
        <interface>
          <nicname>wport6</nicname>
          <myip>
            <ip>0.0.0.0</ip>
            <mask>0.0.0.0</mask>
            <gateway>0.0.0.0</gateway>
            <type>ip</type>
          </myip>
          <VLAN
            ID="1">Untagged</VLAN>
        </interface>
      </nic>
      <nic>
        <nictype>wport</nictype>
        <nicname>wport7</nicname>
        <myid>
          <hostid>182</hostid>
          <nicid>192</nicid>
          <hostname>wap1</hostname>
          <nicname>wport7</nicname>
        </myid>
        <nictype>wport</nictype>
        <uniqueidentifier>192</uniqueidentifier>
        <usesdhcp>False</usesdhcp>
        <encryptionkey>OtherKey</encryptionkey>
        <ssid>Staff</ssid>
        <interface>
          <nicname>wport7</nicname>
          <myip>
            <ip>0.0.0.0</ip>
            <mask>0.0.0.0</mask>
            <gateway>0.0.0.0</gateway>
            <type>ip</type>
          </myip>
          <VLAN
            ID="1">Untagged</VLAN>
        </interface>
      </nic>
    </device>
    <link>
      <SrcNic>
        <hostid>100</hostid>
        <nicid>109</nicid>
        <hostname>net_switch0</hostname>
        <nicname>port7</nicname>
      </SrcNic>
      <DstNic>
        <hostid>110</hostid>
        <nicid>118</nicid>
        <hostname>net_switch1</hostname>
        <nicname>port6</nicname>
      </DstNic>
      <hostname />
      <linktype>normal</linktype>
      <uniqueidentifier>153</uniqueidentifier>
    </link>
    <link>
      <SrcNic>
        <hostid>182</hostid>
        <nicid>186</nicid>
        <hostname>wap1</hostname>
        <nicname>eth1</nicname>
      </SrcNic>
      <DstNic>
        <hostid>100</hostid>
        <nicid>108</nicid>
        <hostname>net_switch0</hostname>
        <nicname>port6</nicname>
      </DstNic>
      <hostname />
      <linktype>normal</linktype>
      <uniqueidentifier>193</uniqueidentifier>
    </link>
    <link>
      <SrcNic>
        <hostid>145</hostid>
        <nicid>147</nicid>
        <hostname>pc5</hostname>
        <nicname>eth0</nicname>
      </SrcNic>
      <DstNic>
        <hostid>120</hostid>
        <nicid>123</nicid>
        <hostname>net_switch2</hostname>
        <nicname>port1</nicname>
      </DstNic>
      <hostname />
      <linktype>normal</linktype>
      <uniqueidentifier>159</uniqueidentifier>
    </link>
    <link>
      <SrcNic>
        <hostid>139</hostid>
        <nicid>141</nicid>
        <hostname>pc3</hostname>
        <nicname>eth0</nicname>
      </SrcNic>
      <DstNic>
        <hostid>110</hostid>
        <nicid>114</nicid>
        <hostname>net_switch1</hostname>
        <nicname>port2</nicname>
      </DstNic>
      <hostname />
      <linktype>normal</linktype>
      <uniqueidentifier>158</uniqueidentifier>
    </link>
    <link>
      <SrcNic>
        <hostid>136</hostid>
        <nicid>138</nicid>
        <hostname>pc2</hostname>
        <nicname>eth0</nicname>
      </SrcNic>
      <DstNic>
        <hostid>110</hostid>
        <nicid>113</nicid>
        <hostname>net_switch1</hostname>
        <nicname>port1</nicname>
      </DstNic>
      <hostname />
      <linktype>normal</linktype>
      <uniqueidentifier>157</uniqueidentifier>
    </link>
    <link>
      <SrcNic>
        <hostid>110</hostid>
        <nicid>117</nicid>
        <hostname>net_switch1</hostname>
        <nicname>port5</nicname>
      </SrcNic>
      <DstNic>
        <hostid>148</hostid>
        <nicid>150</nicid>
        <hostname>firewall0</hostname>
        <nicname>eth0</nicname>
      </DstNic>
      <hostname />
      <linktype>normal</linktype>
      <uniqueidentifier>161</uniqueidentifier>
    </link>
    <link>
      <SrcNic>
        <hostid>110</hostid>
        <nicid>119</nicid>
        <hostname>net_switch1</hostname>
        <nicname>port7</nicname>
      </SrcNic>
      <DstNic>
        <hostid>120</hostid>
        <nicid>128</nicid>
        <hostname>net_switch2</hostname>
        <nicname>port6</nicname>
      </DstNic>
      <hostname />
      <linktype>normal</linktype>
      <uniqueidentifier>154</uniqueidentifier>
    </link>
    <link>
      <SrcNic>
        <hostid>142</hostid>
        <nicid>144</nicid>
        <hostname>pc4</hostname>
        <nicname>eth0</nicname>
      </SrcNic>
      <DstNic>
        <hostid>120</hostid>
        <nicid>124</nicid>
        <hostname>net_switch2</hostname>
        <nicname>port2</nicname>
      </DstNic>
      <hostname />
      <linktype>normal</linktype>
      <uniqueidentifier>160</uniqueidentifier>
    </link>
    <link>
      <SrcNic>
        <hostid>162</hostid>
        <nicid>165</nicid>
        <hostname>router0</hostname>
        <nicname>eth1</nicname>
      </SrcNic>
      <DstNic>
        <hostid>166</hostid>
        <nicid>168</nicid>
        <hostname>pc6</hostname>
        <nicname>eth0</nicname>
      </DstNic>
      <hostname />
      <linktype>normal</linktype>
      <uniqueidentifier>170</uniqueidentifier>
    </link>
    <link>
      <SrcNic>
        <hostid>148</hostid>
        <nicid>152</nicid>
        <hostname>firewall0</hostname>
        <nicname>wan0</nicname>
      </SrcNic>
      <DstNic>
        <hostid>162</hostid>
        <nicid>164</nicid>
        <hostname>router0</hostname>
        <nicname>eth0</nicname>
      </DstNic>
      <hostname />
      <linktype>normal</linktype>
      <uniqueidentifier>169</uniqueidentifier>
    </link>
    <link>
      <SrcNic>
        <hostid>171</hostid>
        <nicid>175</nicid>
        <hostname>wap0</hostname>
        <nicname>eth1</nicname>
      </SrcNic>
      <DstNic>
        <hostid>100</hostid>
        <nicid>107</nicid>
        <hostname>net_switch0</hostname>
        <nicname>port5</nicname>
      </DstNic>
      <hostname />
      <linktype>normal</linktype>
      <uniqueidentifier>194</uniqueidentifier>
    </link>
    <link>
      <SrcNic>
        <hostid>195</hostid>
        <nicid>198</nicid>
        <hostname>laptop0</hostname>
        <nicname>wlan2</nicname>
      </SrcNic>
      <DstNic>
        <hostid>171</hostid>
        <nicid>176</nicid>
        <hostname>wap0</hostname>
        <nicname>wport2</nicname>
      </DstNic>
      <hostname />
      <linktype>wireless</linktype>
      <uniqueidentifier>201</uniqueidentifier>
    </link>
    <nettest>
      <shost>laptop0</shost>
      <dhost>pc2</dhost>
      <thetest>NeedsLocalIPTo</thetest>
    </nettest>
    <nettest>
      <shost>net_switch0</shost>
      <dhost>All</dhost>
      <thetest>LockVLANsOnHost</thetest>
    </nettest>
    <nettest>
      <shost>net_switch1</shost>
      <dhost>All</dhost>
      <thetest>LockVLANsOnHost</thetest>
    </nettest>
    <nettest>
      <shost>net_switch2</shost>
      <dhost>All</dhost>
      <thetest>LockVLANsOnHost</thetest>
    </nettest>
    <tag>WirelessAP</tag>
    <tag>VLAN</tag>
    <VLANName
      ID="1"
      Color="Blue">Default</VLANName>
    <VLANName
      ID="2"
      Color="Green">Staff</VLANName>
    <VLANName
      ID="3"
      Color="Yellow">students</VLANName>
  </Network>
</EduNetworkBuilder>