<?xml version="1.0" encoding="utf-8"?>
<EduNetworkBuilder>
  <!--This is a network file for EduNetworkBuilder.-->
  <Network>
    <en_message>This shows what a VLAN does (Virtual LAN).  It allows you to separate networks; the devices on each VLAN cannot connect to ones on different VLANs unless they go through a router.</en_message>
    <en_title>What is a VLAN</en_title>
    <height>1024</height>
    <width>1024</width>
    <itemsize>100</itemsize>
    <showlabels>False</showlabels>
    <level>6</level>
    <sortorder>0</sortorder>
    <uniqueidentifier>173</uniqueidentifier>
    <startinghelplevel>full</startinghelplevel>
    <vlansenabled>True</vlansenabled>
    <device>
      <hostname>net_switch0</hostname>
      <size>100</size>
      <uniqueidentifier>104</uniqueidentifier>
      <location>40,410</location>
      <mytype>net_switch</mytype>
      <isdns>False</isdns>
      <isdhcp>False</isdhcp>
      <gateway>
        <ip>0.0.0.0</ip>
        <mask>0.0.0.0</mask>
        <gateway>0.0.0.0</gateway>
        <type>gw</type>
      </gateway>
      <nic>
        <nictype>lo</nictype>
        <nicname>lo0</nicname>
        <myid>
          <hostid>104</hostid>
          <nicid>105</nicid>
          <hostname>net_switch0</hostname>
          <nicname>lo0</nicname>
        </myid>
        <nictype>lo</nictype>
        <uniqueidentifier>105</uniqueidentifier>
        <usesdhcp>False</usesdhcp>
        <encryptionkey />
        <ssid />
        <interface>
          <nicname>lo0</nicname>
          <myip>
            <ip>127.0.0.1</ip>
            <mask>255.0.0.0</mask>
            <gateway>0.0.0.0</gateway>
            <type>ip</type>
          </myip>
          <VLAN
            ID="1">Untagged</VLAN>
        </interface>
      </nic>
      <nic>
        <nictype>management_interface</nictype>
        <nicname>management_interface0</nicname>
        <myid>
          <hostid>104</hostid>
          <nicid>106</nicid>
          <hostname>net_switch0</hostname>
          <nicname>management_interface0</nicname>
        </myid>
        <nictype>management_interface</nictype>
        <uniqueidentifier>106</uniqueidentifier>
        <usesdhcp>False</usesdhcp>
        <encryptionkey />
        <ssid />
        <interface>
          <nicname>management_interface0</nicname>
          <myip>
            <ip>0.0.0.0</ip>
            <mask>0.0.0.0</mask>
            <gateway>0.0.0.0</gateway>
            <type>ip</type>
          </myip>
          <VLAN
            ID="1">Untagged</VLAN>
        </interface>
      </nic>
      <nic>
        <nictype>port</nictype>
        <nicname>port1</nicname>
        <myid>
          <hostid>104</hostid>
          <nicid>107</nicid>
          <hostname>net_switch0</hostname>
          <nicname>port1</nicname>
        </myid>
        <nictype>port</nictype>
        <uniqueidentifier>107</uniqueidentifier>
        <usesdhcp>False</usesdhcp>
        <encryptionkey />
        <ssid />
        <interface>
          <nicname>port1</nicname>
          <myip>
            <ip>0.0.0.0</ip>
            <mask>0.0.0.0</mask>
            <gateway>0.0.0.0</gateway>
            <type>ip</type>
          </myip>
          <VLAN
            ID="1">Untagged</VLAN>
        </interface>
      </nic>
      <nic>
        <nictype>port</nictype>
        <nicname>port2</nicname>
        <myid>
          <hostid>104</hostid>
          <nicid>108</nicid>
          <hostname>net_switch0</hostname>
          <nicname>port2</nicname>
        </myid>
        <nictype>port</nictype>
        <uniqueidentifier>108</uniqueidentifier>
        <usesdhcp>False</usesdhcp>
        <encryptionkey />
        <ssid />
        <interface>
          <nicname>port2</nicname>
          <myip>
            <ip>0.0.0.0</ip>
            <mask>0.0.0.0</mask>
            <gateway>0.0.0.0</gateway>
            <type>ip</type>
          </myip>
          <VLAN
            ID="1">Untagged</VLAN>
        </interface>
      </nic>
      <nic>
        <nictype>port</nictype>
        <nicname>port3</nicname>
        <myid>
          <hostid>104</hostid>
          <nicid>109</nicid>
          <hostname>net_switch0</hostname>
          <nicname>port3</nicname>
        </myid>
        <nictype>port</nictype>
        <uniqueidentifier>109</uniqueidentifier>
        <usesdhcp>False</usesdhcp>
        <encryptionkey />
        <ssid />
        <interface>
          <nicname>port3</nicname>
          <myip>
            <ip>0.0.0.0</ip>
            <mask>0.0.0.0</mask>
            <gateway>0.0.0.0</gateway>
            <type>ip</type>
          </myip>
          <VLAN
            ID="1">Untagged</VLAN>
        </interface>
      </nic>
      <nic>
        <nictype>port</nictype>
        <nicname>port4</nicname>
        <myid>
          <hostid>104</hostid>
          <nicid>110</nicid>
          <hostname>net_switch0</hostname>
          <nicname>port4</nicname>
        </myid>
        <nictype>port</nictype>
        <uniqueidentifier>110</uniqueidentifier>
        <usesdhcp>False</usesdhcp>
        <encryptionkey />
        <ssid />
        <interface>
          <nicname>port4</nicname>
          <myip>
            <ip>0.0.0.0</ip>
            <mask>0.0.0.0</mask>
            <gateway>0.0.0.0</gateway>
            <type>ip</type>
          </myip>
          <VLAN
            ID="1">Untagged</VLAN>
        </interface>
      </nic>
      <nic>
        <nictype>port</nictype>
        <nicname>port5</nicname>
        <myid>
          <hostid>104</hostid>
          <nicid>111</nicid>
          <hostname>net_switch0</hostname>
          <nicname>port5</nicname>
        </myid>
        <nictype>port</nictype>
        <uniqueidentifier>111</uniqueidentifier>
        <usesdhcp>False</usesdhcp>
        <encryptionkey />
        <ssid />
        <interface>
          <nicname>port5</nicname>
          <myip>
            <ip>0.0.0.0</ip>
            <mask>0.0.0.0</mask>
            <gateway>0.0.0.0</gateway>
            <type>ip</type>
          </myip>
          <VLAN
            ID="1">Untagged</VLAN>
        </interface>
      </nic>
      <nic>
        <nictype>port</nictype>
        <nicname>port6</nicname>
        <myid>
          <hostid>104</hostid>
          <nicid>112</nicid>
          <hostname>net_switch0</hostname>
          <nicname>port6</nicname>
        </myid>
        <nictype>port</nictype>
        <uniqueidentifier>112</uniqueidentifier>
        <usesdhcp>False</usesdhcp>
        <encryptionkey />
        <ssid />
        <interface>
          <nicname>port6</nicname>
          <myip>
            <ip>0.0.0.0</ip>
            <mask>0.0.0.0</mask>
            <gateway>0.0.0.0</gateway>
            <type>ip</type>
          </myip>
          <VLAN
            ID="1">Untagged</VLAN>
        </interface>
      </nic>
      <nic>
        <nictype>port</nictype>
        <nicname>port7</nicname>
        <myid>
          <hostid>104</hostid>
          <nicid>113</nicid>
          <hostname>net_switch0</hostname>
          <nicname>port7</nicname>
        </myid>
        <nictype>port</nictype>
        <uniqueidentifier>113</uniqueidentifier>
        <usesdhcp>False</usesdhcp>
        <encryptionkey />
        <ssid />
        <interface>
          <nicname>port7</nicname>
          <myip>
            <ip>0.0.0.0</ip>
            <mask>0.0.0.0</mask>
            <gateway>0.0.0.0</gateway>
            <type>ip</type>
          </myip>
          <VLAN
            ID="1">Untagged</VLAN>
        </interface>
      </nic>
    </device>
    <device>
      <hostname>net_switch1</hostname>
      <size>100</size>
      <uniqueidentifier>114</uniqueidentifier>
      <location>240,410</location>
      <mytype>net_switch</mytype>
      <isdns>False</isdns>
      <isdhcp>False</isdhcp>
      <gateway>
        <ip>0.0.0.0</ip>
        <mask>0.0.0.0</mask>
        <gateway>0.0.0.0</gateway>
        <type>gw</type>
      </gateway>
      <nic>
        <nictype>lo</nictype>
        <nicname>lo0</nicname>
        <myid>
          <hostid>114</hostid>
          <nicid>115</nicid>
          <hostname>net_switch1</hostname>
          <nicname>lo0</nicname>
        </myid>
        <nictype>lo</nictype>
        <uniqueidentifier>115</uniqueidentifier>
        <usesdhcp>False</usesdhcp>
        <encryptionkey />
        <ssid />
        <interface>
          <nicname>lo0</nicname>
          <myip>
            <ip>127.0.0.1</ip>
            <mask>255.0.0.0</mask>
            <gateway>0.0.0.0</gateway>
            <type>ip</type>
          </myip>
          <VLAN
            ID="1">Untagged</VLAN>
        </interface>
      </nic>
      <nic>
        <nictype>management_interface</nictype>
        <nicname>management_interface0</nicname>
        <myid>
          <hostid>114</hostid>
          <nicid>116</nicid>
          <hostname>net_switch1</hostname>
          <nicname>management_interface0</nicname>
        </myid>
        <nictype>management_interface</nictype>
        <uniqueidentifier>116</uniqueidentifier>
        <usesdhcp>False</usesdhcp>
        <encryptionkey />
        <ssid />
        <interface>
          <nicname>management_interface0</nicname>
          <myip>
            <ip>0.0.0.0</ip>
            <mask>0.0.0.0</mask>
            <gateway>0.0.0.0</gateway>
            <type>ip</type>
          </myip>
          <VLAN
            ID="1">Untagged</VLAN>
        </interface>
      </nic>
      <nic>
        <nictype>port</nictype>
        <nicname>port1</nicname>
        <myid>
          <hostid>114</hostid>
          <nicid>117</nicid>
          <hostname>net_switch1</hostname>
          <nicname>port1</nicname>
        </myid>
        <nictype>port</nictype>
        <uniqueidentifier>117</uniqueidentifier>
        <usesdhcp>False</usesdhcp>
        <encryptionkey />
        <ssid />
        <interface>
          <nicname>port1</nicname>
          <myip>
            <ip>0.0.0.0</ip>
            <mask>0.0.0.0</mask>
            <gateway>0.0.0.0</gateway>
            <type>ip</type>
          </myip>
          <VLAN
            ID="1">Untagged</VLAN>
        </interface>
      </nic>
      <nic>
        <nictype>port</nictype>
        <nicname>port2</nicname>
        <myid>
          <hostid>114</hostid>
          <nicid>118</nicid>
          <hostname>net_switch1</hostname>
          <nicname>port2</nicname>
        </myid>
        <nictype>port</nictype>
        <uniqueidentifier>118</uniqueidentifier>
        <usesdhcp>False</usesdhcp>
        <encryptionkey />
        <ssid />
        <interface>
          <nicname>port2</nicname>
          <myip>
            <ip>0.0.0.0</ip>
            <mask>0.0.0.0</mask>
            <gateway>0.0.0.0</gateway>
            <type>ip</type>
          </myip>
          <VLAN
            ID="1">Untagged</VLAN>
        </interface>
      </nic>
      <nic>
        <nictype>port</nictype>
        <nicname>port3</nicname>
        <myid>
          <hostid>114</hostid>
          <nicid>119</nicid>
          <hostname>net_switch1</hostname>
          <nicname>port3</nicname>
        </myid>
        <nictype>port</nictype>
        <uniqueidentifier>119</uniqueidentifier>
        <usesdhcp>False</usesdhcp>
        <encryptionkey />
        <ssid />
        <interface>
          <nicname>port3</nicname>
          <myip>
            <ip>0.0.0.0</ip>
            <mask>0.0.0.0</mask>
            <gateway>0.0.0.0</gateway>
            <type>ip</type>
          </myip>
          <VLAN
            ID="1">Untagged</VLAN>
        </interface>
      </nic>
      <nic>
        <nictype>port</nictype>
        <nicname>port4</nicname>
        <myid>
          <hostid>114</hostid>
          <nicid>120</nicid>
          <hostname>net_switch1</hostname>
          <nicname>port4</nicname>
        </myid>
        <nictype>port</nictype>
        <uniqueidentifier>120</uniqueidentifier>
        <usesdhcp>False</usesdhcp>
        <encryptionkey />
        <ssid />
        <interface>
          <nicname>port4</nicname>
          <myip>
            <ip>0.0.0.0</ip>
            <mask>0.0.0.0</mask>
            <gateway>0.0.0.0</gateway>
            <type>ip</type>
          </myip>
          <VLAN
            ID="1">Untagged</VLAN>
        </interface>
      </nic>
      <nic>
        <nictype>port</nictype>
        <nicname>port5</nicname>
        <myid>
          <hostid>114</hostid>
          <nicid>121</nicid>
          <hostname>net_switch1</hostname>
          <nicname>port5</nicname>
        </myid>
        <nictype>port</nictype>
        <uniqueidentifier>121</uniqueidentifier>
        <usesdhcp>False</usesdhcp>
        <encryptionkey />
        <ssid />
        <interface>
          <nicname>port5</nicname>
          <myip>
            <ip>0.0.0.0</ip>
            <mask>0.0.0.0</mask>
            <gateway>0.0.0.0</gateway>
            <type>ip</type>
          </myip>
          <VLAN
            ID="1">Untagged</VLAN>
        </interface>
      </nic>
      <nic>
        <nictype>port</nictype>
        <nicname>port6</nicname>
        <myid>
          <hostid>114</hostid>
          <nicid>122</nicid>
          <hostname>net_switch1</hostname>
          <nicname>port6</nicname>
        </myid>
        <nictype>port</nictype>
        <uniqueidentifier>122</uniqueidentifier>
        <usesdhcp>False</usesdhcp>
        <encryptionkey />
        <ssid />
        <interface>
          <nicname>port6</nicname>
          <myip>
            <ip>0.0.0.0</ip>
            <mask>0.0.0.0</mask>
            <gateway>0.0.0.0</gateway>
            <type>ip</type>
          </myip>
          <VLAN
            ID="1">Untagged</VLAN>
        </interface>
      </nic>
      <nic>
        <nictype>port</nictype>
        <nicname>port7</nicname>
        <myid>
          <hostid>114</hostid>
          <nicid>123</nicid>
          <hostname>net_switch1</hostname>
          <nicname>port7</nicname>
        </myid>
        <nictype>port</nictype>
        <uniqueidentifier>123</uniqueidentifier>
        <usesdhcp>False</usesdhcp>
        <encryptionkey />
        <ssid />
        <interface>
          <nicname>port7</nicname>
          <myip>
            <ip>0.0.0.0</ip>
            <mask>0.0.0.0</mask>
            <gateway>0.0.0.0</gateway>
            <type>ip</type>
          </myip>
          <VLAN
            ID="1">Untagged</VLAN>
        </interface>
      </nic>
    </device>
    <device>
      <hostname>net_switch2</hostname>
      <size>100</size>
      <uniqueidentifier>134</uniqueidentifier>
      <location>700,410</location>
      <mytype>net_switch</mytype>
      <isdns>False</isdns>
      <isdhcp>False</isdhcp>
      <gateway>
        <ip>0.0.0.0</ip>
        <mask>0.0.0.0</mask>
        <gateway>0.0.0.0</gateway>
        <type>gw</type>
      </gateway>
      <nic>
        <nictype>lo</nictype>
        <nicname>lo0</nicname>
        <myid>
          <hostid>134</hostid>
          <nicid>135</nicid>
          <hostname>net_switch2</hostname>
          <nicname>lo0</nicname>
        </myid>
        <nictype>lo</nictype>
        <uniqueidentifier>135</uniqueidentifier>
        <usesdhcp>False</usesdhcp>
        <encryptionkey />
        <ssid />
        <interface>
          <nicname>lo0</nicname>
          <myip>
            <ip>127.0.0.1</ip>
            <mask>255.0.0.0</mask>
            <gateway>0.0.0.0</gateway>
            <type>ip</type>
          </myip>
          <VLAN
            ID="1">Untagged</VLAN>
        </interface>
      </nic>
      <nic>
        <nictype>management_interface</nictype>
        <nicname>management_interface0</nicname>
        <myid>
          <hostid>134</hostid>
          <nicid>136</nicid>
          <hostname>net_switch2</hostname>
          <nicname>management_interface0</nicname>
        </myid>
        <nictype>management_interface</nictype>
        <uniqueidentifier>136</uniqueidentifier>
        <usesdhcp>False</usesdhcp>
        <encryptionkey />
        <ssid />
        <interface>
          <nicname>management_interface0</nicname>
          <myip>
            <ip>0.0.0.0</ip>
            <mask>0.0.0.0</mask>
            <gateway>0.0.0.0</gateway>
            <type>ip</type>
          </myip>
          <VLAN
            ID="1">Untagged</VLAN>
        </interface>
      </nic>
      <nic>
        <nictype>port</nictype>
        <nicname>port1</nicname>
        <myid>
          <hostid>134</hostid>
          <nicid>137</nicid>
          <hostname>net_switch2</hostname>
          <nicname>port1</nicname>
        </myid>
        <nictype>port</nictype>
        <uniqueidentifier>137</uniqueidentifier>
        <usesdhcp>False</usesdhcp>
        <encryptionkey />
        <ssid />
        <interface>
          <nicname>port1</nicname>
          <myip>
            <ip>0.0.0.0</ip>
            <mask>0.0.0.0</mask>
            <gateway>0.0.0.0</gateway>
            <type>ip</type>
          </myip>
          <VLAN
            ID="1">Tagged</VLAN>
          <VLAN
            ID="2">Tagged</VLAN>
          <VLAN
            ID="3">Tagged</VLAN>
        </interface>
      </nic>
      <nic>
        <nictype>port</nictype>
        <nicname>port2</nicname>
        <myid>
          <hostid>134</hostid>
          <nicid>138</nicid>
          <hostname>net_switch2</hostname>
          <nicname>port2</nicname>
        </myid>
        <nictype>port</nictype>
        <uniqueidentifier>138</uniqueidentifier>
        <usesdhcp>False</usesdhcp>
        <encryptionkey />
        <ssid />
        <interface>
          <nicname>port2</nicname>
          <myip>
            <ip>0.0.0.0</ip>
            <mask>0.0.0.0</mask>
            <gateway>0.0.0.0</gateway>
            <type>ip</type>
          </myip>
          <VLAN
            ID="1">Forbidden</VLAN>
          <VLAN
            ID="2">Untagged</VLAN>
          <VLAN
            ID="3">Forbidden</VLAN>
        </interface>
      </nic>
      <nic>
        <nictype>port</nictype>
        <nicname>port3</nicname>
        <myid>
          <hostid>134</hostid>
          <nicid>139</nicid>
          <hostname>net_switch2</hostname>
          <nicname>port3</nicname>
        </myid>
        <nictype>port</nictype>
        <uniqueidentifier>139</uniqueidentifier>
        <usesdhcp>False</usesdhcp>
        <encryptionkey />
        <ssid />
        <interface>
          <nicname>port3</nicname>
          <myip>
            <ip>0.0.0.0</ip>
            <mask>0.0.0.0</mask>
            <gateway>0.0.0.0</gateway>
            <type>ip</type>
          </myip>
          <VLAN
            ID="1">Forbidden</VLAN>
          <VLAN
            ID="3">Untagged</VLAN>
          <VLAN
            ID="2">Forbidden</VLAN>
        </interface>
      </nic>
      <nic>
        <nictype>port</nictype>
        <nicname>port4</nicname>
        <myid>
          <hostid>134</hostid>
          <nicid>140</nicid>
          <hostname>net_switch2</hostname>
          <nicname>port4</nicname>
        </myid>
        <nictype>port</nictype>
        <uniqueidentifier>140</uniqueidentifier>
        <usesdhcp>False</usesdhcp>
        <encryptionkey />
        <ssid />
        <interface>
          <nicname>port4</nicname>
          <myip>
            <ip>0.0.0.0</ip>
            <mask>0.0.0.0</mask>
            <gateway>0.0.0.0</gateway>
            <type>ip</type>
          </myip>
          <VLAN
            ID="1">Untagged</VLAN>
          <VLAN
            ID="3">Forbidden</VLAN>
          <VLAN
            ID="2">Forbidden</VLAN>
        </interface>
      </nic>
      <nic>
        <nictype>port</nictype>
        <nicname>port5</nicname>
        <myid>
          <hostid>134</hostid>
          <nicid>141</nicid>
          <hostname>net_switch2</hostname>
          <nicname>port5</nicname>
        </myid>
        <nictype>port</nictype>
        <uniqueidentifier>141</uniqueidentifier>
        <usesdhcp>False</usesdhcp>
        <encryptionkey />
        <ssid />
        <interface>
          <nicname>port5</nicname>
          <myip>
            <ip>0.0.0.0</ip>
            <mask>0.0.0.0</mask>
            <gateway>0.0.0.0</gateway>
            <type>ip</type>
          </myip>
          <VLAN
            ID="1">Untagged</VLAN>
          <VLAN
            ID="3">Forbidden</VLAN>
          <VLAN
            ID="2">Forbidden</VLAN>
        </interface>
      </nic>
      <nic>
        <nictype>port</nictype>
        <nicname>port6</nicname>
        <myid>
          <hostid>134</hostid>
          <nicid>142</nicid>
          <hostname>net_switch2</hostname>
          <nicname>port6</nicname>
        </myid>
        <nictype>port</nictype>
        <uniqueidentifier>142</uniqueidentifier>
        <usesdhcp>False</usesdhcp>
        <encryptionkey />
        <ssid />
        <interface>
          <nicname>port6</nicname>
          <myip>
            <ip>0.0.0.0</ip>
            <mask>0.0.0.0</mask>
            <gateway>0.0.0.0</gateway>
            <type>ip</type>
          </myip>
          <VLAN
            ID="1">Untagged</VLAN>
          <VLAN
            ID="3">Forbidden</VLAN>
          <VLAN
            ID="2">Forbidden</VLAN>
        </interface>
      </nic>
      <nic>
        <nictype>port</nictype>
        <nicname>port7</nicname>
        <myid>
          <hostid>134</hostid>
          <nicid>143</nicid>
          <hostname>net_switch2</hostname>
          <nicname>port7</nicname>
        </myid>
        <nictype>port</nictype>
        <uniqueidentifier>143</uniqueidentifier>
        <usesdhcp>False</usesdhcp>
        <encryptionkey />
        <ssid />
        <interface>
          <nicname>port7</nicname>
          <myip>
            <ip>0.0.0.0</ip>
            <mask>0.0.0.0</mask>
            <gateway>0.0.0.0</gateway>
            <type>ip</type>
          </myip>
          <VLAN
            ID="1">Untagged</VLAN>
          <VLAN
            ID="3">Forbidden</VLAN>
          <VLAN
            ID="2">Forbidden</VLAN>
        </interface>
      </nic>
    </device>
    <device>
      <hostname>pc0</hostname>
      <size>100</size>
      <uniqueidentifier>157</uniqueidentifier>
      <location>30,580</location>
      <mytype>pc</mytype>
      <isdns>False</isdns>
      <isdhcp>False</isdhcp>
      <morphcolor>Yellow</morphcolor>
      <gateway>
        <ip>192.168.1.1</ip>
        <mask>0.0.0.0</mask>
        <gateway>0.0.0.0</gateway>
        <type>gw</type>
      </gateway>
      <nic>
        <nictype>lo</nictype>
        <nicname>lo0</nicname>
        <myid>
          <hostid>157</hostid>
          <nicid>158</nicid>
          <hostname>pc0</hostname>
          <nicname>lo0</nicname>
        </myid>
        <nictype>lo</nictype>
        <uniqueidentifier>158</uniqueidentifier>
        <usesdhcp>False</usesdhcp>
        <interface>
          <nicname>lo0</nicname>
          <myip>
            <ip>127.0.0.1</ip>
            <mask>255.0.0.0</mask>
            <gateway>0.0.0.0</gateway>
            <type>ip</type>
          </myip>
          <VLAN
            ID="1">Untagged</VLAN>
        </interface>
      </nic>
      <nic>
        <nictype>eth</nictype>
        <nicname>eth0</nicname>
        <myid>
          <hostid>157</hostid>
          <nicid>159</nicid>
          <hostname>pc0</hostname>
          <nicname>eth0</nicname>
        </myid>
        <nictype>eth</nictype>
        <uniqueidentifier>159</uniqueidentifier>
        <usesdhcp>False</usesdhcp>
        <interface>
          <nicname>eth0</nicname>
          <myip>
            <ip>192.168.1.2</ip>
            <mask>255.255.255.0</mask>
            <gateway>0.0.0.0</gateway>
            <type>ip</type>
          </myip>
          <VLAN
            ID="1">Untagged</VLAN>
        </interface>
      </nic>
    </device>
    <device>
      <hostname>pc1</hostname>
      <size>100</size>
      <uniqueidentifier>160</uniqueidentifier>
      <location>240,570</location>
      <mytype>pc</mytype>
      <isdns>False</isdns>
      <isdhcp>False</isdhcp>
      <morphcolor>Green</morphcolor>
      <gateway>
        <ip>192.168.2.1</ip>
        <mask>0.0.0.0</mask>
        <gateway>0.0.0.0</gateway>
        <type>gw</type>
      </gateway>
      <nic>
        <nictype>lo</nictype>
        <nicname>lo0</nicname>
        <myid>
          <hostid>160</hostid>
          <nicid>161</nicid>
          <hostname>pc1</hostname>
          <nicname>lo0</nicname>
        </myid>
        <nictype>lo</nictype>
        <uniqueidentifier>161</uniqueidentifier>
        <usesdhcp>False</usesdhcp>
        <interface>
          <nicname>lo0</nicname>
          <myip>
            <ip>127.0.0.1</ip>
            <mask>255.0.0.0</mask>
            <gateway>0.0.0.0</gateway>
            <type>ip</type>
          </myip>
          <VLAN
            ID="1">Untagged</VLAN>
        </interface>
      </nic>
      <nic>
        <nictype>eth</nictype>
        <nicname>eth0</nicname>
        <myid>
          <hostid>160</hostid>
          <nicid>162</nicid>
          <hostname>pc1</hostname>
          <nicname>eth0</nicname>
        </myid>
        <nictype>eth</nictype>
        <uniqueidentifier>162</uniqueidentifier>
        <usesdhcp>False</usesdhcp>
        <interface>
          <nicname>eth0</nicname>
          <myip>
            <ip>192.168.2.2</ip>
            <mask>255.255.255.0</mask>
            <gateway>0.0.0.0</gateway>
            <type>ip</type>
          </myip>
          <VLAN
            ID="1">Untagged</VLAN>
        </interface>
      </nic>
    </device>
    <device>
      <hostname>pc2</hostname>
      <size>100</size>
      <uniqueidentifier>163</uniqueidentifier>
      <location>590,590</location>
      <mytype>pc</mytype>
      <isdns>False</isdns>
      <isdhcp>False</isdhcp>
      <morphcolor>Yellow</morphcolor>
      <gateway>
        <ip>192.168.3.1</ip>
        <mask>0.0.0.0</mask>
        <gateway>0.0.0.0</gateway>
        <type>gw</type>
      </gateway>
      <nic>
        <nictype>lo</nictype>
        <nicname>lo0</nicname>
        <myid>
          <hostid>163</hostid>
          <nicid>164</nicid>
          <hostname>pc2</hostname>
          <nicname>lo0</nicname>
        </myid>
        <nictype>lo</nictype>
        <uniqueidentifier>164</uniqueidentifier>
        <usesdhcp>False</usesdhcp>
        <interface>
          <nicname>lo0</nicname>
          <myip>
            <ip>127.0.0.1</ip>
            <mask>255.0.0.0</mask>
            <gateway>0.0.0.0</gateway>
            <type>ip</type>
          </myip>
          <VLAN
            ID="1">Untagged</VLAN>
        </interface>
      </nic>
      <nic>
        <nictype>eth</nictype>
        <nicname>eth0</nicname>
        <myid>
          <hostid>163</hostid>
          <nicid>165</nicid>
          <hostname>pc2</hostname>
          <nicname>eth0</nicname>
        </myid>
        <nictype>eth</nictype>
        <uniqueidentifier>165</uniqueidentifier>
        <usesdhcp>False</usesdhcp>
        <interface>
          <nicname>eth0</nicname>
          <myip>
            <ip>192.168.3.2</ip>
            <mask>255.255.255.0</mask>
            <gateway>0.0.0.0</gateway>
            <type>ip</type>
          </myip>
          <VLAN
            ID="1">Untagged</VLAN>
        </interface>
      </nic>
    </device>
    <device>
      <hostname>pc3</hostname>
      <size>100</size>
      <uniqueidentifier>166</uniqueidentifier>
      <location>800,590</location>
      <mytype>pc</mytype>
      <isdns>False</isdns>
      <isdhcp>False</isdhcp>
      <morphcolor>Green</morphcolor>
      <gateway>
        <ip>192.168.4.1</ip>
        <mask>0.0.0.0</mask>
        <gateway>0.0.0.0</gateway>
        <type>gw</type>
      </gateway>
      <nic>
        <nictype>lo</nictype>
        <nicname>lo0</nicname>
        <myid>
          <hostid>166</hostid>
          <nicid>167</nicid>
          <hostname>pc3</hostname>
          <nicname>lo0</nicname>
        </myid>
        <nictype>lo</nictype>
        <uniqueidentifier>167</uniqueidentifier>
        <usesdhcp>False</usesdhcp>
        <interface>
          <nicname>lo0</nicname>
          <myip>
            <ip>127.0.0.1</ip>
            <mask>255.0.0.0</mask>
            <gateway>0.0.0.0</gateway>
            <type>ip</type>
          </myip>
          <VLAN
            ID="1">Untagged</VLAN>
        </interface>
      </nic>
      <nic>
        <nictype>eth</nictype>
        <nicname>eth0</nicname>
        <myid>
          <hostid>166</hostid>
          <nicid>168</nicid>
          <hostname>pc3</hostname>
          <nicname>eth0</nicname>
        </myid>
        <nictype>eth</nictype>
        <uniqueidentifier>168</uniqueidentifier>
        <usesdhcp>False</usesdhcp>
        <interface>
          <nicname>eth0</nicname>
          <myip>
            <ip>192.168.4.2</ip>
            <mask>255.255.255.0</mask>
            <gateway>0.0.0.0</gateway>
            <type>ip</type>
          </myip>
          <VLAN
            ID="1">Untagged</VLAN>
        </interface>
      </nic>
    </device>
    <device>
      <hostname>router0</hostname>
      <size>100</size>
      <uniqueidentifier>100</uniqueidentifier>
      <location>700,190</location>
      <mytype>router</mytype>
      <isdns>False</isdns>
      <isdhcp>False</isdhcp>
      <gateway>
        <ip>0.0.0.0</ip>
        <mask>0.0.0.0</mask>
        <gateway>0.0.0.0</gateway>
        <type>gw</type>
      </gateway>
      <nic>
        <nictype>lo</nictype>
        <nicname>lo0</nicname>
        <myid>
          <hostid>100</hostid>
          <nicid>101</nicid>
          <hostname>router0</hostname>
          <nicname>lo0</nicname>
        </myid>
        <nictype>lo</nictype>
        <uniqueidentifier>101</uniqueidentifier>
        <usesdhcp>False</usesdhcp>
        <encryptionkey />
        <ssid />
        <interface>
          <nicname>lo0</nicname>
          <myip>
            <ip>127.0.0.1</ip>
            <mask>255.0.0.0</mask>
            <gateway>0.0.0.0</gateway>
            <type>ip</type>
          </myip>
          <VLAN
            ID="1">Untagged</VLAN>
        </interface>
      </nic>
      <nic>
        <nictype>eth</nictype>
        <nicname>eth0</nicname>
        <myid>
          <hostid>100</hostid>
          <nicid>102</nicid>
          <hostname>router0</hostname>
          <nicname>eth0</nicname>
        </myid>
        <nictype>eth</nictype>
        <uniqueidentifier>102</uniqueidentifier>
        <usesdhcp>False</usesdhcp>
        <encryptionkey />
        <ssid />
        <interface>
          <nicname>eth0</nicname>
          <myip>
            <ip>192.168.3.1</ip>
            <mask>255.255.255.0</mask>
            <gateway>0.0.0.0</gateway>
            <type>ip</type>
          </myip>
          <VLAN
            ID="1">Forbidden</VLAN>
          <VLAN
            ID="2">Tagged</VLAN>
          <VLAN
            ID="3">Forbidden</VLAN>
        </interface>
        <interface>
          <nicname>eth0:1</nicname>
          <myip>
            <ip>192.168.4.1</ip>
            <mask>255.255.255.0</mask>
            <gateway>0.0.0.0</gateway>
            <type>ip</type>
          </myip>
          <VLAN
            ID="1">Forbidden</VLAN>
          <VLAN
            ID="3">Tagged</VLAN>
          <VLAN
            ID="2">Forbidden</VLAN>
        </interface>
      </nic>
      <nic>
        <nictype>eth</nictype>
        <nicname>eth1</nicname>
        <myid>
          <hostid>100</hostid>
          <nicid>103</nicid>
          <hostname>router0</hostname>
          <nicname>eth1</nicname>
        </myid>
        <nictype>eth</nictype>
        <uniqueidentifier>103</uniqueidentifier>
        <usesdhcp>False</usesdhcp>
        <encryptionkey />
        <ssid />
        <interface>
          <nicname>eth1</nicname>
          <myip>
            <ip>0.0.0.0</ip>
            <mask>0.0.0.0</mask>
            <gateway>0.0.0.0</gateway>
            <type>ip</type>
          </myip>
          <VLAN
            ID="1">Untagged</VLAN>
        </interface>
      </nic>
    </device>
    <device>
      <hostname>router1</hostname>
      <size>100</size>
      <uniqueidentifier>130</uniqueidentifier>
      <location>130,190</location>
      <mytype>router</mytype>
      <isdns>False</isdns>
      <isdhcp>False</isdhcp>
      <gateway>
        <ip>0.0.0.0</ip>
        <mask>0.0.0.0</mask>
        <gateway>0.0.0.0</gateway>
        <type>gw</type>
      </gateway>
      <nic>
        <nictype>lo</nictype>
        <nicname>lo0</nicname>
        <myid>
          <hostid>130</hostid>
          <nicid>131</nicid>
          <hostname>router1</hostname>
          <nicname>lo0</nicname>
        </myid>
        <nictype>lo</nictype>
        <uniqueidentifier>131</uniqueidentifier>
        <usesdhcp>False</usesdhcp>
        <encryptionkey />
        <ssid />
        <interface>
          <nicname>lo0</nicname>
          <myip>
            <ip>127.0.0.1</ip>
            <mask>255.0.0.0</mask>
            <gateway>0.0.0.0</gateway>
            <type>ip</type>
          </myip>
          <VLAN
            ID="1">Untagged</VLAN>
        </interface>
      </nic>
      <nic>
        <nictype>eth</nictype>
        <nicname>eth0</nicname>
        <myid>
          <hostid>130</hostid>
          <nicid>132</nicid>
          <hostname>router1</hostname>
          <nicname>eth0</nicname>
        </myid>
        <nictype>eth</nictype>
        <uniqueidentifier>132</uniqueidentifier>
        <usesdhcp>False</usesdhcp>
        <encryptionkey />
        <ssid />
        <interface>
          <nicname>eth0</nicname>
          <myip>
            <ip>192.168.1.1</ip>
            <mask>255.255.255.0</mask>
            <gateway>0.0.0.0</gateway>
            <type>ip</type>
          </myip>
          <VLAN
            ID="1">Untagged</VLAN>
        </interface>
      </nic>
      <nic>
        <nictype>eth</nictype>
        <nicname>eth1</nicname>
        <myid>
          <hostid>130</hostid>
          <nicid>133</nicid>
          <hostname>router1</hostname>
          <nicname>eth1</nicname>
        </myid>
        <nictype>eth</nictype>
        <uniqueidentifier>133</uniqueidentifier>
        <usesdhcp>False</usesdhcp>
        <encryptionkey />
        <ssid />
        <interface>
          <nicname>eth1</nicname>
          <myip>
            <ip>192.168.2.1</ip>
            <mask>255.255.255.0</mask>
            <gateway>0.0.0.0</gateway>
            <type>ip</type>
          </myip>
          <VLAN
            ID="1">Untagged</VLAN>
        </interface>
      </nic>
    </device>
    <link>
      <SrcNic>
        <hostid>104</hostid>
        <nicid>107</nicid>
        <hostname>net_switch0</hostname>
        <nicname>port1</nicname>
      </SrcNic>
      <DstNic>
        <hostid>130</hostid>
        <nicid>132</nicid>
        <hostname>router1</hostname>
        <nicname>eth0</nicname>
      </DstNic>
      <hostname />
      <linktype>normal</linktype>
      <uniqueidentifier>151</uniqueidentifier>
    </link>
    <link>
      <SrcNic>
        <hostid>130</hostid>
        <nicid>133</nicid>
        <hostname>router1</hostname>
        <nicname>eth1</nicname>
      </SrcNic>
      <DstNic>
        <hostid>114</hostid>
        <nicid>117</nicid>
        <hostname>net_switch1</hostname>
        <nicname>port1</nicname>
      </DstNic>
      <hostname />
      <linktype>normal</linktype>
      <uniqueidentifier>152</uniqueidentifier>
    </link>
    <link>
      <SrcNic>
        <hostid>134</hostid>
        <nicid>137</nicid>
        <hostname>net_switch2</hostname>
        <nicname>port1</nicname>
      </SrcNic>
      <DstNic>
        <hostid>100</hostid>
        <nicid>102</nicid>
        <hostname>router0</hostname>
        <nicname>eth0</nicname>
      </DstNic>
      <hostname />
      <linktype>normal</linktype>
      <uniqueidentifier>156</uniqueidentifier>
    </link>
    <link>
      <SrcNic>
        <hostid>157</hostid>
        <nicid>159</nicid>
        <hostname>pc0</hostname>
        <nicname>eth0</nicname>
      </SrcNic>
      <DstNic>
        <hostid>104</hostid>
        <nicid>108</nicid>
        <hostname>net_switch0</hostname>
        <nicname>port2</nicname>
      </DstNic>
      <hostname />
      <linktype>normal</linktype>
      <uniqueidentifier>169</uniqueidentifier>
    </link>
    <link>
      <SrcNic>
        <hostid>160</hostid>
        <nicid>162</nicid>
        <hostname>pc1</hostname>
        <nicname>eth0</nicname>
      </SrcNic>
      <DstNic>
        <hostid>114</hostid>
        <nicid>118</nicid>
        <hostname>net_switch1</hostname>
        <nicname>port2</nicname>
      </DstNic>
      <hostname />
      <linktype>normal</linktype>
      <uniqueidentifier>170</uniqueidentifier>
    </link>
    <link>
      <SrcNic>
        <hostid>163</hostid>
        <nicid>165</nicid>
        <hostname>pc2</hostname>
        <nicname>eth0</nicname>
      </SrcNic>
      <DstNic>
        <hostid>134</hostid>
        <nicid>138</nicid>
        <hostname>net_switch2</hostname>
        <nicname>port2</nicname>
      </DstNic>
      <hostname />
      <linktype>normal</linktype>
      <uniqueidentifier>171</uniqueidentifier>
    </link>
    <link>
      <SrcNic>
        <hostid>166</hostid>
        <nicid>168</nicid>
        <hostname>pc3</hostname>
        <nicname>eth0</nicname>
      </SrcNic>
      <DstNic>
        <hostid>134</hostid>
        <nicid>139</nicid>
        <hostname>net_switch2</hostname>
        <nicname>port3</nicname>
      </DstNic>
      <hostname />
      <linktype>normal</linktype>
      <uniqueidentifier>172</uniqueidentifier>
    </link>
    <nettest>
      <shost>pc0</shost>
      <dhost>pc1</dhost>
      <thetest>SuccessfullyPings</thetest>
    </nettest>
    <nettest>
      <shost>pc2</shost>
      <dhost>pc3</dhost>
      <thetest>SuccessfullyPings</thetest>
    </nettest>
    <tag>VLAN</tag>
    <VLANName
      ID="1">Default</VLANName>
    <VLANName
      ID="2">Staff</VLANName>
    <VLANName
      ID="3">Students</VLANName>
  </Network>
</EduNetworkBuilder>