<?xml version="1.0" encoding="utf-8"?>
<EduNetworkBuilder>
  <!--This is a network file for EduNetworkBuilder.-->
  <Network>
    <en_message />
    <en_title>Practice4</en_title>
    <en_url />
    <height>1024</height>
    <width>1024</width>
    <itemsize>60</itemsize>
    <showlabels>host</showlabels>
    <level>1</level>
    <sortorder>24</sortorder>
    <uniqueidentifier>502</uniqueidentifier>
    <startinghelplevel>none</startinghelplevel>
    <vlansenabled>True</vlansenabled>
    <VLANPacketColors>False</VLANPacketColors>
    <device>
      <hostname>firewall0</hostname>
      <size>60</size>
      <uniqueidentifier>175</uniqueidentifier>
      <location>670,200</location>
      <mytype>firewall</mytype>
      <isdns>False</isdns>
      <isdhcp>False</isdhcp>
      <gateway>
        <ip>192.168.5.1</ip>
        <mask>0.0.0.0</mask>
        <gateway>0.0.0.0</gateway>
        <type>gw</type>
      </gateway>
      <nic>
        <nictype>lo</nictype>
        <nicname>lo0</nicname>
        <myid>
          <hostid>175</hostid>
          <nicid>176</nicid>
          <hostname>firewall0</hostname>
          <nicname>lo0</nicname>
        </myid>
        <nictype>lo</nictype>
        <uniqueidentifier>176</uniqueidentifier>
        <usesdhcp>False</usesdhcp>
        <encryptionkey />
        <ssid />
        <interface>
          <nicname>lo0</nicname>
          <myip>
            <ip>127.0.0.1</ip>
            <mask>255.0.0.0</mask>
            <gateway>0.0.0.0</gateway>
            <type>ip</type>
          </myip>
          <VLAN
            ID="1">Untagged</VLAN>
        </interface>
      </nic>
      <nic>
        <nictype>wan</nictype>
        <nicname>wan0</nicname>
        <myid>
          <hostid>175</hostid>
          <nicid>179</nicid>
          <hostname>firewall0</hostname>
          <nicname>wan0</nicname>
        </myid>
        <nictype>wan</nictype>
        <uniqueidentifier>179</uniqueidentifier>
        <usesdhcp>False</usesdhcp>
        <encryptionkey />
        <ssid />
        <interface>
          <nicname>wan0</nicname>
          <myip>
            <ip>192.168.5.2</ip>
            <mask>255.255.255.0</mask>
            <gateway>0.0.0.0</gateway>
            <type>ip</type>
          </myip>
          <VLAN
            ID="1">Untagged</VLAN>
        </interface>
      </nic>
      <nic>
        <nictype>eth</nictype>
        <nicname>eth0</nicname>
        <myid>
          <hostid>175</hostid>
          <nicid>177</nicid>
          <hostname>firewall0</hostname>
          <nicname>eth0</nicname>
        </myid>
        <nictype>eth</nictype>
        <uniqueidentifier>177</uniqueidentifier>
        <usesdhcp>False</usesdhcp>
        <encryptionkey />
        <ssid />
        <interface>
          <nicname>eth0</nicname>
          <myip>
            <ip>192.168.1.1</ip>
            <mask>255.255.255.0</mask>
            <gateway>0.0.0.0</gateway>
            <type>ip</type>
          </myip>
          <VLAN
            ID="1">Untagged</VLAN>
        </interface>
      </nic>
      <nic>
        <nictype>eth</nictype>
        <nicname>eth1</nicname>
        <myid>
          <hostid>175</hostid>
          <nicid>178</nicid>
          <hostname>firewall0</hostname>
          <nicname>eth1</nicname>
        </myid>
        <nictype>eth</nictype>
        <uniqueidentifier>178</uniqueidentifier>
        <usesdhcp>False</usesdhcp>
        <encryptionkey />
        <ssid />
        <interface>
          <nicname>eth1</nicname>
          <myip>
            <ip>0.0.0.0</ip>
            <mask>0.0.0.0</mask>
            <gateway>0.0.0.0</gateway>
            <type>ip</type>
          </myip>
          <VLAN
            ID="1">Untagged</VLAN>
        </interface>
      </nic>
    </device>
    <device>
      <hostname>google.com</hostname>
      <size>60</size>
      <uniqueidentifier>190</uniqueidentifier>
      <location>330,50</location>
      <mytype>server</mytype>
      <isdns>False</isdns>
      <isdhcp>False</isdhcp>
      <gateway>
        <ip>8.8.8.1</ip>
        <mask>0.0.0.0</mask>
        <gateway>0.0.0.0</gateway>
        <type>gw</type>
      </gateway>
      <nic>
        <nictype>lo</nictype>
        <nicname>lo0</nicname>
        <myid>
          <hostid>190</hostid>
          <nicid>191</nicid>
          <hostname>server0</hostname>
          <nicname>lo0</nicname>
        </myid>
        <nictype>lo</nictype>
        <uniqueidentifier>191</uniqueidentifier>
        <usesdhcp>False</usesdhcp>
        <encryptionkey />
        <ssid />
        <interface>
          <nicname>lo0</nicname>
          <myip>
            <ip>127.0.0.1</ip>
            <mask>255.0.0.0</mask>
            <gateway>0.0.0.0</gateway>
            <type>ip</type>
          </myip>
          <VLAN
            ID="1">Untagged</VLAN>
        </interface>
      </nic>
      <nic>
        <nictype>eth</nictype>
        <nicname>eth0</nicname>
        <myid>
          <hostid>190</hostid>
          <nicid>192</nicid>
          <hostname>server0</hostname>
          <nicname>eth0</nicname>
        </myid>
        <nictype>eth</nictype>
        <uniqueidentifier>192</uniqueidentifier>
        <usesdhcp>False</usesdhcp>
        <encryptionkey />
        <ssid />
        <interface>
          <nicname>eth0</nicname>
          <myip>
            <ip>8.8.8.8</ip>
            <mask>255.255.255.0</mask>
            <gateway>0.0.0.0</gateway>
            <type>ip</type>
          </myip>
          <VLAN
            ID="1">Untagged</VLAN>
        </interface>
      </nic>
    </device>
    <device>
      <hostname>laptop0</hostname>
      <size>60</size>
      <uniqueidentifier>410</uniqueidentifier>
      <location>30,560</location>
      <mytype>laptop</mytype>
      <isdns>False</isdns>
      <isdhcp>False</isdhcp>
      <gateway>
        <ip>0.0.0.0</ip>
        <mask>0.0.0.0</mask>
        <gateway>0.0.0.0</gateway>
        <type>gw</type>
      </gateway>
      <nic>
        <nictype>lo</nictype>
        <nicname>lo0</nicname>
        <myid>
          <hostid>410</hostid>
          <nicid>411</nicid>
          <hostname>laptop0</hostname>
          <nicname>lo0</nicname>
        </myid>
        <nictype>lo</nictype>
        <uniqueidentifier>411</uniqueidentifier>
        <usesdhcp>False</usesdhcp>
        <interface>
          <nicname>lo0</nicname>
          <myip>
            <ip>127.0.0.1</ip>
            <mask>255.0.0.0</mask>
            <gateway>0.0.0.0</gateway>
            <type>ip</type>
          </myip>
          <VLAN
            ID="1">Untagged</VLAN>
        </interface>
      </nic>
      <nic>
        <nictype>eth</nictype>
        <nicname>eth0</nicname>
        <myid>
          <hostid>410</hostid>
          <nicid>412</nicid>
          <hostname>laptop0</hostname>
          <nicname>eth0</nicname>
        </myid>
        <nictype>eth</nictype>
        <uniqueidentifier>412</uniqueidentifier>
        <usesdhcp>True</usesdhcp>
        <interface>
          <nicname>eth0</nicname>
          <myip>
            <ip>0.0.0.0</ip>
            <mask>0.0.0.0</mask>
            <gateway>0.0.0.0</gateway>
            <type>ip</type>
          </myip>
          <VLAN
            ID="1">Untagged</VLAN>
        </interface>
      </nic>
      <nic>
        <nictype>wlan</nictype>
        <nicname>wlan2</nicname>
        <myid>
          <hostid>410</hostid>
          <nicid>413</nicid>
          <hostname>laptop0</hostname>
          <nicname>wlan2</nicname>
        </myid>
        <nictype>wlan</nictype>
        <uniqueidentifier>413</uniqueidentifier>
        <usesdhcp>True</usesdhcp>
        <interface>
          <nicname>wlan2</nicname>
          <myip>
            <ip>0.0.0.0</ip>
            <mask>0.0.0.0</mask>
            <gateway>0.0.0.0</gateway>
            <type>ip</type>
          </myip>
          <VLAN
            ID="1">Untagged</VLAN>
        </interface>
      </nic>
    </device>
    <device>
      <hostname>laptop1</hostname>
      <size>60</size>
      <uniqueidentifier>436</uniqueidentifier>
      <location>30,410</location>
      <mytype>laptop</mytype>
      <isdns>False</isdns>
      <isdhcp>False</isdhcp>
      <gateway>
        <ip>0.0.0.0</ip>
        <mask>0.0.0.0</mask>
        <gateway>0.0.0.0</gateway>
        <type>gw</type>
      </gateway>
      <nic>
        <nictype>lo</nictype>
        <nicname>lo0</nicname>
        <myid>
          <hostid>436</hostid>
          <nicid>437</nicid>
          <hostname>laptop1</hostname>
          <nicname>lo0</nicname>
        </myid>
        <nictype>lo</nictype>
        <uniqueidentifier>437</uniqueidentifier>
        <usesdhcp>False</usesdhcp>
        <interface>
          <nicname>lo0</nicname>
          <myip>
            <ip>127.0.0.1</ip>
            <mask>255.0.0.0</mask>
            <gateway>0.0.0.0</gateway>
            <type>ip</type>
          </myip>
          <VLAN
            ID="1">Untagged</VLAN>
        </interface>
      </nic>
      <nic>
        <nictype>eth</nictype>
        <nicname>eth0</nicname>
        <myid>
          <hostid>436</hostid>
          <nicid>438</nicid>
          <hostname>laptop1</hostname>
          <nicname>eth0</nicname>
        </myid>
        <nictype>eth</nictype>
        <uniqueidentifier>438</uniqueidentifier>
        <usesdhcp>False</usesdhcp>
        <interface>
          <nicname>eth0</nicname>
          <myip>
            <ip>0.0.0.0</ip>
            <mask>0.0.0.0</mask>
            <gateway>0.0.0.0</gateway>
            <type>ip</type>
          </myip>
          <VLAN
            ID="1">Untagged</VLAN>
        </interface>
      </nic>
      <nic>
        <nictype>wlan</nictype>
        <nicname>wlan2</nicname>
        <myid>
          <hostid>436</hostid>
          <nicid>439</nicid>
          <hostname>laptop1</hostname>
          <nicname>wlan2</nicname>
        </myid>
        <nictype>wlan</nictype>
        <uniqueidentifier>439</uniqueidentifier>
        <usesdhcp>True</usesdhcp>
        <encryptionkey>WirelessKey</encryptionkey>
        <ssid>LAN</ssid>
        <interface>
          <nicname>wlan2</nicname>
          <myip>
            <ip>0.0.0.0</ip>
            <mask>0.0.0.0</mask>
            <gateway>0.0.0.0</gateway>
            <type>ip</type>
          </myip>
          <VLAN
            ID="1">Untagged</VLAN>
        </interface>
      </nic>
    </device>
    <device>
      <hostname>net_switch0</hostname>
      <size>60</size>
      <uniqueidentifier>132</uniqueidentifier>
      <location>180,790</location>
      <mytype>net_switch</mytype>
      <isdns>False</isdns>
      <isdhcp>False</isdhcp>
      <gateway>
        <ip>192.168.1.1</ip>
        <mask>0.0.0.0</mask>
        <gateway>0.0.0.0</gateway>
        <type>gw</type>
      </gateway>
      <nic>
        <nictype>lo</nictype>
        <nicname>lo0</nicname>
        <myid>
          <hostid>132</hostid>
          <nicid>133</nicid>
          <hostname>net_switch0</hostname>
          <nicname>lo0</nicname>
        </myid>
        <nictype>lo</nictype>
        <uniqueidentifier>133</uniqueidentifier>
        <usesdhcp>False</usesdhcp>
        <encryptionkey />
        <ssid />
        <interface>
          <nicname>lo0</nicname>
          <myip>
            <ip>127.0.0.1</ip>
            <mask>255.0.0.0</mask>
            <gateway>0.0.0.0</gateway>
            <type>ip</type>
          </myip>
          <VLAN
            ID="1">Untagged</VLAN>
        </interface>
      </nic>
      <nic>
        <nictype>management_interface</nictype>
        <nicname>management_interface0</nicname>
        <myid>
          <hostid>132</hostid>
          <nicid>134</nicid>
          <hostname>net_switch0</hostname>
          <nicname>management_interface0</nicname>
        </myid>
        <nictype>management_interface</nictype>
        <uniqueidentifier>134</uniqueidentifier>
        <usesdhcp>False</usesdhcp>
        <encryptionkey />
        <ssid />
        <interface>
          <nicname>management_interface0</nicname>
          <myip>
            <ip>192.168.1.13</ip>
            <mask>255.255.255.0</mask>
            <gateway>0.0.0.0</gateway>
            <type>ip</type>
          </myip>
          <VLAN
            ID="1">Untagged</VLAN>
        </interface>
      </nic>
      <nic>
        <nictype>port</nictype>
        <nicname>port1</nicname>
        <myid>
          <hostid>132</hostid>
          <nicid>135</nicid>
          <hostname>net_switch0</hostname>
          <nicname>port1</nicname>
        </myid>
        <nictype>port</nictype>
        <uniqueidentifier>135</uniqueidentifier>
        <usesdhcp>False</usesdhcp>
        <encryptionkey />
        <ssid />
        <interface>
          <nicname>port1</nicname>
          <myip>
            <ip>0.0.0.0</ip>
            <mask>0.0.0.0</mask>
            <gateway>0.0.0.0</gateway>
            <type>ip</type>
          </myip>
          <VLAN
            ID="1">Untagged</VLAN>
        </interface>
      </nic>
      <nic>
        <nictype>port</nictype>
        <nicname>port2</nicname>
        <myid>
          <hostid>132</hostid>
          <nicid>136</nicid>
          <hostname>net_switch0</hostname>
          <nicname>port2</nicname>
        </myid>
        <nictype>port</nictype>
        <uniqueidentifier>136</uniqueidentifier>
        <usesdhcp>False</usesdhcp>
        <encryptionkey />
        <ssid />
        <interface>
          <nicname>port2</nicname>
          <myip>
            <ip>0.0.0.0</ip>
            <mask>0.0.0.0</mask>
            <gateway>0.0.0.0</gateway>
            <type>ip</type>
          </myip>
          <VLAN
            ID="1">Untagged</VLAN>
        </interface>
      </nic>
      <nic>
        <nictype>port</nictype>
        <nicname>port3</nicname>
        <myid>
          <hostid>132</hostid>
          <nicid>137</nicid>
          <hostname>net_switch0</hostname>
          <nicname>port3</nicname>
        </myid>
        <nictype>port</nictype>
        <uniqueidentifier>137</uniqueidentifier>
        <usesdhcp>False</usesdhcp>
        <encryptionkey />
        <ssid />
        <interface>
          <nicname>port3</nicname>
          <myip>
            <ip>0.0.0.0</ip>
            <mask>0.0.0.0</mask>
            <gateway>0.0.0.0</gateway>
            <type>ip</type>
          </myip>
          <VLAN
            ID="1">Untagged</VLAN>
        </interface>
      </nic>
      <nic>
        <nictype>port</nictype>
        <nicname>port4</nicname>
        <myid>
          <hostid>132</hostid>
          <nicid>138</nicid>
          <hostname>net_switch0</hostname>
          <nicname>port4</nicname>
        </myid>
        <nictype>port</nictype>
        <uniqueidentifier>138</uniqueidentifier>
        <usesdhcp>False</usesdhcp>
        <encryptionkey />
        <ssid />
        <interface>
          <nicname>port4</nicname>
          <myip>
            <ip>0.0.0.0</ip>
            <mask>0.0.0.0</mask>
            <gateway>0.0.0.0</gateway>
            <type>ip</type>
          </myip>
          <VLAN
            ID="1">Untagged</VLAN>
        </interface>
      </nic>
      <nic>
        <nictype>port</nictype>
        <nicname>port5</nicname>
        <myid>
          <hostid>132</hostid>
          <nicid>139</nicid>
          <hostname>net_switch0</hostname>
          <nicname>port5</nicname>
        </myid>
        <nictype>port</nictype>
        <uniqueidentifier>139</uniqueidentifier>
        <usesdhcp>False</usesdhcp>
        <encryptionkey />
        <ssid />
        <interface>
          <nicname>port5</nicname>
          <myip>
            <ip>0.0.0.0</ip>
            <mask>0.0.0.0</mask>
            <gateway>0.0.0.0</gateway>
            <type>ip</type>
          </myip>
          <VLAN
            ID="1">Untagged</VLAN>
        </interface>
      </nic>
      <nic>
        <nictype>port</nictype>
        <nicname>port6</nicname>
        <myid>
          <hostid>132</hostid>
          <nicid>140</nicid>
          <hostname>net_switch0</hostname>
          <nicname>port6</nicname>
        </myid>
        <nictype>port</nictype>
        <uniqueidentifier>140</uniqueidentifier>
        <usesdhcp>False</usesdhcp>
        <encryptionkey />
        <ssid />
        <interface>
          <nicname>port6</nicname>
          <myip>
            <ip>0.0.0.0</ip>
            <mask>0.0.0.0</mask>
            <gateway>0.0.0.0</gateway>
            <type>ip</type>
          </myip>
          <VLAN
            ID="1">Untagged</VLAN>
        </interface>
      </nic>
      <nic>
        <nictype>port</nictype>
        <nicname>port7</nicname>
        <myid>
          <hostid>132</hostid>
          <nicid>141</nicid>
          <hostname>net_switch0</hostname>
          <nicname>port7</nicname>
        </myid>
        <nictype>port</nictype>
        <uniqueidentifier>141</uniqueidentifier>
        <usesdhcp>False</usesdhcp>
        <encryptionkey />
        <ssid />
        <interface>
          <nicname>port7</nicname>
          <myip>
            <ip>0.0.0.0</ip>
            <mask>0.0.0.0</mask>
            <gateway>0.0.0.0</gateway>
            <type>ip</type>
          </myip>
          <VLAN
            ID="1">Untagged</VLAN>
        </interface>
      </nic>
    </device>
    <device>
      <hostname>net_switch1</hostname>
      <size>60</size>
      <uniqueidentifier>142</uniqueidentifier>
      <location>670,510</location>
      <mytype>net_switch</mytype>
      <isdns>False</isdns>
      <isdhcp>False</isdhcp>
      <gateway>
        <ip>192.168.1.1</ip>
        <mask>0.0.0.0</mask>
        <gateway>0.0.0.0</gateway>
        <type>gw</type>
      </gateway>
      <nic>
        <nictype>lo</nictype>
        <nicname>lo0</nicname>
        <myid>
          <hostid>142</hostid>
          <nicid>143</nicid>
          <hostname>net_switch1</hostname>
          <nicname>lo0</nicname>
        </myid>
        <nictype>lo</nictype>
        <uniqueidentifier>143</uniqueidentifier>
        <usesdhcp>False</usesdhcp>
        <encryptionkey />
        <ssid />
        <interface>
          <nicname>lo0</nicname>
          <myip>
            <ip>127.0.0.1</ip>
            <mask>255.0.0.0</mask>
            <gateway>0.0.0.0</gateway>
            <type>ip</type>
          </myip>
          <VLAN
            ID="1">Untagged</VLAN>
        </interface>
      </nic>
      <nic>
        <nictype>management_interface</nictype>
        <nicname>management_interface0</nicname>
        <myid>
          <hostid>142</hostid>
          <nicid>144</nicid>
          <hostname>net_switch1</hostname>
          <nicname>management_interface0</nicname>
        </myid>
        <nictype>management_interface</nictype>
        <uniqueidentifier>144</uniqueidentifier>
        <usesdhcp>False</usesdhcp>
        <encryptionkey />
        <ssid />
        <interface>
          <nicname>management_interface0</nicname>
          <myip>
            <ip>192.168.1.11</ip>
            <mask>255.255.255.0</mask>
            <gateway>0.0.0.0</gateway>
            <type>ip</type>
          </myip>
          <VLAN
            ID="1">Untagged</VLAN>
        </interface>
      </nic>
      <nic>
        <nictype>port</nictype>
        <nicname>port1</nicname>
        <myid>
          <hostid>142</hostid>
          <nicid>145</nicid>
          <hostname>net_switch1</hostname>
          <nicname>port1</nicname>
        </myid>
        <nictype>port</nictype>
        <uniqueidentifier>145</uniqueidentifier>
        <usesdhcp>False</usesdhcp>
        <encryptionkey />
        <ssid />
        <interface>
          <nicname>port1</nicname>
          <myip>
            <ip>0.0.0.0</ip>
            <mask>0.0.0.0</mask>
            <gateway>0.0.0.0</gateway>
            <type>ip</type>
          </myip>
          <VLAN
            ID="1">Untagged</VLAN>
        </interface>
      </nic>
      <nic>
        <nictype>port</nictype>
        <nicname>port2</nicname>
        <myid>
          <hostid>142</hostid>
          <nicid>146</nicid>
          <hostname>net_switch1</hostname>
          <nicname>port2</nicname>
        </myid>
        <nictype>port</nictype>
        <uniqueidentifier>146</uniqueidentifier>
        <usesdhcp>False</usesdhcp>
        <encryptionkey />
        <ssid />
        <interface>
          <nicname>port2</nicname>
          <myip>
            <ip>0.0.0.0</ip>
            <mask>0.0.0.0</mask>
            <gateway>0.0.0.0</gateway>
            <type>ip</type>
          </myip>
          <VLAN
            ID="1">Untagged</VLAN>
        </interface>
      </nic>
      <nic>
        <nictype>port</nictype>
        <nicname>port3</nicname>
        <myid>
          <hostid>142</hostid>
          <nicid>147</nicid>
          <hostname>net_switch1</hostname>
          <nicname>port3</nicname>
        </myid>
        <nictype>port</nictype>
        <uniqueidentifier>147</uniqueidentifier>
        <usesdhcp>False</usesdhcp>
        <encryptionkey />
        <ssid />
        <interface>
          <nicname>port3</nicname>
          <myip>
            <ip>0.0.0.0</ip>
            <mask>0.0.0.0</mask>
            <gateway>0.0.0.0</gateway>
            <type>ip</type>
          </myip>
          <VLAN
            ID="1">Untagged</VLAN>
        </interface>
      </nic>
      <nic>
        <nictype>port</nictype>
        <nicname>port4</nicname>
        <myid>
          <hostid>142</hostid>
          <nicid>148</nicid>
          <hostname>net_switch1</hostname>
          <nicname>port4</nicname>
        </myid>
        <nictype>port</nictype>
        <uniqueidentifier>148</uniqueidentifier>
        <usesdhcp>False</usesdhcp>
        <encryptionkey />
        <ssid />
        <interface>
          <nicname>port4</nicname>
          <myip>
            <ip>0.0.0.0</ip>
            <mask>0.0.0.0</mask>
            <gateway>0.0.0.0</gateway>
            <type>ip</type>
          </myip>
          <VLAN
            ID="1">Untagged</VLAN>
        </interface>
      </nic>
      <nic>
        <nictype>port</nictype>
        <nicname>port5</nicname>
        <myid>
          <hostid>142</hostid>
          <nicid>149</nicid>
          <hostname>net_switch1</hostname>
          <nicname>port5</nicname>
        </myid>
        <nictype>port</nictype>
        <uniqueidentifier>149</uniqueidentifier>
        <usesdhcp>False</usesdhcp>
        <encryptionkey />
        <ssid />
        <interface>
          <nicname>port5</nicname>
          <myip>
            <ip>0.0.0.0</ip>
            <mask>0.0.0.0</mask>
            <gateway>0.0.0.0</gateway>
            <type>ip</type>
          </myip>
          <VLAN
            ID="1">Untagged</VLAN>
        </interface>
      </nic>
      <nic>
        <nictype>port</nictype>
        <nicname>port6</nicname>
        <myid>
          <hostid>142</hostid>
          <nicid>150</nicid>
          <hostname>net_switch1</hostname>
          <nicname>port6</nicname>
        </myid>
        <nictype>port</nictype>
        <uniqueidentifier>150</uniqueidentifier>
        <usesdhcp>False</usesdhcp>
        <encryptionkey />
        <ssid />
        <interface>
          <nicname>port6</nicname>
          <myip>
            <ip>0.0.0.0</ip>
            <mask>0.0.0.0</mask>
            <gateway>0.0.0.0</gateway>
            <type>ip</type>
          </myip>
          <VLAN
            ID="1">Untagged</VLAN>
        </interface>
      </nic>
      <nic>
        <nictype>port</nictype>
        <nicname>port7</nicname>
        <myid>
          <hostid>142</hostid>
          <nicid>151</nicid>
          <hostname>net_switch1</hostname>
          <nicname>port7</nicname>
        </myid>
        <nictype>port</nictype>
        <uniqueidentifier>151</uniqueidentifier>
        <usesdhcp>False</usesdhcp>
        <encryptionkey />
        <ssid />
        <interface>
          <nicname>port7</nicname>
          <myip>
            <ip>0.0.0.0</ip>
            <mask>0.0.0.0</mask>
            <gateway>0.0.0.0</gateway>
            <type>ip</type>
          </myip>
          <VLAN
            ID="1">Untagged</VLAN>
        </interface>
      </nic>
    </device>
    <device>
      <hostname>net_switch2</hostname>
      <size>60</size>
      <uniqueidentifier>283</uniqueidentifier>
      <location>670,270</location>
      <mytype>net_switch</mytype>
      <isdns>False</isdns>
      <isdhcp>False</isdhcp>
      <gateway>
        <ip>192.168.1.1</ip>
        <mask>0.0.0.0</mask>
        <gateway>0.0.0.0</gateway>
        <type>gw</type>
      </gateway>
      <nic>
        <nictype>lo</nictype>
        <nicname>lo0</nicname>
        <myid>
          <hostid>283</hostid>
          <nicid>284</nicid>
          <hostname>net_switch2</hostname>
          <nicname>lo0</nicname>
        </myid>
        <nictype>lo</nictype>
        <uniqueidentifier>284</uniqueidentifier>
        <usesdhcp>False</usesdhcp>
        <encryptionkey />
        <ssid />
        <interface>
          <nicname>lo0</nicname>
          <myip>
            <ip>127.0.0.1</ip>
            <mask>255.0.0.0</mask>
            <gateway>0.0.0.0</gateway>
            <type>ip</type>
          </myip>
          <VLAN
            ID="1">Untagged</VLAN>
        </interface>
      </nic>
      <nic>
        <nictype>management_interface</nictype>
        <nicname>management_interface0</nicname>
        <myid>
          <hostid>283</hostid>
          <nicid>285</nicid>
          <hostname>net_switch2</hostname>
          <nicname>management_interface0</nicname>
        </myid>
        <nictype>management_interface</nictype>
        <uniqueidentifier>285</uniqueidentifier>
        <usesdhcp>False</usesdhcp>
        <encryptionkey />
        <ssid />
        <interface>
          <nicname>management_interface0</nicname>
          <myip>
            <ip>192.168.1.10</ip>
            <mask>255.255.255.0</mask>
            <gateway>0.0.0.0</gateway>
            <type>ip</type>
          </myip>
          <VLAN
            ID="1">Untagged</VLAN>
        </interface>
      </nic>
      <nic>
        <nictype>port</nictype>
        <nicname>port1</nicname>
        <myid>
          <hostid>283</hostid>
          <nicid>286</nicid>
          <hostname>net_switch2</hostname>
          <nicname>port1</nicname>
        </myid>
        <nictype>port</nictype>
        <uniqueidentifier>286</uniqueidentifier>
        <usesdhcp>False</usesdhcp>
        <encryptionkey />
        <ssid />
        <interface>
          <nicname>port1</nicname>
          <myip>
            <ip>0.0.0.0</ip>
            <mask>0.0.0.0</mask>
            <gateway>0.0.0.0</gateway>
            <type>ip</type>
          </myip>
          <VLAN
            ID="1">Untagged</VLAN>
        </interface>
      </nic>
      <nic>
        <nictype>port</nictype>
        <nicname>port2</nicname>
        <myid>
          <hostid>283</hostid>
          <nicid>287</nicid>
          <hostname>net_switch2</hostname>
          <nicname>port2</nicname>
        </myid>
        <nictype>port</nictype>
        <uniqueidentifier>287</uniqueidentifier>
        <usesdhcp>False</usesdhcp>
        <encryptionkey />
        <ssid />
        <interface>
          <nicname>port2</nicname>
          <myip>
            <ip>0.0.0.0</ip>
            <mask>0.0.0.0</mask>
            <gateway>0.0.0.0</gateway>
            <type>ip</type>
          </myip>
          <VLAN
            ID="1">Untagged</VLAN>
        </interface>
      </nic>
      <nic>
        <nictype>port</nictype>
        <nicname>port3</nicname>
        <myid>
          <hostid>283</hostid>
          <nicid>288</nicid>
          <hostname>net_switch2</hostname>
          <nicname>port3</nicname>
        </myid>
        <nictype>port</nictype>
        <uniqueidentifier>288</uniqueidentifier>
        <usesdhcp>False</usesdhcp>
        <encryptionkey />
        <ssid />
        <interface>
          <nicname>port3</nicname>
          <myip>
            <ip>0.0.0.0</ip>
            <mask>0.0.0.0</mask>
            <gateway>0.0.0.0</gateway>
            <type>ip</type>
          </myip>
          <VLAN
            ID="1">Untagged</VLAN>
        </interface>
      </nic>
      <nic>
        <nictype>port</nictype>
        <nicname>port4</nicname>
        <myid>
          <hostid>283</hostid>
          <nicid>289</nicid>
          <hostname>net_switch2</hostname>
          <nicname>port4</nicname>
        </myid>
        <nictype>port</nictype>
        <uniqueidentifier>289</uniqueidentifier>
        <usesdhcp>False</usesdhcp>
        <encryptionkey />
        <ssid />
        <interface>
          <nicname>port4</nicname>
          <myip>
            <ip>0.0.0.0</ip>
            <mask>0.0.0.0</mask>
            <gateway>0.0.0.0</gateway>
            <type>ip</type>
          </myip>
          <VLAN
            ID="1">Untagged</VLAN>
        </interface>
      </nic>
      <nic>
        <nictype>port</nictype>
        <nicname>port5</nicname>
        <myid>
          <hostid>283</hostid>
          <nicid>290</nicid>
          <hostname>net_switch2</hostname>
          <nicname>port5</nicname>
        </myid>
        <nictype>port</nictype>
        <uniqueidentifier>290</uniqueidentifier>
        <usesdhcp>False</usesdhcp>
        <encryptionkey />
        <ssid />
        <interface>
          <nicname>port5</nicname>
          <myip>
            <ip>0.0.0.0</ip>
            <mask>0.0.0.0</mask>
            <gateway>0.0.0.0</gateway>
            <type>ip</type>
          </myip>
          <VLAN
            ID="1">Untagged</VLAN>
        </interface>
      </nic>
      <nic>
        <nictype>port</nictype>
        <nicname>port6</nicname>
        <myid>
          <hostid>283</hostid>
          <nicid>291</nicid>
          <hostname>net_switch2</hostname>
          <nicname>port6</nicname>
        </myid>
        <nictype>port</nictype>
        <uniqueidentifier>291</uniqueidentifier>
        <usesdhcp>False</usesdhcp>
        <encryptionkey />
        <ssid />
        <interface>
          <nicname>port6</nicname>
          <myip>
            <ip>0.0.0.0</ip>
            <mask>0.0.0.0</mask>
            <gateway>0.0.0.0</gateway>
            <type>ip</type>
          </myip>
          <VLAN
            ID="1">Untagged</VLAN>
        </interface>
      </nic>
      <nic>
        <nictype>port</nictype>
        <nicname>port7</nicname>
        <myid>
          <hostid>283</hostid>
          <nicid>292</nicid>
          <hostname>net_switch2</hostname>
          <nicname>port7</nicname>
        </myid>
        <nictype>port</nictype>
        <uniqueidentifier>292</uniqueidentifier>
        <usesdhcp>False</usesdhcp>
        <encryptionkey />
        <ssid />
        <interface>
          <nicname>port7</nicname>
          <myip>
            <ip>0.0.0.0</ip>
            <mask>0.0.0.0</mask>
            <gateway>0.0.0.0</gateway>
            <type>ip</type>
          </myip>
          <VLAN
            ID="1">Untagged</VLAN>
        </interface>
      </nic>
    </device>
    <device>
      <hostname>net_switch3</hostname>
      <size>60</size>
      <uniqueidentifier>388</uniqueidentifier>
      <location>180,230</location>
      <mytype>net_switch</mytype>
      <isdns>False</isdns>
      <isdhcp>False</isdhcp>
      <gateway>
        <ip>192.168.1.1</ip>
        <mask>0.0.0.0</mask>
        <gateway>0.0.0.0</gateway>
        <type>gw</type>
      </gateway>
      <nic>
        <nictype>lo</nictype>
        <nicname>lo0</nicname>
        <myid>
          <hostid>388</hostid>
          <nicid>389</nicid>
          <hostname>net_switch3</hostname>
          <nicname>lo0</nicname>
        </myid>
        <nictype>lo</nictype>
        <uniqueidentifier>389</uniqueidentifier>
        <usesdhcp>False</usesdhcp>
        <interface>
          <nicname>lo0</nicname>
          <myip>
            <ip>127.0.0.1</ip>
            <mask>255.0.0.0</mask>
            <gateway>0.0.0.0</gateway>
            <type>ip</type>
          </myip>
          <VLAN
            ID="1">Untagged</VLAN>
        </interface>
      </nic>
      <nic>
        <nictype>management_interface</nictype>
        <nicname>management_interface0</nicname>
        <myid>
          <hostid>388</hostid>
          <nicid>390</nicid>
          <hostname>net_switch3</hostname>
          <nicname>management_interface0</nicname>
        </myid>
        <nictype>management_interface</nictype>
        <uniqueidentifier>390</uniqueidentifier>
        <usesdhcp>False</usesdhcp>
        <interface>
          <nicname>management_interface0</nicname>
          <myip>
            <ip>192.168.1.12</ip>
            <mask>255.255.255.0</mask>
            <gateway>0.0.0.0</gateway>
            <type>ip</type>
          </myip>
          <VLAN
            ID="1">Untagged</VLAN>
        </interface>
      </nic>
      <nic>
        <nictype>port</nictype>
        <nicname>port1</nicname>
        <myid>
          <hostid>388</hostid>
          <nicid>391</nicid>
          <hostname>net_switch3</hostname>
          <nicname>port1</nicname>
        </myid>
        <nictype>port</nictype>
        <uniqueidentifier>391</uniqueidentifier>
        <usesdhcp>False</usesdhcp>
        <interface>
          <nicname>port1</nicname>
          <myip>
            <ip>0.0.0.0</ip>
            <mask>0.0.0.0</mask>
            <gateway>0.0.0.0</gateway>
            <type>ip</type>
          </myip>
          <VLAN
            ID="1">Untagged</VLAN>
        </interface>
      </nic>
      <nic>
        <nictype>port</nictype>
        <nicname>port2</nicname>
        <myid>
          <hostid>388</hostid>
          <nicid>392</nicid>
          <hostname>net_switch3</hostname>
          <nicname>port2</nicname>
        </myid>
        <nictype>port</nictype>
        <uniqueidentifier>392</uniqueidentifier>
        <usesdhcp>False</usesdhcp>
        <interface>
          <nicname>port2</nicname>
          <myip>
            <ip>0.0.0.0</ip>
            <mask>0.0.0.0</mask>
            <gateway>0.0.0.0</gateway>
            <type>ip</type>
          </myip>
          <VLAN
            ID="1">Untagged</VLAN>
        </interface>
      </nic>
      <nic>
        <nictype>port</nictype>
        <nicname>port3</nicname>
        <myid>
          <hostid>388</hostid>
          <nicid>393</nicid>
          <hostname>net_switch3</hostname>
          <nicname>port3</nicname>
        </myid>
        <nictype>port</nictype>
        <uniqueidentifier>393</uniqueidentifier>
        <usesdhcp>False</usesdhcp>
        <interface>
          <nicname>port3</nicname>
          <myip>
            <ip>0.0.0.0</ip>
            <mask>0.0.0.0</mask>
            <gateway>0.0.0.0</gateway>
            <type>ip</type>
          </myip>
          <VLAN
            ID="1">Untagged</VLAN>
        </interface>
      </nic>
      <nic>
        <nictype>port</nictype>
        <nicname>port4</nicname>
        <myid>
          <hostid>388</hostid>
          <nicid>394</nicid>
          <hostname>net_switch3</hostname>
          <nicname>port4</nicname>
        </myid>
        <nictype>port</nictype>
        <uniqueidentifier>394</uniqueidentifier>
        <usesdhcp>False</usesdhcp>
        <interface>
          <nicname>port4</nicname>
          <myip>
            <ip>0.0.0.0</ip>
            <mask>0.0.0.0</mask>
            <gateway>0.0.0.0</gateway>
            <type>ip</type>
          </myip>
          <VLAN
            ID="1">Untagged</VLAN>
        </interface>
      </nic>
      <nic>
        <nictype>port</nictype>
        <nicname>port5</nicname>
        <myid>
          <hostid>388</hostid>
          <nicid>395</nicid>
          <hostname>net_switch3</hostname>
          <nicname>port5</nicname>
        </myid>
        <nictype>port</nictype>
        <uniqueidentifier>395</uniqueidentifier>
        <usesdhcp>False</usesdhcp>
        <interface>
          <nicname>port5</nicname>
          <myip>
            <ip>0.0.0.0</ip>
            <mask>0.0.0.0</mask>
            <gateway>0.0.0.0</gateway>
            <type>ip</type>
          </myip>
          <VLAN
            ID="1">Untagged</VLAN>
        </interface>
      </nic>
      <nic>
        <nictype>port</nictype>
        <nicname>port6</nicname>
        <myid>
          <hostid>388</hostid>
          <nicid>396</nicid>
          <hostname>net_switch3</hostname>
          <nicname>port6</nicname>
        </myid>
        <nictype>port</nictype>
        <uniqueidentifier>396</uniqueidentifier>
        <usesdhcp>False</usesdhcp>
        <interface>
          <nicname>port6</nicname>
          <myip>
            <ip>0.0.0.0</ip>
            <mask>0.0.0.0</mask>
            <gateway>0.0.0.0</gateway>
            <type>ip</type>
          </myip>
          <VLAN
            ID="1">Untagged</VLAN>
        </interface>
      </nic>
      <nic>
        <nictype>port</nictype>
        <nicname>port7</nicname>
        <myid>
          <hostid>388</hostid>
          <nicid>397</nicid>
          <hostname>net_switch3</hostname>
          <nicname>port7</nicname>
        </myid>
        <nictype>port</nictype>
        <uniqueidentifier>397</uniqueidentifier>
        <usesdhcp>False</usesdhcp>
        <interface>
          <nicname>port7</nicname>
          <myip>
            <ip>0.0.0.0</ip>
            <mask>0.0.0.0</mask>
            <gateway>0.0.0.0</gateway>
            <type>ip</type>
          </myip>
          <VLAN
            ID="1">Untagged</VLAN>
        </interface>
      </nic>
    </device>
    <device>
      <hostname>net_switch4</hostname>
      <size>60</size>
      <uniqueidentifier>467</uniqueidentifier>
      <location>180,510</location>
      <mytype>net_switch</mytype>
      <isdns>False</isdns>
      <isdhcp>False</isdhcp>
      <gateway>
        <ip>192.168.1.1</ip>
        <mask>0.0.0.0</mask>
        <gateway>0.0.0.0</gateway>
        <type>gw</type>
      </gateway>
      <nic>
        <nictype>lo</nictype>
        <nicname>lo0</nicname>
        <myid>
          <hostid>467</hostid>
          <nicid>468</nicid>
          <hostname>net_switch4</hostname>
          <nicname>lo0</nicname>
        </myid>
        <nictype>lo</nictype>
        <uniqueidentifier>468</uniqueidentifier>
        <usesdhcp>False</usesdhcp>
        <interface>
          <nicname>lo0</nicname>
          <myip>
            <ip>127.0.0.1</ip>
            <mask>255.0.0.0</mask>
            <gateway>0.0.0.0</gateway>
            <type>ip</type>
          </myip>
          <VLAN
            ID="1">Untagged</VLAN>
        </interface>
      </nic>
      <nic>
        <nictype>management_interface</nictype>
        <nicname>management_interface0</nicname>
        <myid>
          <hostid>467</hostid>
          <nicid>469</nicid>
          <hostname>net_switch4</hostname>
          <nicname>management_interface0</nicname>
        </myid>
        <nictype>management_interface</nictype>
        <uniqueidentifier>469</uniqueidentifier>
        <usesdhcp>False</usesdhcp>
        <interface>
          <nicname>management_interface0</nicname>
          <myip>
            <ip>192.168.1.14</ip>
            <mask>255.255.255.0</mask>
            <gateway>0.0.0.0</gateway>
            <type>ip</type>
          </myip>
          <VLAN
            ID="1">Untagged</VLAN>
        </interface>
      </nic>
      <nic>
        <nictype>port</nictype>
        <nicname>port1</nicname>
        <myid>
          <hostid>467</hostid>
          <nicid>470</nicid>
          <hostname>net_switch4</hostname>
          <nicname>port1</nicname>
        </myid>
        <nictype>port</nictype>
        <uniqueidentifier>470</uniqueidentifier>
        <usesdhcp>False</usesdhcp>
        <interface>
          <nicname>port1</nicname>
          <myip>
            <ip>0.0.0.0</ip>
            <mask>0.0.0.0</mask>
            <gateway>0.0.0.0</gateway>
            <type>ip</type>
          </myip>
          <VLAN
            ID="1">Untagged</VLAN>
        </interface>
      </nic>
      <nic>
        <nictype>port</nictype>
        <nicname>port2</nicname>
        <myid>
          <hostid>467</hostid>
          <nicid>471</nicid>
          <hostname>net_switch4</hostname>
          <nicname>port2</nicname>
        </myid>
        <nictype>port</nictype>
        <uniqueidentifier>471</uniqueidentifier>
        <usesdhcp>False</usesdhcp>
        <interface>
          <nicname>port2</nicname>
          <myip>
            <ip>0.0.0.0</ip>
            <mask>0.0.0.0</mask>
            <gateway>0.0.0.0</gateway>
            <type>ip</type>
          </myip>
          <VLAN
            ID="1">Untagged</VLAN>
        </interface>
      </nic>
      <nic>
        <nictype>port</nictype>
        <nicname>port3</nicname>
        <myid>
          <hostid>467</hostid>
          <nicid>472</nicid>
          <hostname>net_switch4</hostname>
          <nicname>port3</nicname>
        </myid>
        <nictype>port</nictype>
        <uniqueidentifier>472</uniqueidentifier>
        <usesdhcp>False</usesdhcp>
        <interface>
          <nicname>port3</nicname>
          <myip>
            <ip>0.0.0.0</ip>
            <mask>0.0.0.0</mask>
            <gateway>0.0.0.0</gateway>
            <type>ip</type>
          </myip>
          <VLAN
            ID="1">Untagged</VLAN>
        </interface>
      </nic>
      <nic>
        <nictype>port</nictype>
        <nicname>port4</nicname>
        <myid>
          <hostid>467</hostid>
          <nicid>473</nicid>
          <hostname>net_switch4</hostname>
          <nicname>port4</nicname>
        </myid>
        <nictype>port</nictype>
        <uniqueidentifier>473</uniqueidentifier>
        <usesdhcp>False</usesdhcp>
        <interface>
          <nicname>port4</nicname>
          <myip>
            <ip>0.0.0.0</ip>
            <mask>0.0.0.0</mask>
            <gateway>0.0.0.0</gateway>
            <type>ip</type>
          </myip>
          <VLAN
            ID="1">Untagged</VLAN>
        </interface>
      </nic>
      <nic>
        <nictype>port</nictype>
        <nicname>port5</nicname>
        <myid>
          <hostid>467</hostid>
          <nicid>474</nicid>
          <hostname>net_switch4</hostname>
          <nicname>port5</nicname>
        </myid>
        <nictype>port</nictype>
        <uniqueidentifier>474</uniqueidentifier>
        <usesdhcp>False</usesdhcp>
        <interface>
          <nicname>port5</nicname>
          <myip>
            <ip>0.0.0.0</ip>
            <mask>0.0.0.0</mask>
            <gateway>0.0.0.0</gateway>
            <type>ip</type>
          </myip>
          <VLAN
            ID="1">Untagged</VLAN>
        </interface>
      </nic>
      <nic>
        <nictype>port</nictype>
        <nicname>port6</nicname>
        <myid>
          <hostid>467</hostid>
          <nicid>475</nicid>
          <hostname>net_switch4</hostname>
          <nicname>port6</nicname>
        </myid>
        <nictype>port</nictype>
        <uniqueidentifier>475</uniqueidentifier>
        <usesdhcp>False</usesdhcp>
        <interface>
          <nicname>port6</nicname>
          <myip>
            <ip>0.0.0.0</ip>
            <mask>0.0.0.0</mask>
            <gateway>0.0.0.0</gateway>
            <type>ip</type>
          </myip>
          <VLAN
            ID="1">Untagged</VLAN>
        </interface>
      </nic>
      <nic>
        <nictype>port</nictype>
        <nicname>port7</nicname>
        <myid>
          <hostid>467</hostid>
          <nicid>476</nicid>
          <hostname>net_switch4</hostname>
          <nicname>port7</nicname>
        </myid>
        <nictype>port</nictype>
        <uniqueidentifier>476</uniqueidentifier>
        <usesdhcp>False</usesdhcp>
        <interface>
          <nicname>port7</nicname>
          <myip>
            <ip>0.0.0.0</ip>
            <mask>0.0.0.0</mask>
            <gateway>0.0.0.0</gateway>
            <type>ip</type>
          </myip>
          <VLAN
            ID="1">Untagged</VLAN>
        </interface>
      </nic>
    </device>
    <device>
      <hostname>net_switch5</hostname>
      <size>60</size>
      <uniqueidentifier>477</uniqueidentifier>
      <location>670,790</location>
      <mytype>net_switch</mytype>
      <isdns>False</isdns>
      <isdhcp>False</isdhcp>
      <gateway>
        <ip>192.168.1.11</ip>
        <mask>0.0.0.0</mask>
        <gateway>0.0.0.0</gateway>
        <type>gw</type>
      </gateway>
      <nic>
        <nictype>lo</nictype>
        <nicname>lo0</nicname>
        <myid>
          <hostid>477</hostid>
          <nicid>478</nicid>
          <hostname>net_switch5</hostname>
          <nicname>lo0</nicname>
        </myid>
        <nictype>lo</nictype>
        <uniqueidentifier>478</uniqueidentifier>
        <usesdhcp>False</usesdhcp>
        <interface>
          <nicname>lo0</nicname>
          <myip>
            <ip>127.0.0.1</ip>
            <mask>255.0.0.0</mask>
            <gateway>0.0.0.0</gateway>
            <type>ip</type>
          </myip>
          <VLAN
            ID="1">Untagged</VLAN>
        </interface>
      </nic>
      <nic>
        <nictype>management_interface</nictype>
        <nicname>management_interface0</nicname>
        <myid>
          <hostid>477</hostid>
          <nicid>479</nicid>
          <hostname>net_switch5</hostname>
          <nicname>management_interface0</nicname>
        </myid>
        <nictype>management_interface</nictype>
        <uniqueidentifier>479</uniqueidentifier>
        <usesdhcp>False</usesdhcp>
        <interface>
          <nicname>management_interface0</nicname>
          <myip>
            <ip>192.168.1.15</ip>
            <mask>255.255.255.0</mask>
            <gateway>0.0.0.0</gateway>
            <type>ip</type>
          </myip>
          <VLAN
            ID="1">Untagged</VLAN>
        </interface>
      </nic>
      <nic>
        <nictype>port</nictype>
        <nicname>port1</nicname>
        <myid>
          <hostid>477</hostid>
          <nicid>480</nicid>
          <hostname>net_switch5</hostname>
          <nicname>port1</nicname>
        </myid>
        <nictype>port</nictype>
        <uniqueidentifier>480</uniqueidentifier>
        <usesdhcp>False</usesdhcp>
        <interface>
          <nicname>port1</nicname>
          <myip>
            <ip>0.0.0.0</ip>
            <mask>0.0.0.0</mask>
            <gateway>0.0.0.0</gateway>
            <type>ip</type>
          </myip>
          <VLAN
            ID="1">Untagged</VLAN>
        </interface>
      </nic>
      <nic>
        <nictype>port</nictype>
        <nicname>port2</nicname>
        <myid>
          <hostid>477</hostid>
          <nicid>481</nicid>
          <hostname>net_switch5</hostname>
          <nicname>port2</nicname>
        </myid>
        <nictype>port</nictype>
        <uniqueidentifier>481</uniqueidentifier>
        <usesdhcp>False</usesdhcp>
        <interface>
          <nicname>port2</nicname>
          <myip>
            <ip>0.0.0.0</ip>
            <mask>0.0.0.0</mask>
            <gateway>0.0.0.0</gateway>
            <type>ip</type>
          </myip>
          <VLAN
            ID="1">Untagged</VLAN>
        </interface>
      </nic>
      <nic>
        <nictype>port</nictype>
        <nicname>port3</nicname>
        <myid>
          <hostid>477</hostid>
          <nicid>482</nicid>
          <hostname>net_switch5</hostname>
          <nicname>port3</nicname>
        </myid>
        <nictype>port</nictype>
        <uniqueidentifier>482</uniqueidentifier>
        <usesdhcp>False</usesdhcp>
        <interface>
          <nicname>port3</nicname>
          <myip>
            <ip>0.0.0.0</ip>
            <mask>0.0.0.0</mask>
            <gateway>0.0.0.0</gateway>
            <type>ip</type>
          </myip>
          <VLAN
            ID="1">Untagged</VLAN>
        </interface>
      </nic>
      <nic>
        <nictype>port</nictype>
        <nicname>port4</nicname>
        <myid>
          <hostid>477</hostid>
          <nicid>483</nicid>
          <hostname>net_switch5</hostname>
          <nicname>port4</nicname>
        </myid>
        <nictype>port</nictype>
        <uniqueidentifier>483</uniqueidentifier>
        <usesdhcp>False</usesdhcp>
        <interface>
          <nicname>port4</nicname>
          <myip>
            <ip>0.0.0.0</ip>
            <mask>0.0.0.0</mask>
            <gateway>0.0.0.0</gateway>
            <type>ip</type>
          </myip>
          <VLAN
            ID="1">Untagged</VLAN>
        </interface>
      </nic>
      <nic>
        <nictype>port</nictype>
        <nicname>port5</nicname>
        <myid>
          <hostid>477</hostid>
          <nicid>484</nicid>
          <hostname>net_switch5</hostname>
          <nicname>port5</nicname>
        </myid>
        <nictype>port</nictype>
        <uniqueidentifier>484</uniqueidentifier>
        <usesdhcp>False</usesdhcp>
        <interface>
          <nicname>port5</nicname>
          <myip>
            <ip>0.0.0.0</ip>
            <mask>0.0.0.0</mask>
            <gateway>0.0.0.0</gateway>
            <type>ip</type>
          </myip>
          <VLAN
            ID="1">Untagged</VLAN>
        </interface>
      </nic>
      <nic>
        <nictype>port</nictype>
        <nicname>port6</nicname>
        <myid>
          <hostid>477</hostid>
          <nicid>485</nicid>
          <hostname>net_switch5</hostname>
          <nicname>port6</nicname>
        </myid>
        <nictype>port</nictype>
        <uniqueidentifier>485</uniqueidentifier>
        <usesdhcp>False</usesdhcp>
        <interface>
          <nicname>port6</nicname>
          <myip>
            <ip>0.0.0.0</ip>
            <mask>0.0.0.0</mask>
            <gateway>0.0.0.0</gateway>
            <type>ip</type>
          </myip>
          <VLAN
            ID="1">Untagged</VLAN>
        </interface>
      </nic>
      <nic>
        <nictype>port</nictype>
        <nicname>port7</nicname>
        <myid>
          <hostid>477</hostid>
          <nicid>486</nicid>
          <hostname>net_switch5</hostname>
          <nicname>port7</nicname>
        </myid>
        <nictype>port</nictype>
        <uniqueidentifier>486</uniqueidentifier>
        <usesdhcp>False</usesdhcp>
        <interface>
          <nicname>port7</nicname>
          <myip>
            <ip>0.0.0.0</ip>
            <mask>0.0.0.0</mask>
            <gateway>0.0.0.0</gateway>
            <type>ip</type>
          </myip>
          <VLAN
            ID="1">Untagged</VLAN>
        </interface>
      </nic>
    </device>
    <device>
      <hostname>pc0</hostname>
      <size>60</size>
      <uniqueidentifier>109</uniqueidentifier>
      <location>40,660</location>
      <mytype>pc</mytype>
      <isdns>False</isdns>
      <isdhcp>False</isdhcp>
      <gateway>
        <ip>192.168.1.1</ip>
        <mask>0.0.0.0</mask>
        <gateway>0.0.0.0</gateway>
        <type>gw</type>
      </gateway>
      <nic>
        <nictype>lo</nictype>
        <nicname>lo0</nicname>
        <myid>
          <hostid>109</hostid>
          <nicid>110</nicid>
          <hostname>pc0</hostname>
          <nicname>lo0</nicname>
        </myid>
        <nictype>lo</nictype>
        <uniqueidentifier>110</uniqueidentifier>
        <usesdhcp>False</usesdhcp>
        <encryptionkey />
        <ssid />
        <interface>
          <nicname>lo0</nicname>
          <myip>
            <ip>127.0.0.1</ip>
            <mask>255.0.0.0</mask>
            <gateway>0.0.0.0</gateway>
            <type>ip</type>
          </myip>
          <VLAN
            ID="1">Untagged</VLAN>
        </interface>
      </nic>
      <nic>
        <nictype>eth</nictype>
        <nicname>eth0</nicname>
        <myid>
          <hostid>109</hostid>
          <nicid>111</nicid>
          <hostname>pc0</hostname>
          <nicname>eth0</nicname>
        </myid>
        <nictype>eth</nictype>
        <uniqueidentifier>111</uniqueidentifier>
        <usesdhcp>False</usesdhcp>
        <encryptionkey />
        <ssid />
        <interface>
          <nicname>eth0</nicname>
          <myip>
            <ip>192.168.1.22</ip>
            <mask>255.255.255.0</mask>
            <gateway>0.0.0.0</gateway>
            <type>ip</type>
          </myip>
          <VLAN
            ID="1">Untagged</VLAN>
        </interface>
      </nic>
    </device>
    <device>
      <hostname>pc1</hostname>
      <size>60</size>
      <uniqueidentifier>112</uniqueidentifier>
      <location>40,780</location>
      <mytype>pc</mytype>
      <isdns>False</isdns>
      <isdhcp>False</isdhcp>
      <gateway>
        <ip>192.168.1.1</ip>
        <mask>0.0.0.0</mask>
        <gateway>0.0.0.0</gateway>
        <type>gw</type>
      </gateway>
      <nic>
        <nictype>lo</nictype>
        <nicname>lo0</nicname>
        <myid>
          <hostid>112</hostid>
          <nicid>113</nicid>
          <hostname>pc1</hostname>
          <nicname>lo0</nicname>
        </myid>
        <nictype>lo</nictype>
        <uniqueidentifier>113</uniqueidentifier>
        <usesdhcp>False</usesdhcp>
        <encryptionkey />
        <ssid />
        <interface>
          <nicname>lo0</nicname>
          <myip>
            <ip>127.0.0.1</ip>
            <mask>255.0.0.0</mask>
            <gateway>0.0.0.0</gateway>
            <type>ip</type>
          </myip>
          <VLAN
            ID="1">Untagged</VLAN>
        </interface>
      </nic>
      <nic>
        <nictype>eth</nictype>
        <nicname>eth0</nicname>
        <myid>
          <hostid>112</hostid>
          <nicid>114</nicid>
          <hostname>pc1</hostname>
          <nicname>eth0</nicname>
        </myid>
        <nictype>eth</nictype>
        <uniqueidentifier>114</uniqueidentifier>
        <usesdhcp>False</usesdhcp>
        <encryptionkey />
        <ssid />
        <interface>
          <nicname>eth0</nicname>
          <myip>
            <ip>192.168.1.23</ip>
            <mask>255.255.255.0</mask>
            <gateway>0.0.0.0</gateway>
            <type>ip</type>
          </myip>
          <VLAN
            ID="1">Untagged</VLAN>
        </interface>
      </nic>
    </device>
    <device>
      <hostname>pc2</hostname>
      <size>60</size>
      <uniqueidentifier>115</uniqueidentifier>
      <location>820,510</location>
      <mytype>pc</mytype>
      <isdns>False</isdns>
      <isdhcp>False</isdhcp>
      <gateway>
        <ip>192.168.1.1</ip>
        <mask>0.0.0.0</mask>
        <gateway>0.0.0.0</gateway>
        <type>gw</type>
      </gateway>
      <nic>
        <nictype>lo</nictype>
        <nicname>lo0</nicname>
        <myid>
          <hostid>115</hostid>
          <nicid>116</nicid>
          <hostname>pc2</hostname>
          <nicname>lo0</nicname>
        </myid>
        <nictype>lo</nictype>
        <uniqueidentifier>116</uniqueidentifier>
        <usesdhcp>False</usesdhcp>
        <encryptionkey />
        <ssid />
        <interface>
          <nicname>lo0</nicname>
          <myip>
            <ip>127.0.0.1</ip>
            <mask>255.0.0.0</mask>
            <gateway>0.0.0.0</gateway>
            <type>ip</type>
          </myip>
          <VLAN
            ID="1">Untagged</VLAN>
        </interface>
      </nic>
      <nic>
        <nictype>eth</nictype>
        <nicname>eth0</nicname>
        <myid>
          <hostid>115</hostid>
          <nicid>117</nicid>
          <hostname>pc2</hostname>
          <nicname>eth0</nicname>
        </myid>
        <nictype>eth</nictype>
        <uniqueidentifier>117</uniqueidentifier>
        <usesdhcp>False</usesdhcp>
        <encryptionkey />
        <ssid />
        <interface>
          <nicname>eth0</nicname>
          <myip>
            <ip>192.168.1.20</ip>
            <mask>255.255.255.0</mask>
            <gateway>0.0.0.0</gateway>
            <type>ip</type>
          </myip>
          <VLAN
            ID="1">Untagged</VLAN>
        </interface>
      </nic>
    </device>
    <device>
      <hostname>pc3</hostname>
      <size>60</size>
      <uniqueidentifier>118</uniqueidentifier>
      <location>820,790</location>
      <mytype>pc</mytype>
      <isdns>False</isdns>
      <isdhcp>False</isdhcp>
      <gateway>
        <ip>192.168.1.1</ip>
        <mask>0.0.0.0</mask>
        <gateway>0.0.0.0</gateway>
        <type>gw</type>
      </gateway>
      <nic>
        <nictype>lo</nictype>
        <nicname>lo0</nicname>
        <myid>
          <hostid>118</hostid>
          <nicid>119</nicid>
          <hostname>pc3</hostname>
          <nicname>lo0</nicname>
        </myid>
        <nictype>lo</nictype>
        <uniqueidentifier>119</uniqueidentifier>
        <usesdhcp>False</usesdhcp>
        <encryptionkey />
        <ssid />
        <interface>
          <nicname>lo0</nicname>
          <myip>
            <ip>127.0.0.1</ip>
            <mask>255.0.0.0</mask>
            <gateway>0.0.0.0</gateway>
            <type>ip</type>
          </myip>
          <VLAN
            ID="1">Untagged</VLAN>
        </interface>
      </nic>
      <nic>
        <nictype>eth</nictype>
        <nicname>eth0</nicname>
        <myid>
          <hostid>118</hostid>
          <nicid>120</nicid>
          <hostname>pc3</hostname>
          <nicname>eth0</nicname>
        </myid>
        <nictype>eth</nictype>
        <uniqueidentifier>120</uniqueidentifier>
        <usesdhcp>False</usesdhcp>
        <encryptionkey />
        <ssid />
        <interface>
          <nicname>eth0</nicname>
          <myip>
            <ip>192.168.1.21</ip>
            <mask>255.255.255.0</mask>
            <gateway>0.0.0.0</gateway>
            <type>ip</type>
          </myip>
          <VLAN
            ID="1">Untagged</VLAN>
        </interface>
      </nic>
    </device>
    <device>
      <hostname>pc4</hostname>
      <size>60</size>
      <uniqueidentifier>398</uniqueidentifier>
      <location>30,200</location>
      <mytype>pc</mytype>
      <isdns>False</isdns>
      <isdhcp>False</isdhcp>
      <gateway>
        <ip>0.0.0.0</ip>
        <mask>0.0.0.0</mask>
        <gateway>0.0.0.0</gateway>
        <type>gw</type>
      </gateway>
      <nic>
        <nictype>lo</nictype>
        <nicname>lo0</nicname>
        <myid>
          <hostid>398</hostid>
          <nicid>399</nicid>
          <hostname>pc4</hostname>
          <nicname>lo0</nicname>
        </myid>
        <nictype>lo</nictype>
        <uniqueidentifier>399</uniqueidentifier>
        <usesdhcp>False</usesdhcp>
        <interface>
          <nicname>lo0</nicname>
          <myip>
            <ip>127.0.0.1</ip>
            <mask>255.0.0.0</mask>
            <gateway>0.0.0.0</gateway>
            <type>ip</type>
          </myip>
          <VLAN
            ID="1">Untagged</VLAN>
        </interface>
      </nic>
      <nic>
        <nictype>eth</nictype>
        <nicname>eth0</nicname>
        <myid>
          <hostid>398</hostid>
          <nicid>400</nicid>
          <hostname>pc4</hostname>
          <nicname>eth0</nicname>
        </myid>
        <nictype>eth</nictype>
        <uniqueidentifier>400</uniqueidentifier>
        <usesdhcp>True</usesdhcp>
        <interface>
          <nicname>eth0</nicname>
          <myip>
            <ip>0.0.0.0</ip>
            <mask>0.0.0.0</mask>
            <gateway>0.0.0.0</gateway>
            <type>ip</type>
          </myip>
          <VLAN
            ID="1">Untagged</VLAN>
        </interface>
      </nic>
    </device>
    <device>
      <hostname>pc5</hostname>
      <size>60</size>
      <uniqueidentifier>401</uniqueidentifier>
      <location>20,310</location>
      <mytype>pc</mytype>
      <isdns>False</isdns>
      <isdhcp>False</isdhcp>
      <gateway>
        <ip>0.0.0.0</ip>
        <mask>0.0.0.0</mask>
        <gateway>0.0.0.0</gateway>
        <type>gw</type>
      </gateway>
      <nic>
        <nictype>lo</nictype>
        <nicname>lo0</nicname>
        <myid>
          <hostid>401</hostid>
          <nicid>402</nicid>
          <hostname>pc5</hostname>
          <nicname>lo0</nicname>
        </myid>
        <nictype>lo</nictype>
        <uniqueidentifier>402</uniqueidentifier>
        <usesdhcp>False</usesdhcp>
        <interface>
          <nicname>lo0</nicname>
          <myip>
            <ip>127.0.0.1</ip>
            <mask>255.0.0.0</mask>
            <gateway>0.0.0.0</gateway>
            <type>ip</type>
          </myip>
          <VLAN
            ID="1">Untagged</VLAN>
        </interface>
      </nic>
      <nic>
        <nictype>eth</nictype>
        <nicname>eth0</nicname>
        <myid>
          <hostid>401</hostid>
          <nicid>403</nicid>
          <hostname>pc5</hostname>
          <nicname>eth0</nicname>
        </myid>
        <nictype>eth</nictype>
        <uniqueidentifier>403</uniqueidentifier>
        <usesdhcp>True</usesdhcp>
        <interface>
          <nicname>eth0</nicname>
          <myip>
            <ip>0.0.0.0</ip>
            <mask>0.0.0.0</mask>
            <gateway>0.0.0.0</gateway>
            <type>ip</type>
          </myip>
          <VLAN
            ID="1">Untagged</VLAN>
        </interface>
      </nic>
    </device>
    <device>
      <hostname>pc6</hostname>
      <size>60</size>
      <uniqueidentifier>404</uniqueidentifier>
      <location>820,360</location>
      <mytype>pc</mytype>
      <isdns>False</isdns>
      <isdhcp>False</isdhcp>
      <gateway>
        <ip>0.0.0.0</ip>
        <mask>0.0.0.0</mask>
        <gateway>0.0.0.0</gateway>
        <type>gw</type>
      </gateway>
      <nic>
        <nictype>lo</nictype>
        <nicname>lo0</nicname>
        <myid>
          <hostid>404</hostid>
          <nicid>405</nicid>
          <hostname>pc6</hostname>
          <nicname>lo0</nicname>
        </myid>
        <nictype>lo</nictype>
        <uniqueidentifier>405</uniqueidentifier>
        <usesdhcp>False</usesdhcp>
        <interface>
          <nicname>lo0</nicname>
          <myip>
            <ip>127.0.0.1</ip>
            <mask>255.0.0.0</mask>
            <gateway>0.0.0.0</gateway>
            <type>ip</type>
          </myip>
          <VLAN
            ID="1">Untagged</VLAN>
        </interface>
      </nic>
      <nic>
        <nictype>eth</nictype>
        <nicname>eth0</nicname>
        <myid>
          <hostid>404</hostid>
          <nicid>406</nicid>
          <hostname>pc6</hostname>
          <nicname>eth0</nicname>
        </myid>
        <nictype>eth</nictype>
        <uniqueidentifier>406</uniqueidentifier>
        <usesdhcp>True</usesdhcp>
        <interface>
          <nicname>eth0</nicname>
          <myip>
            <ip>0.0.0.0</ip>
            <mask>0.0.0.0</mask>
            <gateway>0.0.0.0</gateway>
            <type>ip</type>
          </myip>
          <VLAN
            ID="1">Untagged</VLAN>
        </interface>
      </nic>
    </device>
    <device>
      <hostname>pc7</hostname>
      <size>60</size>
      <uniqueidentifier>407</uniqueidentifier>
      <location>820,650</location>
      <mytype>pc</mytype>
      <isdns>False</isdns>
      <isdhcp>False</isdhcp>
      <gateway>
        <ip>0.0.0.0</ip>
        <mask>0.0.0.0</mask>
        <gateway>0.0.0.0</gateway>
        <type>gw</type>
      </gateway>
      <nic>
        <nictype>lo</nictype>
        <nicname>lo0</nicname>
        <myid>
          <hostid>407</hostid>
          <nicid>408</nicid>
          <hostname>pc7</hostname>
          <nicname>lo0</nicname>
        </myid>
        <nictype>lo</nictype>
        <uniqueidentifier>408</uniqueidentifier>
        <usesdhcp>False</usesdhcp>
        <interface>
          <nicname>lo0</nicname>
          <myip>
            <ip>127.0.0.1</ip>
            <mask>255.0.0.0</mask>
            <gateway>0.0.0.0</gateway>
            <type>ip</type>
          </myip>
          <VLAN
            ID="1">Untagged</VLAN>
        </interface>
      </nic>
      <nic>
        <nictype>eth</nictype>
        <nicname>eth0</nicname>
        <myid>
          <hostid>407</hostid>
          <nicid>409</nicid>
          <hostname>pc7</hostname>
          <nicname>eth0</nicname>
        </myid>
        <nictype>eth</nictype>
        <uniqueidentifier>409</uniqueidentifier>
        <usesdhcp>True</usesdhcp>
        <interface>
          <nicname>eth0</nicname>
          <myip>
            <ip>0.0.0.0</ip>
            <mask>0.0.0.0</mask>
            <gateway>0.0.0.0</gateway>
            <type>ip</type>
          </myip>
          <VLAN
            ID="1">Untagged</VLAN>
        </interface>
      </nic>
    </device>
    <device>
      <hostname>router0</hostname>
      <size>60</size>
      <uniqueidentifier>182</uniqueidentifier>
      <location>670,50</location>
      <mytype>router</mytype>
      <isdns>False</isdns>
      <isdhcp>False</isdhcp>
      <gateway>
        <ip>192.168.7.1</ip>
        <mask>0.0.0.0</mask>
        <gateway>0.0.0.0</gateway>
        <type>gw</type>
      </gateway>
      <nic>
        <nictype>lo</nictype>
        <nicname>lo0</nicname>
        <myid>
          <hostid>182</hostid>
          <nicid>183</nicid>
          <hostname>router0</hostname>
          <nicname>lo0</nicname>
        </myid>
        <nictype>lo</nictype>
        <uniqueidentifier>183</uniqueidentifier>
        <usesdhcp>False</usesdhcp>
        <encryptionkey />
        <ssid />
        <interface>
          <nicname>lo0</nicname>
          <myip>
            <ip>127.0.0.1</ip>
            <mask>255.0.0.0</mask>
            <gateway>0.0.0.0</gateway>
            <type>ip</type>
          </myip>
          <VLAN
            ID="1">Untagged</VLAN>
        </interface>
      </nic>
      <nic>
        <nictype>eth</nictype>
        <nicname>eth0</nicname>
        <myid>
          <hostid>182</hostid>
          <nicid>184</nicid>
          <hostname>router0</hostname>
          <nicname>eth0</nicname>
        </myid>
        <nictype>eth</nictype>
        <uniqueidentifier>184</uniqueidentifier>
        <usesdhcp>False</usesdhcp>
        <encryptionkey />
        <ssid />
        <interface>
          <nicname>eth0</nicname>
          <myip>
            <ip>192.168.5.1</ip>
            <mask>255.255.255.0</mask>
            <gateway>0.0.0.0</gateway>
            <type>ip</type>
          </myip>
          <VLAN
            ID="1">Untagged</VLAN>
        </interface>
      </nic>
      <nic>
        <nictype>eth</nictype>
        <nicname>eth1</nicname>
        <myid>
          <hostid>182</hostid>
          <nicid>185</nicid>
          <hostname>router0</hostname>
          <nicname>eth1</nicname>
        </myid>
        <nictype>eth</nictype>
        <uniqueidentifier>185</uniqueidentifier>
        <usesdhcp>False</usesdhcp>
        <encryptionkey />
        <ssid />
        <interface>
          <nicname>eth1</nicname>
          <myip>
            <ip>192.168.7.2</ip>
            <mask>255.255.255.0</mask>
            <gateway>0.0.0.0</gateway>
            <type>ip</type>
          </myip>
          <VLAN
            ID="1">Untagged</VLAN>
        </interface>
      </nic>
    </device>
    <device>
      <hostname>router1</hostname>
      <size>60</size>
      <uniqueidentifier>186</uniqueidentifier>
      <location>510,50</location>
      <mytype>router</mytype>
      <isdns>False</isdns>
      <isdhcp>False</isdhcp>
      <gateway>
        <ip>0.0.0.0</ip>
        <mask>0.0.0.0</mask>
        <gateway>0.0.0.0</gateway>
        <type>gw</type>
      </gateway>
      <nic>
        <nictype>lo</nictype>
        <nicname>lo0</nicname>
        <myid>
          <hostid>186</hostid>
          <nicid>187</nicid>
          <hostname>router1</hostname>
          <nicname>lo0</nicname>
        </myid>
        <nictype>lo</nictype>
        <uniqueidentifier>187</uniqueidentifier>
        <usesdhcp>False</usesdhcp>
        <encryptionkey />
        <ssid />
        <interface>
          <nicname>lo0</nicname>
          <myip>
            <ip>127.0.0.1</ip>
            <mask>255.0.0.0</mask>
            <gateway>0.0.0.0</gateway>
            <type>ip</type>
          </myip>
          <VLAN
            ID="1">Untagged</VLAN>
        </interface>
      </nic>
      <nic>
        <nictype>eth</nictype>
        <nicname>eth0</nicname>
        <myid>
          <hostid>186</hostid>
          <nicid>188</nicid>
          <hostname>router1</hostname>
          <nicname>eth0</nicname>
        </myid>
        <nictype>eth</nictype>
        <uniqueidentifier>188</uniqueidentifier>
        <usesdhcp>False</usesdhcp>
        <encryptionkey />
        <ssid />
        <interface>
          <nicname>eth0</nicname>
          <myip>
            <ip>8.8.8.1</ip>
            <mask>255.255.255.0</mask>
            <gateway>0.0.0.0</gateway>
            <type>ip</type>
          </myip>
          <VLAN
            ID="1">Untagged</VLAN>
        </interface>
      </nic>
      <nic>
        <nictype>eth</nictype>
        <nicname>eth1</nicname>
        <myid>
          <hostid>186</hostid>
          <nicid>189</nicid>
          <hostname>router1</hostname>
          <nicname>eth1</nicname>
        </myid>
        <nictype>eth</nictype>
        <uniqueidentifier>189</uniqueidentifier>
        <usesdhcp>False</usesdhcp>
        <encryptionkey />
        <ssid />
        <interface>
          <nicname>eth1</nicname>
          <myip>
            <ip>192.168.7.1</ip>
            <mask>255.255.255.0</mask>
            <gateway>0.0.0.0</gateway>
            <type>ip</type>
          </myip>
          <VLAN
            ID="1">Untagged</VLAN>
        </interface>
      </nic>
      <route>
        <ip>192.168.5.0</ip>
        <mask>255.255.255.0</mask>
        <gateway>192.168.7.2</gateway>
        <type>route</type>
      </route>
    </device>
    <device>
      <hostname>server0</hostname>
      <size>60</size>
      <uniqueidentifier>302</uniqueidentifier>
      <location>826,209</location>
      <mytype>server</mytype>
      <isdns>False</isdns>
      <isdhcp>True</isdhcp>
      <gateway>
        <ip>192.168.1.1</ip>
        <mask>0.0.0.0</mask>
        <gateway>0.0.0.0</gateway>
        <type>gw</type>
      </gateway>
      <nic>
        <nictype>lo</nictype>
        <nicname>lo0</nicname>
        <myid>
          <hostid>302</hostid>
          <nicid>303</nicid>
          <hostname>server0</hostname>
          <nicname>lo0</nicname>
        </myid>
        <nictype>lo</nictype>
        <uniqueidentifier>303</uniqueidentifier>
        <usesdhcp>False</usesdhcp>
        <encryptionkey />
        <ssid />
        <interface>
          <nicname>lo0</nicname>
          <myip>
            <ip>127.0.0.1</ip>
            <mask>255.0.0.0</mask>
            <gateway>0.0.0.0</gateway>
            <type>ip</type>
          </myip>
          <VLAN
            ID="1">Untagged</VLAN>
        </interface>
      </nic>
      <nic>
        <nictype>eth</nictype>
        <nicname>eth0</nicname>
        <myid>
          <hostid>302</hostid>
          <nicid>304</nicid>
          <hostname>server0</hostname>
          <nicname>eth0</nicname>
        </myid>
        <nictype>eth</nictype>
        <uniqueidentifier>304</uniqueidentifier>
        <usesdhcp>False</usesdhcp>
        <encryptionkey />
        <ssid />
        <interface>
          <nicname>eth0</nicname>
          <myip>
            <ip>192.168.1.2</ip>
            <mask>255.255.255.0</mask>
            <gateway>0.0.0.0</gateway>
            <type>ip</type>
          </myip>
          <VLAN
            ID="1">Untagged</VLAN>
        </interface>
      </nic>
      <dhcprange>
        <ip>127.0.0.1</ip>
        <mask>0.0.0.0</mask>
        <gateway>0.0.0.0</gateway>
        <type>route</type>
      </dhcprange>
      <dhcprange>
        <ip>192.168.1.2</ip>
        <mask>192.168.1.50</mask>
        <gateway>192.168.1.70</gateway>
        <type>route</type>
      </dhcprange>
    </device>
    <device>
      <hostname>server1</hostname>
      <size>60</size>
      <uniqueidentifier>495</uniqueidentifier>
      <location>100,350</location>
      <mytype>server</mytype>
      <isdns>False</isdns>
      <isdhcp>False</isdhcp>
      <gateway>
        <ip>192.168.1.1</ip>
        <mask>0.0.0.0</mask>
        <gateway>0.0.0.0</gateway>
        <type>gw</type>
      </gateway>
      <nic>
        <nictype>lo</nictype>
        <nicname>lo0</nicname>
        <myid>
          <hostid>495</hostid>
          <nicid>496</nicid>
          <hostname>server1</hostname>
          <nicname>lo0</nicname>
        </myid>
        <nictype>lo</nictype>
        <uniqueidentifier>496</uniqueidentifier>
        <usesdhcp>False</usesdhcp>
        <interface>
          <nicname>lo0</nicname>
          <myip>
            <ip>127.0.0.1</ip>
            <mask>255.0.0.0</mask>
            <gateway>0.0.0.0</gateway>
            <type>ip</type>
          </myip>
          <VLAN
            ID="1">Untagged</VLAN>
        </interface>
      </nic>
      <nic>
        <nictype>eth</nictype>
        <nicname>eth0</nicname>
        <myid>
          <hostid>495</hostid>
          <nicid>497</nicid>
          <hostname>server1</hostname>
          <nicname>eth0</nicname>
        </myid>
        <nictype>eth</nictype>
        <uniqueidentifier>497</uniqueidentifier>
        <usesdhcp>False</usesdhcp>
        <interface>
          <nicname>eth0</nicname>
          <myip>
            <ip>192.168.1.3</ip>
            <mask>255.255.255.0</mask>
            <gateway>0.0.0.0</gateway>
            <type>ip</type>
          </myip>
          <VLAN
            ID="1">Untagged</VLAN>
        </interface>
      </nic>
    </device>
    <device>
      <hostname>tree0</hostname>
      <size>60</size>
      <uniqueidentifier>100</uniqueidentifier>
      <location>350,760</location>
      <mytype>tree</mytype>
      <isdns>False</isdns>
      <isdhcp>False</isdhcp>
      <gateway>
        <ip>0.0.0.0</ip>
        <mask>0.0.0.0</mask>
        <gateway>0.0.0.0</gateway>
        <type>gw</type>
      </gateway>
      <nic>
        <nictype>lo</nictype>
        <nicname>lo0</nicname>
        <myid>
          <hostid>100</hostid>
          <nicid>101</nicid>
          <hostname>tree0</hostname>
          <nicname>lo0</nicname>
        </myid>
        <nictype>lo</nictype>
        <uniqueidentifier>101</uniqueidentifier>
        <usesdhcp>False</usesdhcp>
        <encryptionkey />
        <ssid />
        <interface>
          <nicname>lo0</nicname>
          <myip>
            <ip>127.0.0.1</ip>
            <mask>255.0.0.0</mask>
            <gateway>0.0.0.0</gateway>
            <type>ip</type>
          </myip>
          <VLAN
            ID="1">Untagged</VLAN>
        </interface>
      </nic>
      <nic>
        <nictype>eth</nictype>
        <nicname>eth0</nicname>
        <myid>
          <hostid>100</hostid>
          <nicid>102</nicid>
          <hostname>tree0</hostname>
          <nicname>eth0</nicname>
        </myid>
        <nictype>eth</nictype>
        <uniqueidentifier>102</uniqueidentifier>
        <usesdhcp>False</usesdhcp>
        <encryptionkey />
        <ssid />
        <interface>
          <nicname>eth0</nicname>
          <myip>
            <ip>0.0.0.0</ip>
            <mask>0.0.0.0</mask>
            <gateway>0.0.0.0</gateway>
            <type>ip</type>
          </myip>
          <VLAN
            ID="1">Untagged</VLAN>
        </interface>
      </nic>
    </device>
    <device>
      <hostname>tree1</hostname>
      <size>60</size>
      <uniqueidentifier>103</uniqueidentifier>
      <location>390,610</location>
      <mytype>tree</mytype>
      <isdns>False</isdns>
      <isdhcp>False</isdhcp>
      <gateway>
        <ip>0.0.0.0</ip>
        <mask>0.0.0.0</mask>
        <gateway>0.0.0.0</gateway>
        <type>gw</type>
      </gateway>
      <nic>
        <nictype>lo</nictype>
        <nicname>lo0</nicname>
        <myid>
          <hostid>103</hostid>
          <nicid>104</nicid>
          <hostname>tree1</hostname>
          <nicname>lo0</nicname>
        </myid>
        <nictype>lo</nictype>
        <uniqueidentifier>104</uniqueidentifier>
        <usesdhcp>False</usesdhcp>
        <encryptionkey />
        <ssid />
        <interface>
          <nicname>lo0</nicname>
          <myip>
            <ip>127.0.0.1</ip>
            <mask>255.0.0.0</mask>
            <gateway>0.0.0.0</gateway>
            <type>ip</type>
          </myip>
          <VLAN
            ID="1">Untagged</VLAN>
        </interface>
      </nic>
      <nic>
        <nictype>eth</nictype>
        <nicname>eth0</nicname>
        <myid>
          <hostid>103</hostid>
          <nicid>105</nicid>
          <hostname>tree1</hostname>
          <nicname>eth0</nicname>
        </myid>
        <nictype>eth</nictype>
        <uniqueidentifier>105</uniqueidentifier>
        <usesdhcp>False</usesdhcp>
        <encryptionkey />
        <ssid />
        <interface>
          <nicname>eth0</nicname>
          <myip>
            <ip>0.0.0.0</ip>
            <mask>0.0.0.0</mask>
            <gateway>0.0.0.0</gateway>
            <type>ip</type>
          </myip>
          <VLAN
            ID="1">Untagged</VLAN>
        </interface>
      </nic>
    </device>
    <device>
      <hostname>tree10</hostname>
      <size>60</size>
      <uniqueidentifier>361</uniqueidentifier>
      <location>530,570</location>
      <mytype>tree</mytype>
      <isdns>False</isdns>
      <isdhcp>False</isdhcp>
      <gateway>
        <ip>0.0.0.0</ip>
        <mask>0.0.0.0</mask>
        <gateway>0.0.0.0</gateway>
        <type>gw</type>
      </gateway>
      <nic>
        <nictype>lo</nictype>
        <nicname>lo0</nicname>
        <myid>
          <hostid>361</hostid>
          <nicid>362</nicid>
          <hostname>tree10</hostname>
          <nicname>lo0</nicname>
        </myid>
        <nictype>lo</nictype>
        <uniqueidentifier>362</uniqueidentifier>
        <usesdhcp>False</usesdhcp>
        <interface>
          <nicname>lo0</nicname>
          <myip>
            <ip>127.0.0.1</ip>
            <mask>255.0.0.0</mask>
            <gateway>0.0.0.0</gateway>
            <type>ip</type>
          </myip>
          <VLAN
            ID="1">Untagged</VLAN>
        </interface>
      </nic>
      <nic>
        <nictype>eth</nictype>
        <nicname>eth0</nicname>
        <myid>
          <hostid>361</hostid>
          <nicid>363</nicid>
          <hostname>tree10</hostname>
          <nicname>eth0</nicname>
        </myid>
        <nictype>eth</nictype>
        <uniqueidentifier>363</uniqueidentifier>
        <usesdhcp>False</usesdhcp>
        <interface>
          <nicname>eth0</nicname>
          <myip>
            <ip>0.0.0.0</ip>
            <mask>0.0.0.0</mask>
            <gateway>0.0.0.0</gateway>
            <type>ip</type>
          </myip>
          <VLAN
            ID="1">Untagged</VLAN>
        </interface>
      </nic>
    </device>
    <device>
      <hostname>tree11</hostname>
      <size>60</size>
      <uniqueidentifier>364</uniqueidentifier>
      <location>510,840</location>
      <mytype>tree</mytype>
      <isdns>False</isdns>
      <isdhcp>False</isdhcp>
      <gateway>
        <ip>0.0.0.0</ip>
        <mask>0.0.0.0</mask>
        <gateway>0.0.0.0</gateway>
        <type>gw</type>
      </gateway>
      <nic>
        <nictype>lo</nictype>
        <nicname>lo0</nicname>
        <myid>
          <hostid>364</hostid>
          <nicid>365</nicid>
          <hostname>tree11</hostname>
          <nicname>lo0</nicname>
        </myid>
        <nictype>lo</nictype>
        <uniqueidentifier>365</uniqueidentifier>
        <usesdhcp>False</usesdhcp>
        <interface>
          <nicname>lo0</nicname>
          <myip>
            <ip>127.0.0.1</ip>
            <mask>255.0.0.0</mask>
            <gateway>0.0.0.0</gateway>
            <type>ip</type>
          </myip>
          <VLAN
            ID="1">Untagged</VLAN>
        </interface>
      </nic>
      <nic>
        <nictype>eth</nictype>
        <nicname>eth0</nicname>
        <myid>
          <hostid>364</hostid>
          <nicid>366</nicid>
          <hostname>tree11</hostname>
          <nicname>eth0</nicname>
        </myid>
        <nictype>eth</nictype>
        <uniqueidentifier>366</uniqueidentifier>
        <usesdhcp>False</usesdhcp>
        <interface>
          <nicname>eth0</nicname>
          <myip>
            <ip>0.0.0.0</ip>
            <mask>0.0.0.0</mask>
            <gateway>0.0.0.0</gateway>
            <type>ip</type>
          </myip>
          <VLAN
            ID="1">Untagged</VLAN>
        </interface>
      </nic>
    </device>
    <device>
      <hostname>tree12</hostname>
      <size>60</size>
      <uniqueidentifier>367</uniqueidentifier>
      <location>580,210</location>
      <mytype>tree</mytype>
      <isdns>False</isdns>
      <isdhcp>False</isdhcp>
      <gateway>
        <ip>0.0.0.0</ip>
        <mask>0.0.0.0</mask>
        <gateway>0.0.0.0</gateway>
        <type>gw</type>
      </gateway>
      <nic>
        <nictype>lo</nictype>
        <nicname>lo0</nicname>
        <myid>
          <hostid>367</hostid>
          <nicid>368</nicid>
          <hostname>tree12</hostname>
          <nicname>lo0</nicname>
        </myid>
        <nictype>lo</nictype>
        <uniqueidentifier>368</uniqueidentifier>
        <usesdhcp>False</usesdhcp>
        <interface>
          <nicname>lo0</nicname>
          <myip>
            <ip>127.0.0.1</ip>
            <mask>255.0.0.0</mask>
            <gateway>0.0.0.0</gateway>
            <type>ip</type>
          </myip>
          <VLAN
            ID="1">Untagged</VLAN>
        </interface>
      </nic>
      <nic>
        <nictype>eth</nictype>
        <nicname>eth0</nicname>
        <myid>
          <hostid>367</hostid>
          <nicid>369</nicid>
          <hostname>tree12</hostname>
          <nicname>eth0</nicname>
        </myid>
        <nictype>eth</nictype>
        <uniqueidentifier>369</uniqueidentifier>
        <usesdhcp>False</usesdhcp>
        <interface>
          <nicname>eth0</nicname>
          <myip>
            <ip>0.0.0.0</ip>
            <mask>0.0.0.0</mask>
            <gateway>0.0.0.0</gateway>
            <type>ip</type>
          </myip>
          <VLAN
            ID="1">Untagged</VLAN>
        </interface>
      </nic>
    </device>
    <device>
      <hostname>tree13</hostname>
      <size>60</size>
      <uniqueidentifier>370</uniqueidentifier>
      <location>260,210</location>
      <mytype>tree</mytype>
      <isdns>False</isdns>
      <isdhcp>False</isdhcp>
      <gateway>
        <ip>0.0.0.0</ip>
        <mask>0.0.0.0</mask>
        <gateway>0.0.0.0</gateway>
        <type>gw</type>
      </gateway>
      <nic>
        <nictype>lo</nictype>
        <nicname>lo0</nicname>
        <myid>
          <hostid>370</hostid>
          <nicid>371</nicid>
          <hostname>tree13</hostname>
          <nicname>lo0</nicname>
        </myid>
        <nictype>lo</nictype>
        <uniqueidentifier>371</uniqueidentifier>
        <usesdhcp>False</usesdhcp>
        <interface>
          <nicname>lo0</nicname>
          <myip>
            <ip>127.0.0.1</ip>
            <mask>255.0.0.0</mask>
            <gateway>0.0.0.0</gateway>
            <type>ip</type>
          </myip>
          <VLAN
            ID="1">Untagged</VLAN>
        </interface>
      </nic>
      <nic>
        <nictype>eth</nictype>
        <nicname>eth0</nicname>
        <myid>
          <hostid>370</hostid>
          <nicid>372</nicid>
          <hostname>tree13</hostname>
          <nicname>eth0</nicname>
        </myid>
        <nictype>eth</nictype>
        <uniqueidentifier>372</uniqueidentifier>
        <usesdhcp>False</usesdhcp>
        <interface>
          <nicname>eth0</nicname>
          <myip>
            <ip>0.0.0.0</ip>
            <mask>0.0.0.0</mask>
            <gateway>0.0.0.0</gateway>
            <type>ip</type>
          </myip>
          <VLAN
            ID="1">Untagged</VLAN>
        </interface>
      </nic>
    </device>
    <device>
      <hostname>tree14</hostname>
      <size>60</size>
      <uniqueidentifier>373</uniqueidentifier>
      <location>590,390</location>
      <mytype>tree</mytype>
      <isdns>False</isdns>
      <isdhcp>False</isdhcp>
      <gateway>
        <ip>0.0.0.0</ip>
        <mask>0.0.0.0</mask>
        <gateway>0.0.0.0</gateway>
        <type>gw</type>
      </gateway>
      <nic>
        <nictype>lo</nictype>
        <nicname>lo0</nicname>
        <myid>
          <hostid>373</hostid>
          <nicid>374</nicid>
          <hostname>tree14</hostname>
          <nicname>lo0</nicname>
        </myid>
        <nictype>lo</nictype>
        <uniqueidentifier>374</uniqueidentifier>
        <usesdhcp>False</usesdhcp>
        <interface>
          <nicname>lo0</nicname>
          <myip>
            <ip>127.0.0.1</ip>
            <mask>255.0.0.0</mask>
            <gateway>0.0.0.0</gateway>
            <type>ip</type>
          </myip>
          <VLAN
            ID="1">Untagged</VLAN>
        </interface>
      </nic>
      <nic>
        <nictype>eth</nictype>
        <nicname>eth0</nicname>
        <myid>
          <hostid>373</hostid>
          <nicid>375</nicid>
          <hostname>tree14</hostname>
          <nicname>eth0</nicname>
        </myid>
        <nictype>eth</nictype>
        <uniqueidentifier>375</uniqueidentifier>
        <usesdhcp>False</usesdhcp>
        <interface>
          <nicname>eth0</nicname>
          <myip>
            <ip>0.0.0.0</ip>
            <mask>0.0.0.0</mask>
            <gateway>0.0.0.0</gateway>
            <type>ip</type>
          </myip>
          <VLAN
            ID="1">Untagged</VLAN>
        </interface>
      </nic>
    </device>
    <device>
      <hostname>tree15</hostname>
      <size>60</size>
      <uniqueidentifier>376</uniqueidentifier>
      <location>260,380</location>
      <mytype>tree</mytype>
      <isdns>False</isdns>
      <isdhcp>False</isdhcp>
      <gateway>
        <ip>0.0.0.0</ip>
        <mask>0.0.0.0</mask>
        <gateway>0.0.0.0</gateway>
        <type>gw</type>
      </gateway>
      <nic>
        <nictype>lo</nictype>
        <nicname>lo0</nicname>
        <myid>
          <hostid>376</hostid>
          <nicid>377</nicid>
          <hostname>tree15</hostname>
          <nicname>lo0</nicname>
        </myid>
        <nictype>lo</nictype>
        <uniqueidentifier>377</uniqueidentifier>
        <usesdhcp>False</usesdhcp>
        <interface>
          <nicname>lo0</nicname>
          <myip>
            <ip>127.0.0.1</ip>
            <mask>255.0.0.0</mask>
            <gateway>0.0.0.0</gateway>
            <type>ip</type>
          </myip>
          <VLAN
            ID="1">Untagged</VLAN>
        </interface>
      </nic>
      <nic>
        <nictype>eth</nictype>
        <nicname>eth0</nicname>
        <myid>
          <hostid>376</hostid>
          <nicid>378</nicid>
          <hostname>tree15</hostname>
          <nicname>eth0</nicname>
        </myid>
        <nictype>eth</nictype>
        <uniqueidentifier>378</uniqueidentifier>
        <usesdhcp>False</usesdhcp>
        <interface>
          <nicname>eth0</nicname>
          <myip>
            <ip>0.0.0.0</ip>
            <mask>0.0.0.0</mask>
            <gateway>0.0.0.0</gateway>
            <type>ip</type>
          </myip>
          <VLAN
            ID="1">Untagged</VLAN>
        </interface>
      </nic>
    </device>
    <device>
      <hostname>tree2</hostname>
      <size>60</size>
      <uniqueidentifier>106</uniqueidentifier>
      <location>470,720</location>
      <mytype>tree</mytype>
      <isdns>False</isdns>
      <isdhcp>False</isdhcp>
      <gateway>
        <ip>0.0.0.0</ip>
        <mask>0.0.0.0</mask>
        <gateway>0.0.0.0</gateway>
        <type>gw</type>
      </gateway>
      <nic>
        <nictype>lo</nictype>
        <nicname>lo0</nicname>
        <myid>
          <hostid>106</hostid>
          <nicid>107</nicid>
          <hostname>tree2</hostname>
          <nicname>lo0</nicname>
        </myid>
        <nictype>lo</nictype>
        <uniqueidentifier>107</uniqueidentifier>
        <usesdhcp>False</usesdhcp>
        <encryptionkey />
        <ssid />
        <interface>
          <nicname>lo0</nicname>
          <myip>
            <ip>127.0.0.1</ip>
            <mask>255.0.0.0</mask>
            <gateway>0.0.0.0</gateway>
            <type>ip</type>
          </myip>
          <VLAN
            ID="1">Untagged</VLAN>
        </interface>
      </nic>
      <nic>
        <nictype>eth</nictype>
        <nicname>eth0</nicname>
        <myid>
          <hostid>106</hostid>
          <nicid>108</nicid>
          <hostname>tree2</hostname>
          <nicname>eth0</nicname>
        </myid>
        <nictype>eth</nictype>
        <uniqueidentifier>108</uniqueidentifier>
        <usesdhcp>False</usesdhcp>
        <encryptionkey />
        <ssid />
        <interface>
          <nicname>eth0</nicname>
          <myip>
            <ip>0.0.0.0</ip>
            <mask>0.0.0.0</mask>
            <gateway>0.0.0.0</gateway>
            <type>ip</type>
          </myip>
          <VLAN
            ID="1">Untagged</VLAN>
        </interface>
      </nic>
    </device>
    <device>
      <hostname>tree3</hostname>
      <size>60</size>
      <uniqueidentifier>225</uniqueidentifier>
      <location>320,660</location>
      <mytype>tree</mytype>
      <isdns>False</isdns>
      <isdhcp>False</isdhcp>
      <gateway>
        <ip>0.0.0.0</ip>
        <mask>0.0.0.0</mask>
        <gateway>0.0.0.0</gateway>
        <type>gw</type>
      </gateway>
      <nic>
        <nictype>lo</nictype>
        <nicname>lo0</nicname>
        <myid>
          <hostid>225</hostid>
          <nicid>226</nicid>
          <hostname>tree3</hostname>
          <nicname>lo0</nicname>
        </myid>
        <nictype>lo</nictype>
        <uniqueidentifier>226</uniqueidentifier>
        <usesdhcp>False</usesdhcp>
        <encryptionkey />
        <ssid />
        <interface>
          <nicname>lo0</nicname>
          <myip>
            <ip>127.0.0.1</ip>
            <mask>255.0.0.0</mask>
            <gateway>0.0.0.0</gateway>
            <type>ip</type>
          </myip>
          <VLAN
            ID="1">Untagged</VLAN>
        </interface>
      </nic>
      <nic>
        <nictype>eth</nictype>
        <nicname>eth0</nicname>
        <myid>
          <hostid>225</hostid>
          <nicid>227</nicid>
          <hostname>tree3</hostname>
          <nicname>eth0</nicname>
        </myid>
        <nictype>eth</nictype>
        <uniqueidentifier>227</uniqueidentifier>
        <usesdhcp>False</usesdhcp>
        <encryptionkey />
        <ssid />
        <interface>
          <nicname>eth0</nicname>
          <myip>
            <ip>0.0.0.0</ip>
            <mask>0.0.0.0</mask>
            <gateway>0.0.0.0</gateway>
            <type>ip</type>
          </myip>
          <VLAN
            ID="1">Untagged</VLAN>
        </interface>
      </nic>
    </device>
    <device>
      <hostname>tree4</hostname>
      <size>60</size>
      <uniqueidentifier>228</uniqueidentifier>
      <location>510,650</location>
      <mytype>tree</mytype>
      <isdns>False</isdns>
      <isdhcp>False</isdhcp>
      <gateway>
        <ip>0.0.0.0</ip>
        <mask>0.0.0.0</mask>
        <gateway>0.0.0.0</gateway>
        <type>gw</type>
      </gateway>
      <nic>
        <nictype>lo</nictype>
        <nicname>lo0</nicname>
        <myid>
          <hostid>228</hostid>
          <nicid>229</nicid>
          <hostname>tree4</hostname>
          <nicname>lo0</nicname>
        </myid>
        <nictype>lo</nictype>
        <uniqueidentifier>229</uniqueidentifier>
        <usesdhcp>False</usesdhcp>
        <encryptionkey />
        <ssid />
        <interface>
          <nicname>lo0</nicname>
          <myip>
            <ip>127.0.0.1</ip>
            <mask>255.0.0.0</mask>
            <gateway>0.0.0.0</gateway>
            <type>ip</type>
          </myip>
          <VLAN
            ID="1">Untagged</VLAN>
        </interface>
      </nic>
      <nic>
        <nictype>eth</nictype>
        <nicname>eth0</nicname>
        <myid>
          <hostid>228</hostid>
          <nicid>230</nicid>
          <hostname>tree4</hostname>
          <nicname>eth0</nicname>
        </myid>
        <nictype>eth</nictype>
        <uniqueidentifier>230</uniqueidentifier>
        <usesdhcp>False</usesdhcp>
        <encryptionkey />
        <ssid />
        <interface>
          <nicname>eth0</nicname>
          <myip>
            <ip>0.0.0.0</ip>
            <mask>0.0.0.0</mask>
            <gateway>0.0.0.0</gateway>
            <type>ip</type>
          </myip>
          <VLAN
            ID="1">Untagged</VLAN>
        </interface>
      </nic>
    </device>
    <device>
      <hostname>tree5</hostname>
      <size>60</size>
      <uniqueidentifier>314</uniqueidentifier>
      <location>360,300</location>
      <mytype>tree</mytype>
      <isdns>False</isdns>
      <isdhcp>False</isdhcp>
      <gateway>
        <ip>0.0.0.0</ip>
        <mask>0.0.0.0</mask>
        <gateway>0.0.0.0</gateway>
        <type>gw</type>
      </gateway>
      <nic>
        <nictype>lo</nictype>
        <nicname>lo0</nicname>
        <myid>
          <hostid>314</hostid>
          <nicid>315</nicid>
          <hostname>tree5</hostname>
          <nicname>lo0</nicname>
        </myid>
        <nictype>lo</nictype>
        <uniqueidentifier>315</uniqueidentifier>
        <usesdhcp>False</usesdhcp>
        <encryptionkey />
        <ssid />
        <interface>
          <nicname>lo0</nicname>
          <myip>
            <ip>127.0.0.1</ip>
            <mask>255.0.0.0</mask>
            <gateway>0.0.0.0</gateway>
            <type>ip</type>
          </myip>
          <VLAN
            ID="1">Untagged</VLAN>
        </interface>
      </nic>
      <nic>
        <nictype>eth</nictype>
        <nicname>eth0</nicname>
        <myid>
          <hostid>314</hostid>
          <nicid>316</nicid>
          <hostname>tree5</hostname>
          <nicname>eth0</nicname>
        </myid>
        <nictype>eth</nictype>
        <uniqueidentifier>316</uniqueidentifier>
        <usesdhcp>False</usesdhcp>
        <encryptionkey />
        <ssid />
        <interface>
          <nicname>eth0</nicname>
          <myip>
            <ip>0.0.0.0</ip>
            <mask>0.0.0.0</mask>
            <gateway>0.0.0.0</gateway>
            <type>ip</type>
          </myip>
          <VLAN
            ID="1">Untagged</VLAN>
        </interface>
      </nic>
    </device>
    <device>
      <hostname>tree6</hostname>
      <size>60</size>
      <uniqueidentifier>317</uniqueidentifier>
      <location>470,290</location>
      <mytype>tree</mytype>
      <isdns>False</isdns>
      <isdhcp>False</isdhcp>
      <gateway>
        <ip>0.0.0.0</ip>
        <mask>0.0.0.0</mask>
        <gateway>0.0.0.0</gateway>
        <type>gw</type>
      </gateway>
      <nic>
        <nictype>lo</nictype>
        <nicname>lo0</nicname>
        <myid>
          <hostid>317</hostid>
          <nicid>318</nicid>
          <hostname>tree6</hostname>
          <nicname>lo0</nicname>
        </myid>
        <nictype>lo</nictype>
        <uniqueidentifier>318</uniqueidentifier>
        <usesdhcp>False</usesdhcp>
        <encryptionkey />
        <ssid />
        <interface>
          <nicname>lo0</nicname>
          <myip>
            <ip>127.0.0.1</ip>
            <mask>255.0.0.0</mask>
            <gateway>0.0.0.0</gateway>
            <type>ip</type>
          </myip>
          <VLAN
            ID="1">Untagged</VLAN>
        </interface>
      </nic>
      <nic>
        <nictype>eth</nictype>
        <nicname>eth0</nicname>
        <myid>
          <hostid>317</hostid>
          <nicid>319</nicid>
          <hostname>tree6</hostname>
          <nicname>eth0</nicname>
        </myid>
        <nictype>eth</nictype>
        <uniqueidentifier>319</uniqueidentifier>
        <usesdhcp>False</usesdhcp>
        <encryptionkey />
        <ssid />
        <interface>
          <nicname>eth0</nicname>
          <myip>
            <ip>0.0.0.0</ip>
            <mask>0.0.0.0</mask>
            <gateway>0.0.0.0</gateway>
            <type>ip</type>
          </myip>
          <VLAN
            ID="1">Untagged</VLAN>
        </interface>
      </nic>
    </device>
    <device>
      <hostname>tree7</hostname>
      <size>60</size>
      <uniqueidentifier>320</uniqueidentifier>
      <location>370,430</location>
      <mytype>tree</mytype>
      <isdns>False</isdns>
      <isdhcp>False</isdhcp>
      <gateway>
        <ip>0.0.0.0</ip>
        <mask>0.0.0.0</mask>
        <gateway>0.0.0.0</gateway>
        <type>gw</type>
      </gateway>
      <nic>
        <nictype>lo</nictype>
        <nicname>lo0</nicname>
        <myid>
          <hostid>320</hostid>
          <nicid>321</nicid>
          <hostname>tree7</hostname>
          <nicname>lo0</nicname>
        </myid>
        <nictype>lo</nictype>
        <uniqueidentifier>321</uniqueidentifier>
        <usesdhcp>False</usesdhcp>
        <encryptionkey />
        <ssid />
        <interface>
          <nicname>lo0</nicname>
          <myip>
            <ip>127.0.0.1</ip>
            <mask>255.0.0.0</mask>
            <gateway>0.0.0.0</gateway>
            <type>ip</type>
          </myip>
          <VLAN
            ID="1">Untagged</VLAN>
        </interface>
      </nic>
      <nic>
        <nictype>eth</nictype>
        <nicname>eth0</nicname>
        <myid>
          <hostid>320</hostid>
          <nicid>322</nicid>
          <hostname>tree7</hostname>
          <nicname>eth0</nicname>
        </myid>
        <nictype>eth</nictype>
        <uniqueidentifier>322</uniqueidentifier>
        <usesdhcp>False</usesdhcp>
        <encryptionkey />
        <ssid />
        <interface>
          <nicname>eth0</nicname>
          <myip>
            <ip>0.0.0.0</ip>
            <mask>0.0.0.0</mask>
            <gateway>0.0.0.0</gateway>
            <type>ip</type>
          </myip>
          <VLAN
            ID="1">Untagged</VLAN>
        </interface>
      </nic>
    </device>
    <device>
      <hostname>tree8</hostname>
      <size>60</size>
      <uniqueidentifier>323</uniqueidentifier>
      <location>450,410</location>
      <mytype>tree</mytype>
      <isdns>False</isdns>
      <isdhcp>False</isdhcp>
      <gateway>
        <ip>0.0.0.0</ip>
        <mask>0.0.0.0</mask>
        <gateway>0.0.0.0</gateway>
        <type>gw</type>
      </gateway>
      <nic>
        <nictype>lo</nictype>
        <nicname>lo0</nicname>
        <myid>
          <hostid>323</hostid>
          <nicid>324</nicid>
          <hostname>tree8</hostname>
          <nicname>lo0</nicname>
        </myid>
        <nictype>lo</nictype>
        <uniqueidentifier>324</uniqueidentifier>
        <usesdhcp>False</usesdhcp>
        <encryptionkey />
        <ssid />
        <interface>
          <nicname>lo0</nicname>
          <myip>
            <ip>127.0.0.1</ip>
            <mask>255.0.0.0</mask>
            <gateway>0.0.0.0</gateway>
            <type>ip</type>
          </myip>
          <VLAN
            ID="1">Untagged</VLAN>
        </interface>
      </nic>
      <nic>
        <nictype>eth</nictype>
        <nicname>eth0</nicname>
        <myid>
          <hostid>323</hostid>
          <nicid>325</nicid>
          <hostname>tree8</hostname>
          <nicname>eth0</nicname>
        </myid>
        <nictype>eth</nictype>
        <uniqueidentifier>325</uniqueidentifier>
        <usesdhcp>False</usesdhcp>
        <encryptionkey />
        <ssid />
        <interface>
          <nicname>eth0</nicname>
          <myip>
            <ip>0.0.0.0</ip>
            <mask>0.0.0.0</mask>
            <gateway>0.0.0.0</gateway>
            <type>ip</type>
          </myip>
          <VLAN
            ID="1">Untagged</VLAN>
        </interface>
      </nic>
    </device>
    <device>
      <hostname>tree9</hostname>
      <size>60</size>
      <uniqueidentifier>358</uniqueidentifier>
      <location>300,570</location>
      <mytype>tree</mytype>
      <isdns>False</isdns>
      <isdhcp>False</isdhcp>
      <gateway>
        <ip>0.0.0.0</ip>
        <mask>0.0.0.0</mask>
        <gateway>0.0.0.0</gateway>
        <type>gw</type>
      </gateway>
      <nic>
        <nictype>lo</nictype>
        <nicname>lo0</nicname>
        <myid>
          <hostid>358</hostid>
          <nicid>359</nicid>
          <hostname>tree9</hostname>
          <nicname>lo0</nicname>
        </myid>
        <nictype>lo</nictype>
        <uniqueidentifier>359</uniqueidentifier>
        <usesdhcp>False</usesdhcp>
        <interface>
          <nicname>lo0</nicname>
          <myip>
            <ip>127.0.0.1</ip>
            <mask>255.0.0.0</mask>
            <gateway>0.0.0.0</gateway>
            <type>ip</type>
          </myip>
          <VLAN
            ID="1">Untagged</VLAN>
        </interface>
      </nic>
      <nic>
        <nictype>eth</nictype>
        <nicname>eth0</nicname>
        <myid>
          <hostid>358</hostid>
          <nicid>360</nicid>
          <hostname>tree9</hostname>
          <nicname>eth0</nicname>
        </myid>
        <nictype>eth</nictype>
        <uniqueidentifier>360</uniqueidentifier>
        <usesdhcp>False</usesdhcp>
        <interface>
          <nicname>eth0</nicname>
          <myip>
            <ip>0.0.0.0</ip>
            <mask>0.0.0.0</mask>
            <gateway>0.0.0.0</gateway>
            <type>ip</type>
          </myip>
          <VLAN
            ID="1">Untagged</VLAN>
        </interface>
      </nic>
    </device>
    <link>
      <SrcNic>
        <hostid>142</hostid>
        <nicid>151</nicid>
        <hostname>net_switch1</hostname>
        <nicname>port7</nicname>
      </SrcNic>
      <DstNic>
        <hostid>477</hostid>
        <nicid>486</nicid>
        <hostname>net_switch5</hostname>
        <nicname>port7</nicname>
      </DstNic>
      <hostname>net_switch1_link_net_switch5</hostname>
      <linktype>normal</linktype>
      <uniqueidentifier>487</uniqueidentifier>
    </link>
    <link>
      <SrcNic>
        <hostid>467</hostid>
        <nicid>475</nicid>
        <hostname>net_switch4</hostname>
        <nicname>port6</nicname>
      </SrcNic>
      <DstNic>
        <hostid>388</hostid>
        <nicid>397</nicid>
        <hostname>net_switch3</hostname>
        <nicname>port7</nicname>
      </DstNic>
      <hostname>net_switch4_link_net_switch3</hostname>
      <linktype>normal</linktype>
      <uniqueidentifier>490</uniqueidentifier>
    </link>
    <link>
      <SrcNic>
        <hostid>477</hostid>
        <nicid>481</nicid>
        <hostname>net_switch5</hostname>
        <nicname>port2</nicname>
      </SrcNic>
      <DstNic>
        <hostid>118</hostid>
        <nicid>120</nicid>
        <hostname>pc3</hostname>
        <nicname>eth0</nicname>
      </DstNic>
      <hostname>net_switch5_link_pc3</hostname>
      <linktype>normal</linktype>
      <uniqueidentifier>492</uniqueidentifier>
    </link>
    <link>
      <SrcNic>
        <hostid>132</hostid>
        <nicid>141</nicid>
        <hostname>net_switch0</hostname>
        <nicname>port7</nicname>
      </SrcNic>
      <DstNic>
        <hostid>477</hostid>
        <nicid>485</nicid>
        <hostname>net_switch5</hostname>
        <nicname>port6</nicname>
      </DstNic>
      <hostname>net_switch0_link_net_switch5</hostname>
      <linktype>normal</linktype>
      <uniqueidentifier>488</uniqueidentifier>
    </link>
    <link>
      <SrcNic>
        <hostid>436</hostid>
        <nicid>438</nicid>
        <hostname>laptop1</hostname>
        <nicname>eth0</nicname>
      </SrcNic>
      <DstNic>
        <hostid>467</hostid>
        <nicid>471</nicid>
        <hostname>net_switch4</hostname>
        <nicname>port2</nicname>
      </DstNic>
      <hostname>laptop1_link_net_switch4</hostname>
      <linktype>normal</linktype>
      <uniqueidentifier>494</uniqueidentifier>
    </link>
    <link>
      <SrcNic>
        <hostid>132</hostid>
        <nicid>140</nicid>
        <hostname>net_switch0</hostname>
        <nicname>port6</nicname>
      </SrcNic>
      <DstNic>
        <hostid>467</hostid>
        <nicid>476</nicid>
        <hostname>net_switch4</hostname>
        <nicname>port7</nicname>
      </DstNic>
      <hostname>net_switch0_link_net_switch4</hostname>
      <linktype>normal</linktype>
      <uniqueidentifier>489</uniqueidentifier>
    </link>
    <link>
      <SrcNic>
        <hostid>410</hostid>
        <nicid>412</nicid>
        <hostname>laptop0</hostname>
        <nicname>eth0</nicname>
      </SrcNic>
      <DstNic>
        <hostid>467</hostid>
        <nicid>470</nicid>
        <hostname>net_switch4</hostname>
        <nicname>port1</nicname>
      </DstNic>
      <hostname>laptop0_link_net_switch4</hostname>
      <linktype>normal</linktype>
      <uniqueidentifier>493</uniqueidentifier>
    </link>
    <link>
      <SrcNic>
        <hostid>477</hostid>
        <nicid>480</nicid>
        <hostname>net_switch5</hostname>
        <nicname>port1</nicname>
      </SrcNic>
      <DstNic>
        <hostid>407</hostid>
        <nicid>409</nicid>
        <hostname>pc7</hostname>
        <nicname>eth0</nicname>
      </DstNic>
      <hostname>net_switch5_link_pc7</hostname>
      <linktype>normal</linktype>
      <uniqueidentifier>491</uniqueidentifier>
    </link>
    <link>
      <SrcNic>
        <hostid>175</hostid>
        <nicid>179</nicid>
        <hostname>firewall0</hostname>
        <nicname>wan0</nicname>
      </SrcNic>
      <DstNic>
        <hostid>182</hostid>
        <nicid>184</nicid>
        <hostname>router0</hostname>
        <nicname>eth0</nicname>
      </DstNic>
      <hostname>firewall0_link_router0</hostname>
      <linktype>normal</linktype>
      <uniqueidentifier>247</uniqueidentifier>
    </link>
    <link>
      <SrcNic>
        <hostid>190</hostid>
        <nicid>192</nicid>
        <hostname>server0</hostname>
        <nicname>eth0</nicname>
      </SrcNic>
      <DstNic>
        <hostid>186</hostid>
        <nicid>188</nicid>
        <hostname>router1</hostname>
        <nicname>eth0</nicname>
      </DstNic>
      <hostname>google.com_link_router1</hostname>
      <linktype>normal</linktype>
      <uniqueidentifier>193</uniqueidentifier>
    </link>
    <link>
      <SrcNic>
        <hostid>142</hostid>
        <nicid>150</nicid>
        <hostname>net_switch1</hostname>
        <nicname>port6</nicname>
      </SrcNic>
      <DstNic>
        <hostid>283</hostid>
        <nicid>292</nicid>
        <hostname>net_switch2</hostname>
        <nicname>port7</nicname>
      </DstNic>
      <hostname>net_switch1_link_net_switch2</hostname>
      <linktype>normal</linktype>
      <uniqueidentifier>294</uniqueidentifier>
    </link>
    <link>
      <SrcNic>
        <hostid>283</hostid>
        <nicid>286</nicid>
        <hostname>net_switch2</hostname>
        <nicname>port1</nicname>
      </SrcNic>
      <DstNic>
        <hostid>175</hostid>
        <nicid>177</nicid>
        <hostname>firewall0</hostname>
        <nicname>eth0</nicname>
      </DstNic>
      <hostname>net_switch2_link_firewall0</hostname>
      <linktype>normal</linktype>
      <uniqueidentifier>296</uniqueidentifier>
    </link>
    <link>
      <SrcNic>
        <hostid>283</hostid>
        <nicid>288</nicid>
        <hostname>net_switch2</hostname>
        <nicname>port3</nicname>
      </SrcNic>
      <DstNic>
        <hostid>404</hostid>
        <nicid>406</nicid>
        <hostname>pc6</hostname>
        <nicname>eth0</nicname>
      </DstNic>
      <hostname>net_switch2_link_pc6</hostname>
      <linktype>normal</linktype>
      <uniqueidentifier>450</uniqueidentifier>
    </link>
    <link>
      <SrcNic>
        <hostid>283</hostid>
        <nicid>287</nicid>
        <hostname>net_switch2</hostname>
        <nicname>port2</nicname>
      </SrcNic>
      <DstNic>
        <hostid>302</hostid>
        <nicid>304</nicid>
        <hostname>server0</hostname>
        <nicname>eth0</nicname>
      </DstNic>
      <hostname>net_switch2_link_server0</hostname>
      <linktype>normal</linktype>
      <uniqueidentifier>306</uniqueidentifier>
    </link>
    <link>
      <SrcNic>
        <hostid>109</hostid>
        <nicid>111</nicid>
        <hostname>pc0</hostname>
        <nicname>eth0</nicname>
      </SrcNic>
      <DstNic>
        <hostid>132</hostid>
        <nicid>136</nicid>
        <hostname>net_switch0</hostname>
        <nicname>port2</nicname>
      </DstNic>
      <hostname>pc0_link_net_switch0</hostname>
      <linktype>normal</linktype>
      <uniqueidentifier>171</uniqueidentifier>
    </link>
    <link>
      <SrcNic>
        <hostid>112</hostid>
        <nicid>114</nicid>
        <hostname>pc1</hostname>
        <nicname>eth0</nicname>
      </SrcNic>
      <DstNic>
        <hostid>132</hostid>
        <nicid>137</nicid>
        <hostname>net_switch0</hostname>
        <nicname>port3</nicname>
      </DstNic>
      <hostname>pc1_link_net_switch0</hostname>
      <linktype>normal</linktype>
      <uniqueidentifier>173</uniqueidentifier>
    </link>
    <link>
      <SrcNic>
        <hostid>115</hostid>
        <nicid>117</nicid>
        <hostname>pc2</hostname>
        <nicname>eth0</nicname>
      </SrcNic>
      <DstNic>
        <hostid>142</hostid>
        <nicid>145</nicid>
        <hostname>net_switch1</hostname>
        <nicname>port1</nicname>
      </DstNic>
      <hostname>pc2_link_net_switch1</hostname>
      <linktype>normal</linktype>
      <uniqueidentifier>163</uniqueidentifier>
    </link>
    <link>
      <SrcNic>
        <hostid>398</hostid>
        <nicid>400</nicid>
        <hostname>pc4</hostname>
        <nicname>eth0</nicname>
      </SrcNic>
      <DstNic>
        <hostid>388</hostid>
        <nicid>391</nicid>
        <hostname>net_switch3</hostname>
        <nicname>port1</nicname>
      </DstNic>
      <hostname>pc4_link_net_switch3</hostname>
      <linktype>normal</linktype>
      <uniqueidentifier>429</uniqueidentifier>
    </link>
    <link>
      <SrcNic>
        <hostid>401</hostid>
        <nicid>403</nicid>
        <hostname>pc5</hostname>
        <nicname>eth0</nicname>
      </SrcNic>
      <DstNic>
        <hostid>388</hostid>
        <nicid>392</nicid>
        <hostname>net_switch3</hostname>
        <nicname>port2</nicname>
      </DstNic>
      <hostname>pc5_link_net_switch3</hostname>
      <linktype>normal</linktype>
      <uniqueidentifier>431</uniqueidentifier>
    </link>
    <link>
      <SrcNic>
        <hostid>182</hostid>
        <nicid>185</nicid>
        <hostname>router0</hostname>
        <nicname>eth1</nicname>
      </SrcNic>
      <DstNic>
        <hostid>186</hostid>
        <nicid>189</nicid>
        <hostname>router1</hostname>
        <nicname>eth1</nicname>
      </DstNic>
      <hostname>router0_link_router1</hostname>
      <linktype>normal</linktype>
      <uniqueidentifier>249</uniqueidentifier>
    </link>
    <link>
      <SrcNic>
        <hostid>495</hostid>
        <nicid>497</nicid>
        <hostname>server1</hostname>
        <nicname>eth0</nicname>
      </SrcNic>
      <DstNic>
        <hostid>388</hostid>
        <nicid>396</nicid>
        <hostname>net_switch3</hostname>
        <nicname>port6</nicname>
      </DstNic>
      <hostname>server1_link_net_switch3</hostname>
      <linktype>normal</linktype>
      <uniqueidentifier>498</uniqueidentifier>
    </link>
    <nettest>
      <shost>net_switch3</shost>
      <dhost>net_switch1</dhost>
      <thetest>DeviceIsFrozen</thetest>
    </nettest>
    <nettest>
      <shost>server0</shost>
      <dhost>server1</dhost>
      <thetest>SuccessfullyPings</thetest>
    </nettest>
    <shape>
      <name>Grass</name>
      <what>rectangle</what>
      <where>3, 7, 1013, 1004</where>
      <fillcolor>LightGreen</fillcolor>
      <linecolor>LightGreen</linecolor>
    </shape>
    <shape>
      <name>LeftBldg</name>
      <what>rectangle</what>
      <where>20, 170, 250, 700</where>
      <fillcolor>SaddleBrown</fillcolor>
      <linecolor>SaddleBrown</linecolor>
    </shape>
    <shape>
      <name>RightBldg</name>
      <what>rectangle</what>
      <where>650, 170, 250, 700</where>
      <fillcolor>SaddleBrown</fillcolor>
      <linecolor>SaddleBrown</linecolor>
    </shape>
    <shape>
      <name>LB_RWall</name>
      <what>rectangle</what>
      <where>255, 170, 15, 700</where>
      <fillcolor>Gray</fillcolor>
      <linecolor>Gray</linecolor>
    </shape>
    <shape>
      <name>RB_RWall</name>
      <what>rectangle</what>
      <where>650, 170, 15, 700</where>
      <fillcolor>Gray</fillcolor>
      <linecolor>Gray</linecolor>
    </shape>
    <shape>
      <name>LB_TWall</name>
      <what>rectangle</what>
      <where>20, 170, 15, 700</where>
      <fillcolor>Gray</fillcolor>
      <linecolor>Gray</linecolor>
    </shape>
    <shape>
      <name>RB_TWall</name>
      <what>rectangle</what>
      <where>885, 170, 15, 700</where>
      <fillcolor>Gray</fillcolor>
      <linecolor>Gray</linecolor>
    </shape>
    <shape>
      <name>LB_BWall</name>
      <what>rectangle</what>
      <where>20, 870, 250, 15</where>
      <fillcolor>Gray</fillcolor>
      <linecolor>Gray</linecolor>
    </shape>
    <shape>
      <name>RB_BWall</name>
      <what>rectangle</what>
      <where>650, 870, 250, 15</where>
      <fillcolor>Gray</fillcolor>
      <linecolor>Gray</linecolor>
    </shape>
    <shape>
      <name>LB_LWall</name>
      <what>rectangle</what>
      <where>20, 170, 250, 15</where>
      <fillcolor>Gray</fillcolor>
      <linecolor>Gray</linecolor>
    </shape>
    <shape>
      <name>RB_LWall</name>
      <what>rectangle</what>
      <where>650, 170, 250, 15</where>
      <fillcolor>Gray</fillcolor>
      <linecolor>Gray</linecolor>
    </shape>
    <shape>
      <name>CenterCement</name>
      <what>rectangle</what>
      <where>326, 200, 262, 377</where>
      <fillcolor>Gray</fillcolor>
      <linecolor>Gray</linecolor>
    </shape>
    <shape>
      <name>CenterPark</name>
      <what>rectangle</what>
      <where>359, 270, 188, 247</where>
      <fillcolor>LightGreen</fillcolor>
      <linecolor>LightGreen</linecolor>
    </shape>
    <shape>
      <name>LWindow</name>
      <what>rectangle</what>
      <where>260, 500, 5, 100</where>
      <fillcolor>Blue</fillcolor>
      <linecolor>Blue</linecolor>
    </shape>
    <shape>
      <name>R_Window</name>
      <what>rectangle</what>
      <where>655, 500, 5, 100</where>
      <fillcolor>Blue</fillcolor>
      <linecolor>Blue</linecolor>
    </shape>
    <shape>
      <name>LSidewalk</name>
      <what>rectangle</what>
      <where>255, 300, 100, 80</where>
      <fillcolor>Gray</fillcolor>
      <linecolor>Gray</linecolor>
    </shape>
    <shape>
      <name>RSidewalk</name>
      <what>rectangle</what>
      <where>550, 300, 100, 80</where>
      <fillcolor>Gray</fillcolor>
      <linecolor>Gray</linecolor>
    </shape>
    <shape>
      <name>LDoor</name>
      <what>rectangle</what>
      <where>255, 300, 10, 80</where>
      <fillcolor>SaddleBrown</fillcolor>
      <linecolor>SaddleBrown</linecolor>
    </shape>
    <shape>
      <name>RDoor</name>
      <what>rectangle</what>
      <where>655, 300, 10, 80</where>
      <fillcolor>SaddleBrown</fillcolor>
      <linecolor>SaddleBrown</linecolor>
    </shape>
    <VLANName
      ID="1"
      Color="Blue">Default</VLANName>
  </Network>
</EduNetworkBuilder>