<?xml version="1.0" encoding="utf-8"?>
<EduNetworkBuilder>
  <!--This is a network file for EduNetworkBuilder.-->
  <Network>
    <en_message>Start by adding a cellphone, tablet, and laptop all to the network.  When you add them, you need to configure the wireless SSID and Key of the device.  You can do this two ways.  You can drag a link from the device to the wireless access point, or you can edit the wireless nic and manually configure the ssid and key.
You also want to give all three devices IP addresses (via DHCP or static).</en_message>
    <fr_message>Commencez par ajouter un téléphone portable, une tablette et un ordinateur portable au réseau. Lorsque vous les ajoutez, vous devez configurer le SSID sans fil et la clé du périphérique. Vous pouvez faire cela de deux façons. Vous pouvez faire glisser un lien du périphérique vers le point d'accès sans fil, ou vous pouvez modifier le périphérique sans fil et configurer manuellement le ssid et la clé.
Vous souhaitez également attribuer les adresses IP des trois périphériques (via DHCP ou statique).</fr_message>
    <en_title>Wireless Devices</en_title>
    <height>1024</height>
    <width>1024</width>
    <itemsize>100</itemsize>
    <showlabels>none</showlabels>
    <level>5</level>
    <sortorder>2</sortorder>
    <uniqueidentifier>132</uniqueidentifier>
    <startinghelplevel>full</startinghelplevel>
    <vlansenabled>False</vlansenabled>
    <VLANPacketColors>False</VLANPacketColors>
    <device>
      <hostname>pc0</hostname>
      <size>100</size>
      <uniqueidentifier>123</uniqueidentifier>
      <location>630,180</location>
      <mytype>pc</mytype>
      <isdns>False</isdns>
      <isdhcp>False</isdhcp>
      <gateway>
        <ip>192.168.7.1</ip>
        <mask>0.0.0.0</mask>
        <gateway>0.0.0.0</gateway>
        <type>gw</type>
      </gateway>
      <nic>
        <nictype>lo</nictype>
        <nicname>lo0</nicname>
        <myid>
          <hostid>123</hostid>
          <nicid>124</nicid>
          <hostname>pc0</hostname>
          <nicname>lo0</nicname>
        </myid>
        <nictype>lo</nictype>
        <uniqueidentifier>124</uniqueidentifier>
        <usesdhcp>False</usesdhcp>
        <encryptionkey />
        <ssid />
        <interface>
          <nicname>lo0</nicname>
          <myip>
            <ip>127.0.0.1</ip>
            <mask>255.0.0.0</mask>
            <gateway>0.0.0.0</gateway>
            <type>ip</type>
          </myip>
          <VLAN
            ID="1">Untagged</VLAN>
        </interface>
      </nic>
      <nic>
        <nictype>eth</nictype>
        <nicname>eth0</nicname>
        <myid>
          <hostid>123</hostid>
          <nicid>125</nicid>
          <hostname>pc0</hostname>
          <nicname>eth0</nicname>
        </myid>
        <nictype>eth</nictype>
        <uniqueidentifier>125</uniqueidentifier>
        <usesdhcp>False</usesdhcp>
        <encryptionkey />
        <ssid />
        <interface>
          <nicname>eth0</nicname>
          <myip>
            <ip>192.168.7.2</ip>
            <mask>255.255.255.0</mask>
            <gateway>0.0.0.0</gateway>
            <type>ip</type>
          </myip>
          <VLAN
            ID="1">Untagged</VLAN>
        </interface>
      </nic>
    </device>
    <device>
      <hostname>pc1</hostname>
      <size>100</size>
      <uniqueidentifier>128</uniqueidentifier>
      <location>430,560</location>
      <mytype>pc</mytype>
      <isdns>False</isdns>
      <isdhcp>False</isdhcp>
      <gateway>
        <ip>192.168.1.1</ip>
        <mask>0.0.0.0</mask>
        <gateway>0.0.0.0</gateway>
        <type>gw</type>
      </gateway>
      <nic>
        <nictype>lo</nictype>
        <nicname>lo0</nicname>
        <myid>
          <hostid>128</hostid>
          <nicid>129</nicid>
          <hostname>pc1</hostname>
          <nicname>lo0</nicname>
        </myid>
        <nictype>lo</nictype>
        <uniqueidentifier>129</uniqueidentifier>
        <usesdhcp>False</usesdhcp>
        <encryptionkey />
        <ssid />
        <interface>
          <nicname>lo0</nicname>
          <myip>
            <ip>127.0.0.1</ip>
            <mask>255.0.0.0</mask>
            <gateway>0.0.0.0</gateway>
            <type>ip</type>
          </myip>
          <VLAN
            ID="1">Untagged</VLAN>
        </interface>
      </nic>
      <nic>
        <nictype>eth</nictype>
        <nicname>eth0</nicname>
        <myid>
          <hostid>128</hostid>
          <nicid>130</nicid>
          <hostname>pc1</hostname>
          <nicname>eth0</nicname>
        </myid>
        <nictype>eth</nictype>
        <uniqueidentifier>130</uniqueidentifier>
        <usesdhcp>False</usesdhcp>
        <encryptionkey />
        <ssid />
        <interface>
          <nicname>eth0</nicname>
          <myip>
            <ip>192.168.1.2</ip>
            <mask>255.255.255.0</mask>
            <gateway>0.0.0.0</gateway>
            <type>ip</type>
          </myip>
          <VLAN
            ID="1">Untagged</VLAN>
        </interface>
      </nic>
    </device>
    <device>
      <hostname>router0</hostname>
      <size>100</size>
      <uniqueidentifier>119</uniqueidentifier>
      <location>430,180</location>
      <mytype>router</mytype>
      <isdns>False</isdns>
      <isdhcp>False</isdhcp>
      <gateway>
        <ip>0.0.0.0</ip>
        <mask>0.0.0.0</mask>
        <gateway>0.0.0.0</gateway>
        <type>gw</type>
      </gateway>
      <nic>
        <nictype>lo</nictype>
        <nicname>lo0</nicname>
        <myid>
          <hostid>119</hostid>
          <nicid>120</nicid>
          <hostname>router0</hostname>
          <nicname>lo0</nicname>
        </myid>
        <nictype>lo</nictype>
        <uniqueidentifier>120</uniqueidentifier>
        <usesdhcp>False</usesdhcp>
        <encryptionkey />
        <ssid />
        <interface>
          <nicname>lo0</nicname>
          <myip>
            <ip>127.0.0.1</ip>
            <mask>255.0.0.0</mask>
            <gateway>0.0.0.0</gateway>
            <type>ip</type>
          </myip>
          <VLAN
            ID="1">Untagged</VLAN>
        </interface>
      </nic>
      <nic>
        <nictype>eth</nictype>
        <nicname>eth0</nicname>
        <myid>
          <hostid>119</hostid>
          <nicid>121</nicid>
          <hostname>router0</hostname>
          <nicname>eth0</nicname>
        </myid>
        <nictype>eth</nictype>
        <uniqueidentifier>121</uniqueidentifier>
        <usesdhcp>False</usesdhcp>
        <encryptionkey />
        <ssid />
        <interface>
          <nicname>eth0</nicname>
          <myip>
            <ip>192.168.6.1</ip>
            <mask>255.255.255.0</mask>
            <gateway>0.0.0.0</gateway>
            <type>ip</type>
          </myip>
          <VLAN
            ID="1">Untagged</VLAN>
        </interface>
      </nic>
      <nic>
        <nictype>eth</nictype>
        <nicname>eth1</nicname>
        <myid>
          <hostid>119</hostid>
          <nicid>122</nicid>
          <hostname>router0</hostname>
          <nicname>eth1</nicname>
        </myid>
        <nictype>eth</nictype>
        <uniqueidentifier>122</uniqueidentifier>
        <usesdhcp>False</usesdhcp>
        <encryptionkey />
        <ssid />
        <interface>
          <nicname>eth1</nicname>
          <myip>
            <ip>192.168.7.1</ip>
            <mask>255.255.255.0</mask>
            <gateway>0.0.0.0</gateway>
            <type>ip</type>
          </myip>
          <VLAN
            ID="1">Untagged</VLAN>
        </interface>
      </nic>
      <route>
        <ip>192.168.1.1</ip>
        <mask>255.255.255.0</mask>
        <gateway>192.168.6.2</gateway>
        <type>route</type>
      </route>
    </device>
    <device>
      <hostname>wrouter0</hostname>
      <size>100</size>
      <uniqueidentifier>100</uniqueidentifier>
      <location>430,390</location>
      <mytype>wrouter</mytype>
      <isdns>False</isdns>
      <isdhcp>True</isdhcp>
      <gateway>
        <ip>192.168.6.1</ip>
        <mask>0.0.0.0</mask>
        <gateway>0.0.0.0</gateway>
        <type>gw</type>
      </gateway>
      <nic>
        <nictype>lo</nictype>
        <nicname>lo0</nicname>
        <myid>
          <hostid>100</hostid>
          <nicid>103</nicid>
          <hostname>wrouter0</hostname>
          <nicname>lo0</nicname>
        </myid>
        <nictype>lo</nictype>
        <uniqueidentifier>103</uniqueidentifier>
        <usesdhcp>False</usesdhcp>
        <encryptionkey />
        <ssid />
        <interface>
          <nicname>lo0</nicname>
          <myip>
            <ip>127.0.0.1</ip>
            <mask>255.0.0.0</mask>
            <gateway>0.0.0.0</gateway>
            <type>ip</type>
          </myip>
          <VLAN
            ID="1">Untagged</VLAN>
        </interface>
      </nic>
      <nic>
        <nictype>wan</nictype>
        <nicname>wan0</nicname>
        <myid>
          <hostid>100</hostid>
          <nicid>118</nicid>
          <hostname>wrouter0</hostname>
          <nicname>wan0</nicname>
        </myid>
        <nictype>wan</nictype>
        <uniqueidentifier>118</uniqueidentifier>
        <usesdhcp>False</usesdhcp>
        <encryptionkey />
        <ssid />
        <interface>
          <nicname>wan0</nicname>
          <myip>
            <ip>192.168.6.2</ip>
            <mask>255.255.255.0</mask>
            <gateway>0.0.0.0</gateway>
            <type>ip</type>
          </myip>
          <VLAN
            ID="1">Untagged</VLAN>
        </interface>
      </nic>
      <nic>
        <nictype>vpn</nictype>
        <nicname>vpn0</nicname>
        <myid>
          <hostid>100</hostid>
          <nicid>117</nicid>
          <hostname>wrouter0</hostname>
          <nicname>vpn0</nicname>
        </myid>
        <nictype>vpn</nictype>
        <uniqueidentifier>117</uniqueidentifier>
        <usesdhcp>False</usesdhcp>
        <encryptionkey />
        <ssid />
        <interface>
          <nicname>vpn0</nicname>
          <myip>
            <ip>0.0.0.0</ip>
            <mask>0.0.0.0</mask>
            <gateway>0.0.0.0</gateway>
            <type>ip</type>
          </myip>
          <VLAN
            ID="1">Untagged</VLAN>
        </interface>
      </nic>
      <nic>
        <nictype>management_interface</nictype>
        <nicname>management_interface0</nicname>
        <myid>
          <hostid>100</hostid>
          <nicid>104</nicid>
          <hostname>wrouter0</hostname>
          <nicname>management_interface0</nicname>
        </myid>
        <nictype>management_interface</nictype>
        <uniqueidentifier>104</uniqueidentifier>
        <usesdhcp>False</usesdhcp>
        <encryptionkey />
        <ssid />
        <interface>
          <nicname>management_interface0</nicname>
          <myip>
            <ip>192.168.1.1</ip>
            <mask>255.255.255.0</mask>
            <gateway>0.0.0.0</gateway>
            <type>ip</type>
          </myip>
          <VLAN
            ID="1">Untagged</VLAN>
        </interface>
      </nic>
      <nic>
        <nictype>port</nictype>
        <nicname>port2</nicname>
        <myid>
          <hostid>100</hostid>
          <nicid>105</nicid>
          <hostname>wrouter0</hostname>
          <nicname>port2</nicname>
        </myid>
        <nictype>port</nictype>
        <uniqueidentifier>105</uniqueidentifier>
        <usesdhcp>False</usesdhcp>
        <encryptionkey />
        <ssid />
        <interface>
          <nicname>port2</nicname>
          <myip>
            <ip>0.0.0.0</ip>
            <mask>0.0.0.0</mask>
            <gateway>0.0.0.0</gateway>
            <type>ip</type>
          </myip>
          <VLAN
            ID="1">Untagged</VLAN>
        </interface>
      </nic>
      <nic>
        <nictype>port</nictype>
        <nicname>port3</nicname>
        <myid>
          <hostid>100</hostid>
          <nicid>106</nicid>
          <hostname>wrouter0</hostname>
          <nicname>port3</nicname>
        </myid>
        <nictype>port</nictype>
        <uniqueidentifier>106</uniqueidentifier>
        <usesdhcp>False</usesdhcp>
        <encryptionkey />
        <ssid />
        <interface>
          <nicname>port3</nicname>
          <myip>
            <ip>0.0.0.0</ip>
            <mask>0.0.0.0</mask>
            <gateway>0.0.0.0</gateway>
            <type>ip</type>
          </myip>
          <VLAN
            ID="1">Untagged</VLAN>
        </interface>
      </nic>
      <nic>
        <nictype>port</nictype>
        <nicname>port4</nicname>
        <myid>
          <hostid>100</hostid>
          <nicid>107</nicid>
          <hostname>wrouter0</hostname>
          <nicname>port4</nicname>
        </myid>
        <nictype>port</nictype>
        <uniqueidentifier>107</uniqueidentifier>
        <usesdhcp>False</usesdhcp>
        <encryptionkey />
        <ssid />
        <interface>
          <nicname>port4</nicname>
          <myip>
            <ip>0.0.0.0</ip>
            <mask>0.0.0.0</mask>
            <gateway>0.0.0.0</gateway>
            <type>ip</type>
          </myip>
          <VLAN
            ID="1">Untagged</VLAN>
        </interface>
      </nic>
      <nic>
        <nictype>port</nictype>
        <nicname>port5</nicname>
        <myid>
          <hostid>100</hostid>
          <nicid>108</nicid>
          <hostname>wrouter0</hostname>
          <nicname>port5</nicname>
        </myid>
        <nictype>port</nictype>
        <uniqueidentifier>108</uniqueidentifier>
        <usesdhcp>False</usesdhcp>
        <encryptionkey />
        <ssid />
        <interface>
          <nicname>port5</nicname>
          <myip>
            <ip>0.0.0.0</ip>
            <mask>0.0.0.0</mask>
            <gateway>0.0.0.0</gateway>
            <type>ip</type>
          </myip>
          <VLAN
            ID="1">Untagged</VLAN>
        </interface>
      </nic>
      <nic>
        <nictype>wport</nictype>
        <nicname>wport6</nicname>
        <myid>
          <hostid>100</hostid>
          <nicid>109</nicid>
          <hostname>wrouter0</hostname>
          <nicname>wport6</nicname>
        </myid>
        <nictype>wport</nictype>
        <uniqueidentifier>109</uniqueidentifier>
        <usesdhcp>False</usesdhcp>
        <encryptionkey>TheKey</encryptionkey>
        <ssid>my_ssid</ssid>
        <interface>
          <nicname>wport6</nicname>
          <myip>
            <ip>0.0.0.0</ip>
            <mask>0.0.0.0</mask>
            <gateway>0.0.0.0</gateway>
            <type>ip</type>
          </myip>
          <VLAN
            ID="1">Untagged</VLAN>
        </interface>
      </nic>
      <nic>
        <nictype>wport</nictype>
        <nicname>wport7</nicname>
        <myid>
          <hostid>100</hostid>
          <nicid>110</nicid>
          <hostname>wrouter0</hostname>
          <nicname>wport7</nicname>
        </myid>
        <nictype>wport</nictype>
        <uniqueidentifier>110</uniqueidentifier>
        <usesdhcp>False</usesdhcp>
        <encryptionkey>TheKey</encryptionkey>
        <ssid>my_ssid</ssid>
        <interface>
          <nicname>wport7</nicname>
          <myip>
            <ip>0.0.0.0</ip>
            <mask>0.0.0.0</mask>
            <gateway>0.0.0.0</gateway>
            <type>ip</type>
          </myip>
          <VLAN
            ID="1">Untagged</VLAN>
        </interface>
      </nic>
      <nic>
        <nictype>wport</nictype>
        <nicname>wport8</nicname>
        <myid>
          <hostid>100</hostid>
          <nicid>111</nicid>
          <hostname>wrouter0</hostname>
          <nicname>wport8</nicname>
        </myid>
        <nictype>wport</nictype>
        <uniqueidentifier>111</uniqueidentifier>
        <usesdhcp>False</usesdhcp>
        <encryptionkey>TheKey</encryptionkey>
        <ssid>my_ssid</ssid>
        <interface>
          <nicname>wport8</nicname>
          <myip>
            <ip>0.0.0.0</ip>
            <mask>0.0.0.0</mask>
            <gateway>0.0.0.0</gateway>
            <type>ip</type>
          </myip>
          <VLAN
            ID="1">Untagged</VLAN>
        </interface>
      </nic>
      <nic>
        <nictype>wport</nictype>
        <nicname>wport9</nicname>
        <myid>
          <hostid>100</hostid>
          <nicid>112</nicid>
          <hostname>wrouter0</hostname>
          <nicname>wport9</nicname>
        </myid>
        <nictype>wport</nictype>
        <uniqueidentifier>112</uniqueidentifier>
        <usesdhcp>False</usesdhcp>
        <encryptionkey>TheKey</encryptionkey>
        <ssid>my_ssid</ssid>
        <interface>
          <nicname>wport9</nicname>
          <myip>
            <ip>0.0.0.0</ip>
            <mask>0.0.0.0</mask>
            <gateway>0.0.0.0</gateway>
            <type>ip</type>
          </myip>
          <VLAN
            ID="1">Untagged</VLAN>
        </interface>
      </nic>
      <nic>
        <nictype>wport</nictype>
        <nicname>wport10</nicname>
        <myid>
          <hostid>100</hostid>
          <nicid>113</nicid>
          <hostname>wrouter0</hostname>
          <nicname>wport10</nicname>
        </myid>
        <nictype>wport</nictype>
        <uniqueidentifier>113</uniqueidentifier>
        <usesdhcp>False</usesdhcp>
        <encryptionkey>TheKey</encryptionkey>
        <ssid>my_ssid</ssid>
        <interface>
          <nicname>wport10</nicname>
          <myip>
            <ip>0.0.0.0</ip>
            <mask>0.0.0.0</mask>
            <gateway>0.0.0.0</gateway>
            <type>ip</type>
          </myip>
          <VLAN
            ID="1">Untagged</VLAN>
        </interface>
      </nic>
      <nic>
        <nictype>wport</nictype>
        <nicname>wport11</nicname>
        <myid>
          <hostid>100</hostid>
          <nicid>114</nicid>
          <hostname>wrouter0</hostname>
          <nicname>wport11</nicname>
        </myid>
        <nictype>wport</nictype>
        <uniqueidentifier>114</uniqueidentifier>
        <usesdhcp>False</usesdhcp>
        <encryptionkey>TheKey</encryptionkey>
        <ssid>my_ssid</ssid>
        <interface>
          <nicname>wport11</nicname>
          <myip>
            <ip>0.0.0.0</ip>
            <mask>0.0.0.0</mask>
            <gateway>0.0.0.0</gateway>
            <type>ip</type>
          </myip>
          <VLAN
            ID="1">Untagged</VLAN>
        </interface>
      </nic>
      <nic>
        <nictype>wport</nictype>
        <nicname>wport12</nicname>
        <myid>
          <hostid>100</hostid>
          <nicid>115</nicid>
          <hostname>wrouter0</hostname>
          <nicname>wport12</nicname>
        </myid>
        <nictype>wport</nictype>
        <uniqueidentifier>115</uniqueidentifier>
        <usesdhcp>False</usesdhcp>
        <encryptionkey>TheKey</encryptionkey>
        <ssid>my_ssid</ssid>
        <interface>
          <nicname>wport12</nicname>
          <myip>
            <ip>0.0.0.0</ip>
            <mask>0.0.0.0</mask>
            <gateway>0.0.0.0</gateway>
            <type>ip</type>
          </myip>
          <VLAN
            ID="1">Untagged</VLAN>
        </interface>
      </nic>
      <nic>
        <nictype>wport</nictype>
        <nicname>wport13</nicname>
        <myid>
          <hostid>100</hostid>
          <nicid>116</nicid>
          <hostname>wrouter0</hostname>
          <nicname>wport13</nicname>
        </myid>
        <nictype>wport</nictype>
        <uniqueidentifier>116</uniqueidentifier>
        <usesdhcp>False</usesdhcp>
        <encryptionkey>TheKey</encryptionkey>
        <ssid>my_ssid</ssid>
        <interface>
          <nicname>wport13</nicname>
          <myip>
            <ip>0.0.0.0</ip>
            <mask>0.0.0.0</mask>
            <gateway>0.0.0.0</gateway>
            <type>ip</type>
          </myip>
          <VLAN
            ID="1">Untagged</VLAN>
        </interface>
      </nic>
      <dhcprange>
        <ip>127.0.0.1</ip>
        <mask>0.0.0.0</mask>
        <gateway>0.0.0.0</gateway>
        <type>route</type>
      </dhcprange>
      <dhcprange>
        <ip>0.0.0.0</ip>
        <mask>0.0.0.0</mask>
        <gateway>0.0.0.0</gateway>
        <type>route</type>
      </dhcprange>
      <dhcprange>
        <ip>192.168.6.2</ip>
        <mask>0.0.0.0</mask>
        <gateway>0.0.0.0</gateway>
        <type>route</type>
      </dhcprange>
      <dhcprange>
        <ip>192.168.1.1</ip>
        <mask>192.168.1.5</mask>
        <gateway>192.168.1.10</gateway>
        <type>route</type>
      </dhcprange>
    </device>
    <link>
      <SrcNic>
        <hostid>100</hostid>
        <nicid>118</nicid>
        <hostname>wrouter0</hostname>
        <nicname>wan0</nicname>
      </SrcNic>
      <DstNic>
        <hostid>119</hostid>
        <nicid>121</nicid>
        <hostname>router0</hostname>
        <nicname>eth0</nicname>
      </DstNic>
      <hostname>wrouter0_link_router0</hostname>
      <linktype>normal</linktype>
      <uniqueidentifier>126</uniqueidentifier>
    </link>
    <link>
      <SrcNic>
        <hostid>119</hostid>
        <nicid>122</nicid>
        <hostname>router0</hostname>
        <nicname>eth1</nicname>
      </SrcNic>
      <DstNic>
        <hostid>123</hostid>
        <nicid>125</nicid>
        <hostname>pc0</hostname>
        <nicname>eth0</nicname>
      </DstNic>
      <hostname>router0_link_pc0</hostname>
      <linktype>normal</linktype>
      <uniqueidentifier>127</uniqueidentifier>
    </link>
    <link>
      <SrcNic>
        <hostid>128</hostid>
        <nicid>130</nicid>
        <hostname>pc1</hostname>
        <nicname>eth0</nicname>
      </SrcNic>
      <DstNic>
        <hostid>100</hostid>
        <nicid>105</nicid>
        <hostname>wrouter0</hostname>
        <nicname>port2</nicname>
      </DstNic>
      <hostname>pc1_link_wrouter0</hostname>
      <linktype>normal</linktype>
      <uniqueidentifier>131</uniqueidentifier>
    </link>
    <nettest>
      <shost>tablet0</shost>
      <dhost>wrouter0</dhost>
      <thetest>NeedsLinkToDevice</thetest>
    </nettest>
    <nettest>
      <shost>laptop0</shost>
      <dhost>wrouter0</dhost>
      <thetest>NeedsLinkToDevice</thetest>
    </nettest>
    <nettest>
      <shost>cellphone0</shost>
      <dhost>wrouter0</dhost>
      <thetest>NeedsLinkToDevice</thetest>
    </nettest>
    <nettest>
      <shost>cellphone0</shost>
      <dhost>tablet0</dhost>
      <thetest>SuccessfullyPings</thetest>
    </nettest>
    <nettest>
      <shost>cellphone0</shost>
      <dhost>laptop0</dhost>
      <thetest>SuccessfullyPings</thetest>
    </nettest>
    <tag>GeneralWireless</tag>
    <tag>WirelessSSID</tag>
    <tag>WirelessKey</tag>
    <VLANName
      ID="1"
      Color="Blue">Default</VLANName>
  </Network>
</EduNetworkBuilder>